Cyber-shot User Guide
Print
Top page > Useful shooting functions > Using shooting functions > Zoom Func. on Ring

## Zoom Func. on Ring

Sets the zooming method when the zoom function is assigned to the Control Ring.
In the default setting, the zoom function is assigned to the Control Ring when shooting mode is set to [Intelligent Auto] or [Superior Auto].

1. MENU 2 [Zoom Func. on Ring] desired mode

| Standard | Zooms in/out smoothly using the Control Ring.
| Step | Zooms in/out at fixed focal length steps, using the Control Ring. Fixed steps* are 28 mm, 35 mm, 50 mm, 70 mm and 100 mm. * 35 mm equivalent

Notes

- In the following cases, the zoom will be [Standard] even if [Step] is set.

- When you zoom using the W/T (zoom) lever

- While recording movies

- While zoom functions other than optical are used

Related Topic
Control Ring
Back to top