Reader™ User Guide
Print
Top page > Getting started > Parts and Controls > microSD Card Slot

## microSD Card Slot

The microSD card slot is located on the back of the Reader.

1. Remove the Standard Cover (PRS-T3) or Back Panel (PRS-T3S*).

1. Hold the microSD card with its contacts facing down and the arrow pointing toward the microSD card slot, then insert it until it clicks into place.

The access indicator lights up in orange while the Reader is accessing the microSD card.

1. Attach the Standard Cover (PRS-T3) or Back Panel (PRS-T3S*).

* Limited edition only.
You can format the microSD card if necessary. See Details.
Note

- Do not remove the microSD card while the access indicator is lit.

- Push in the microSD card once, carefully slide the card out with your fingertip, then release.

1. Access indicator

Go to page top