# Personal Computer VAIO Fit 14E/15ESVF1432/SVF1532

## Starting Wi-Fi(R) (Wireless LAN) Communications

You can establish Wi-Fi communications between your VAIO computer and an access point (not supplied).

Before using Wi-Fi, make sure a Wi-Fi access point is on and operating.

1. Connect an access point to your VAIO computer.

   Refer to Windows Help and Support (Opening Windows Help and Support) and the manual that came with the access point for more information.

2. Open the charms and select theSettings charm. (See Opening the Charms to open the charms.)
3. Select(the network icon).
4. Change the Wi-Fi setting to On.
5. Select the desired access point and Connect.

   After the connection is established, Connected appears in the selected wireless access point field.

   If a security key entry window appears, enter the security key as required and select OK. See About a Security Key for Wi-Fi(R) (Wireless LAN) for more information.

   Note that security keys are case-sensitive.

#### To check Wi-Fi connection status

Open the desktop and move the mouse pointer over(the Network icon) in the desktop notification area to check the Wi-Fi connection status, such as the access point currently connected to your VAIO computer.

To open the desktop, see Opening the Desktop.

#### Note

- On IEEE 802.11a/b/g/n/ac (draft) equipped models, when only the 2.4 GHz Wi-Fi function is enabled, your VAIO computer cannot connect to a 5 GHz Wi-Fi access point. Also, when only the 5 GHz Wi-Fi function is enabled, the computer cannot connect to a 2.4 GHz Wi-Fi access point.

  On IEEE 802.11b/g/n equipped models, when the 2.4 GHz Wi-Fi function is disabled, the computer cannot connect to an access point. Also, the computer cannot connect to a 5 GHz Wi-Fi access point.

- It may take some time to find and connect to a Wi-Fi access point before starting communications via Wi-Fi.

#### Hint

- Refer to Windows Help and Support (Opening Windows Help and Support) for more information on Airplane mode.

- Once you connect your VAIO computer to the access point by entering the security key, the access point will be registered in the computer. You do not have to enter the security key for subsequent connections.

Go to Page Top

### Related Topic

- About the Wi-Fi(R) (Wireless LAN) Standards
- Stopping Wi-Fi(R) (Wireless LAN) Communications
- Notes on Using the Wi-Fi(R) (Wireless LAN) Function
- About a Security Key for Wi-Fi(R) (Wireless LAN)

Go to Page Top