#

# i-Manual online

- Print
- Font Size

- Top Page >
- Parts Description >
- Back

# Back

- 3D SYNC
- LAN
- HDMI IN 1/4
- / AV 1
- DIGITAL AUDIO OUT (OPTICAL)

1. 3D SYNC

   Connects to the 3D Sync Transmitter that is sold separately.

2. LAN

   Connects to an existing network using an Ethernet cable.

3. HDMI IN 1/4

   HDMI (High-Definition Multimedia Interface) provides an uncompressed, all-digital audio/video interface between this TV and any HDMI-equipped audio/video equipment. In addition, when you connect the equipment that is compatible with “Control for HDMI”, communication with the connected equipment is supported.

   ####

   - Be sure to use only an authorised HDMI cable bearing the HDMI logo.
   - If connecting a digital audio system that is compatible with Audio Return Channel (ARC) technology, use the HDMI IN 1. If not, an additional connection with DIGITAL AUDIO OUT (OPTICAL) is necessary.
   - If the equipment has a DVI jack (socket), connect it to the HDMI IN 2 on the side of the TV through a DVI - HDMI adaptor interface (not supplied), and connect the equipment’s audio out jacks (sockets) to the PC/HDMI 2 AUDIO IN which is located in the PC IN.
4. / AV 1

   Connect with a SCART adaptor. When you connect an analogue decoder, the TV tuner outputs scrambled signals to the decoder, and the decoder unscrambles the signals before outputting them.

5. DIGITAL AUDIO OUT (OPTICAL)

   You can listen to TV sound on the connected Home theatre system with digital input.

6. RF input that connects to your cable or antenna (aerial).

   ####

   - For satellite-compatible models, a satellite input is also available.

Copyright 2010 Sony Corporation