#

# i-Manual online

- Print
- Font Size

- Top Page >
- Fun Features with Connected Equipment >
- PC

# PC

Enjoy music, pictures and other content from your PC by connecting it with dedicated cables.

D-sub 15 cable (not supplied)
Audio cable (not supplied)
PC
TV

####

- It is recommended to use a PC cable with ferrites, such as the “Connector, D-sub 15” (ref. 1-793-504-11, available in Sony Service Centre), or an equivalent.
- You can connect an HDMI-compatible PC with an HDMI cable.

## PC Input Signal Reference Chart

- VGA
- - Horizontal (Pixel)/Vertical (Line): 640/480
- - Horizontal frequency (kHz)/Vertical frequency (Hz): 31.5/60
- - Standard: VGA
- SVGA
- - Horizontal (Pixel)/Vertical (Line): 800/600
- - Horizontal frequency (kHz)/Vertical frequency (Hz): 37.9/60
- - Standard: VESA Guidelines
- XGA
- - Horizontal (Pixel)/Vertical (Line): 1024/768
- - Horizontal frequency (kHz)/Vertical frequency (Hz): 48.4/60
- - Standard: VESA Guidelines
- WXGA
- - Horizontal (Pixel)/Vertical (Line): 1280/768, 1280/768, 1360/768
- - Horizontal frequency (kHz)/Vertical frequency (Hz): 47.4/60, 47.8/60, 47.7/60
- - Standard: VESA
- SXGA (Full HD model only)
- - Horizontal (Pixel)/Vertical (Line): 1280/1024
- - Horizontal frequency (kHz)/Vertical frequency (Hz): 64.0/60
- - Standard: VESA
- HDTV* (Full HD model only)
- - Horizontal (Pixel)/Vertical (Line): 1920/1080
- - Horizontal frequency (kHz)/Vertical frequency (Hz): 67.5/60
- - Standard: EIA*

####

- This TV’s PC input does not support Sync on Green or Composite Sync.
- This TV’s PC input does not support interlaced signals.
- For optimum picture quality, it is recommended to use the signals in the chart with a 60 Hz vertical frequency (boldfaced).

* 1080p timing when applied to the HDMI input will be treated as a video timing and not a PC timing. This will affect the “Video Input Settings” and “Screen” settings. To view PC contents, set “Screen Format” to “Wide” and “Display Area” to “Full Pixel”.

Copyright 2010 Sony Corporation