#

# i-Manual online

- Print
- Font Size

- Top Page >
- Parts Description >
- Bottom

# Bottom

- LAN
- / AV1
- AV2, / COMPONENT IN
- HDMI IN 1/4

1. LAN

   Connects to an existing network using an Ethernet cable.

2. RF input that connects to your cable or antenna (aerial).

   ####

   - For satellite-compatible models, a satellite input is also available.
3. / AV1

   You need to use the supplied adaptor cable.

   When you connect an analogue decoder, the TV tuner outputs scrambled signals to the decoder, and the decoder unscrambles the signals before outputting them.

   ####

   - The SCART out setting must be made when outputting digital RF on certain models or in certain regions. Press OPTIONS, then select [SCART REC on].
4. AV2, / COMPONENT IN

   You need to use the supplied adaptor cable.

   This input can be used as a composite video input or as a component video input. When connecting mono equipment, connect to the L (MONO) jack (socket).

   ####

   - The TV will automatically detect and switch between AV2 and / COMPONENT IN. To manually set the input type, press HOME, select → [External Inputs] → [AV2/Component Input].
5. HDMI IN 1/4

   HDMI (High-Definition Multimedia Interface) provides an uncompressed, all-digital audio/video interface between this TV and any HDMI-equipped audio/video equipment. In addition, when you connect equipment that is compatible with “Control for HDMI”, communication with the connected equipment is supported.

   ####

   - Be sure to use only an authorised HDMI cable bearing the HDMI logo.
   - If connecting a digital audio system that is compatible with Audio Return Channel (ARC) technology, use HDMI IN 1. If not, an additional connection with DIGITAL AUDIO OUT (OPTICAL) is necessary.
   - If the equipment has a DVI jack (socket), connect it to HDMI IN 4 through a DVI - HDMI adaptor interface (not supplied), and connect the equipment’s audio out jacks (sockets) to PC/HDMI 4 AUDIO IN which is located in PC IN.

Copyright 2011 Sony Corporation