#

# i-Manual online

- Print
- Font Size

- Top Page >
- Parts Description >
- Rear

# Rear

- LAN
- DIGITAL AUDIO OUT (OPTICAL)
- / AV1
- AV2, / COMPONENT IN
- HDMI IN 1/3/4

1. LAN

   Connects to an existing network using an Ethernet cable.

2. DIGITAL AUDIO OUT (OPTICAL)

   You can listen to TV sound on a connected home theatre system with digital input.

3. RF input that connects to your cable or antenna (aerial).

   ####

   - For satellite-compatible models, a satellite input is also available.
4. / AV1

   Connect with a SCART cable. When you connect an analogue decoder, the TV tuner outputs scrambled signals to the decoder, and the decoder unscrambles the signals before outputting them.

   ####

   - The SCART out setting must be made when outputting digital RF on certain models or in certain regions. Press OPTIONS, then select [SCART REC on].
5. AV2, / COMPONENT IN

   This input can be used as a composite video input or as a component video input. When connecting mono equipment, connect to the L (MONO) jack (socket).

   For composite use, connect to AV2 for video, and to (L/R) of / COMPONENT IN for audio signals.

   For component connection, use Y, PB, PR for video signals and also connect to (L/R) for audio signals.

   ####

   - The TV will automatically detect and switch between AV2 and / COMPONENT IN. To manually set the input type, press HOME, select → [External Inputs] → [AV2/Component Input].
6. HDMI IN 1/3/4

   HDMI (High-Definition Multimedia Interface) provides an uncompressed, all-digital audio/video interface between this TV and any HDMI-equipped audio/video equipment. In addition, when you connect equipment that is compatible with “Control for HDMI”, communication with the connected equipment is supported.

   ####

   - Be sure to use only an authorised HDMI cable bearing the HDMI logo.
   - If connecting a digital audio system that is compatible with Audio Return Channel (ARC) technology, use HDMI IN 1. If not, an additional connection with DIGITAL AUDIO OUT (OPTICAL) is necessary.
   - If the equipment has a DVI jack (socket), connect it to HDMI IN 4 through a DVI - HDMI adaptor interface (not supplied), and connect the equipment’s audio out jacks (sockets) to PC/HDMI 4 AUDIO IN.

Copyright 2011 Sony Corporation