Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > MENU items (Shooting) > DRO

## DRO

In Program Auto or Manual Exposure Shooting mode, the camera analyzes the shooting scene and automatically corrects the brightness and contrast to improve the image quality.
DRO stands for “Dynamic Range Optimizer,” a function that automatically optimizes the difference between light and dark parts of an image.

1. MENU (DRO) desired mode

| (Off) | Does not adjust.
| (DRO standard) | Adjusts the brightness and contrast of the images automatically.
| (DRO plus) | Adjusts image brightness and contrast automatically and strongly.

Notes

- Depending on shooting conditions, it may not be possible to obtain correction effects.

- Only [ISO AUTO] or values from [ISO 80] to [ISO 800] can be set for the ISO value when [DRO plus] is set.

Back to top