Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > MENU items (Shooting) > Burst Settings

## Burst Settings

You can select Single (single-image) or Burst as the shooting mode.

1. MENU (Burst Settings) desired mode

| (Single) | The camera shoots a single image.
| (Burst) | The camera shoots up to 100 continuous frames in one burst when you hold down the shutter button.

Notes

- [Flash] is set to [Off].

- When recording with the self-timer, only a single image is recorded.

- The recording interval becomes longer, depending on the setting for the image size.

- [Focus], [White Balance], and [EV] are adjusted for the first image, and these settings are also used for the other images.

- When the battery level is low, or when the internal memory or a memory card is full, the burst stops.

- You may not be able to set some functions or MENU items depending on the selected REC mode. For details, see “Functions not available in some REC modes” [Details] and “MENU items not available in some REC modes.” [Details]

Back to top