Cyber-shot User Guide
Print
Top page > Before Use > Names of parts and list of icons displayed on the screen > List of icons displayed on the screen

## List of icons displayed on the screen

List of shooting mode icons
List of viewing mode icons
Icons are displayed on the screen to indicate the camera status.
You can change the screen display using DISP (Screen Display Settings) on the control button.

### List of shooting mode icons

Display | Indication
| Battery remaining
| Low battery warning
| Image size/Panorama image size
| Scene Selection
| Mode dial (Intelligent Auto/Program Auto/Manual Exposure Shooting/Sweep Panorama/Movie Mode)
| Scene Recognition icon
| White balance
| Metering Mode
| Vibration warning
| Anti Blink
| Scene Recognition
| Burst Settings
| Bracket Shooting
| Bracket Setting
| DRO
| Soft Skin Effect
| Smile Detection Sensitivity indicator
1.4 | Zoom scaling

Display | Indication
| AE/AF lock
ISO400 | ISO number
| NR slow shutter
125 | Shutter speed
F3.5 | Aperture value
+2.0EV | Exposure value
| Focus

Display | Indication
| Recording folder
96 | Number of recordable images
100Min | Recordable time
| Recording Media (Memory card, internal memory)
| Eye-Fi Mode display
| AF Illuminator
| Flash mode
| Red-eye reduction
| Flash charging

Display | Indication
| Self-timer
C:32:00 | Self-diagnosis display
| Face detection
| Database file full/Database file error warning
| Destination
| Overheating warning
| AF range finder frame
| Spot metering cross-hairs
| Histogram
REC Standby | Recording a movie/Movie standby
0:12 | Recording time (m:s)

### List of viewing mode icons

Display | Indication
| Battery remaining
| Low battery warning
| Image size/Panorama image size
| Protect
| Print order (DPOF)
| Playback zoom
| View Mode
| TransferJet settings

Display | Indication
101-0012 | Folder-file number
2011 1 1 9:30 AM | Recorded date/time of the playback image

Display | Indication
| Playback folder
12/12 | Image number/Number of images recorded in date range, selected folder
| Playback Media (Memory card, internal memory)
| Eye-Fi Mode display
| Changing folder
| Metering Mode
| Flash mode
| White balance
ISO400 | ISO number
| Database file full/Database file error warning

Display | Indication
C:32:00 | Self-diagnosis display
+2.0EV | Exposure value
500 | Shutter speed
F3.5 | Aperture value
| Playback
| Playback bar
00:00:12 | Counter
| Histogram appears when histogram display is disabled.
| Volume

Back to top