Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > MENU items (Shooting) > DRO

## DRO

The camera analyzes the shooting scene and automatically corrects the brightness and contrast to improve the image quality.
DRO stands for “Dynamic Range Optimizer,” a function that automatically optimizes the difference between light and dark parts of an image.

1. MENU (DRO) desired mode

| (Off) | Does not adjust.
| (DRO Standard) | Adjusts the brightness and contrast of the images automatically.
| (DRO plus) | Adjusts image brightness and contrast automatically and strongly.

Notes

- Depending on shooting conditions, it may not be possible to obtain correction effects.

- Only [ISO AUTO] or values from [ISO 80] to [ISO 800] can be set for the ISO value when [DRO plus] is set.

Back to top