Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > MENU items (Shooting) > Position Information (DSC-HX10V only)

## Position Information (DSC-HX10V only)

The GPS triangulating status can be checked. Set the camera to triangulate when the position information is being displayed.

1. MENU (Position Information) on the control wheel

The position information is displayed on your camera.
GPS indicators
The indicator (A) changes according to the strength of GPS signal reception when GPS is activated.

GPS indicators | Triangulating status | GPS reception status
No indicator | Off | [GPS setting] is set to [Off] or an error occurred.
| Difficult | Your camera cannot find a GPS signal, therefore, it cannot acquire the location information. Use your camera in an open area.
| Searching | Searching for GPS satellites. It may take several minutes to start triangulating.
| Triangulating | Your camera is receiving a GPS signal, and can acquire location information. Latitude and longitude (B) are displayed when triangulating.

Satellite and triangulating indicators
The satellite’s position can be checked on the position information display (C). The satellite information acquisition status is displayed on the triangulating indicator (D). The triangulating indicator turns green when triangulation is successfully completed.
Notes

- Even when the camera acquires information from satellites, triangulation may take time or fail according to the time or place.

- Do not cover the GPS sensor with your finger when searching for GPS satellites or when triangulating. This decreases the sensitivity of the GPS sensor and triangulation may fail.

Related Topic
GPS setting (DSC-HX10V only)
GPS (DSC-HX10V only)
Back to top