Cyber-shot User Guide
Print
Top page > Before Use > Names of parts and list of icons displayed on the screen > List of icons displayed on the screen

## List of icons displayed on the screen

List of shooting mode icons
List of viewing mode icons
Icons are displayed on the screen to indicate the camera status.
You can change the screen display using (Display Setting) on the control wheel.

### List of shooting mode icons

Display | Indication
| Battery remaining
| Low battery warning
| Image size/Panorama image size/Quality
9 | Number of recordable images (Dual Rec)
| Eco mode
| Scene Selection
| Shooting mode
| Scene Recognition icon
| White balance
| Metering Mode
| Picture Effect
| Vibration warning
| Anti Blink
| Scene Recognition
| Overlay icon
| Burst Shooting Interval
| Bracket shooting
| Bracket setting
| Smile Detection Sensitivity indicator
1.4 | Zoom scaling

Display | Indication
| Tracking focus
| AE/AF lock
ISO400 | ISO number
| NR slow shutter
125 | Shutter speed
F3.3 | Aperture value
| Wind Noise Reduction
+2.0EV | Exposure value
| AF range finder frame indicator

Display | Indication
| Recording folder
96 | Number of recordable images
CAPTURE | Importing still images
100Min | Recordable time
| Recording Media (Memory card, internal memory)
| GPS Log REC (DSC-HX10V only)
| Direction (DSC-HX10V only)
| Eye-Fi Mode display
| Warning indicator pertaining to still image recording
| GPS triangulating status (DSC-HX10V only)
| Flash mode
C:32:00 | Self-diagnosis display
| AF Illuminator
| Red-eye reduction
| Defocus Effect
| Flash charging

Display | Indication
| Self-timer
| Airplane Mode (DSC-HX10V only)
| Face detection
| Destination (DSC-HX10 only)
| Soft Skin Effect
| Micref Level
| Database file full/Database file error
| Overheating warning
| Write Date
| AF range finder frame
| Spot metering cross-hairs
| Histogram
REC Standby | Recording a movie/Movie standby
0:12 | Recording time (m:s)

### List of viewing mode icons

Display | Indication
| Battery remaining
| Low battery warning
| Image size/Panorama image size/Quality
| View mode
| Eco mode
| TransferJet settings
| 3D images
| Burst Images
| Main image in the burst group
| Protect
| Print order (DPOF)
| Playback zoom

Display | Indication
101-0012 | Folder-file number
2012-1-1 9:30 AM | Recorded date/time of the playback image

Display | Indication
| Playback folder
12/12 | Image number/Number of images recorded in selected date range, folder
| Playback Media (Memory card, internal memory)
| Eye-Fi Mode display
| Flash mode
| Metering Mode
| White balance
C:32:00 | Self-diagnosis display
ISO400 | ISO number

Display | Indication
500 | Shutter speed
+2.0EV | Exposure value
F3.3 | Aperture value
| Direction
| Airplane Mode (DSC-HX10V only)
| GPS information
| Latitude and longitude display
| Database file full/Database file error
| Overheating warning
| Playback
| Variable speed playback
| Playback bar
00:00:12 | Counter
| Histogram
| Volume

Back to top