Cyber-shot User Guide
Print
Top page > Shooting > Using shooting functions > EV

## EV

You can adjust the exposure manually in 1/3 EV steps in a range of –2.0 EV to +2.0 EV.

1. Press the jog dial to select the EV setting.

1. Turn the jog dial to select the desired EV setting.

Adjusting the exposure for better looking images
A: Overexposure (too much light)
B: Correct exposure
C: Underexposure (too little light)

- When the image shot is overexposed, adjust [EV] to the minus side.

- When the image shot is underexposed, adjust [EV] to the plus side.

Note

- If you shoot a subject in extremely bright or dark conditions, or when you use the flash, the exposure adjustment may not be effective.

Related Topic
Using the jog dial
Functions not available in some REC modes
Back to top