Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > Movie shooting menu > Record Setting

## Record Setting

The larger the size of the movie image, the higher the image quality. The higher the amount of data used per second (average bit-rate), the higher the image quality.

1. MENU 1 [Record Setting] desired mode

#### File Format: AVCHD

Records 60i/50i movies, 24p/25p movies or 60p/50p movies in AVCHD format. This file format is suitable for viewing the movie on a high-definition TV.
You can create a Blu-ray Disc, an AVCHD recording disc, or a DVD-Video disc using “PlayMemories Home.”

- 60i/50i movies are recorded at either 60 fields/second or at 50 fields/second, respectively. Both 60i and 50i movies utilize the interlace scanning system, Dolby Digital audio, and the AVCHD format.

- 24p/25p movies are recorded at either 24 frames/second or at 25 frames/second, respectively. Both 24p and 25p movies utilize the progressive scanning system, Dolby Digital audio, and the AVCHD format.

- 60p/50p movies are recorded at either 60 frames/second, or at 50 frames/second, respectively. Both 60p and 50p movies utilize the progressive scanning system, Dolby Digital audio, and the AVCHD format.

| Record Setting | Average bit-rate | Description
| 60i 24M(FX) 50i 24M(FX) | 24 Mbps | Shoots at the highest picture quality of 1920×1080 (60i/50i) size
| 60i 17M(FH) 50i 17M(FH) | 17 Mbps | Shoots at a high picture quality of 1920×1080 (60i/50i) size
| 60p 28M(PS) 50p 28M(PS) | 28 Mbps | Shoots at the highest picture quality of 1920×1080 (60p/50p) size
| 24p 24M(FX) 25p 24M(FX) | 24 Mbps | Shoots at a high picture quality of 1920×1080 (24p/25p) size
| 24p 17M(FH) 25p 17M(FH) | 17 Mbps | Shoots at a standard picture quality of 1920×1080 (24p/25p) size

#### File Format: MP4

Movies shot are recorded in MPEG-4 format, at approximately 30 frames/sec (for 1080 60i-compatible devices) or approximately 25 frames/sec (for 1080 50i-compatible devices), in progressive mode, with AAC audio, mp4 format.

| Record Setting | Average bit-rate | Description
| 1440×1080 12M | 12 Mbps | Shoots at 1440×1080 size
| VGA 3M | 3 Mbps | Shoots at VGA size

Notes

- A telephoto image is produced when [VGA 3M] image size is selected.

- When you create AVCHD discs from movies recorded in [60p 28M(PS)]/[50p 28M(PS)]/[60i 24M(FX)]/[50i 24M(FX)]/[24p 24M(FX)]/[25p 24M(FX)], it will take time, as the image quality must be converted. To save [60p 28M(PS)]/[50p 28M(PS)]/[60i 24M(FX)]/[50i 24M(FX)]/[24p 24M(FX)]/[25p 24M(FX)] movies without converting the image quality, use Blu-ray discs.

Related Topic
File Format
Back to top