Cyber-shot User Guide
Print
Top page > Changing settings > Setup menu > PAL/NTSC Selector (only for 1080 50i-compatible models)

## PAL/NTSC Selector (only for 1080 50i-compatible models)

Plays back movies recorded with the camera on a PAL/NTSC system TV.

1. MENU 3 [PAL/NTSC Selector] desired mode

| PAL | Plays back movies recorded with the camera on a PAL system TV.
| NTSC | Plays back movies recorded with the camera on an NTSC system TV.

Notes

- This function is provided with 1080 50i-compatible devices only. It is not provided with 1080 60i-compatible devices. The 1080 50i-compatible devices have a “50i” mark on the bottom of the camera.

- If you insert a memory card that has previously been formatted with the PAL system, a message telling you that you must re-format the card appears. When you record using the NTSC system, re-format the memory card or use another memory card.

- When the NTSC mode is selected, the “Running on NTSC.” message always appears on the start-up screen each time you turn the camera on.

Back to top