Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > Still shooting menu > Drive Mode

## Drive Mode

You can set a drive mode, such as continuous, self-timer, or bracket shooting.
[Drive Mode] can be set using the / (Drive Mode) button.

1. MENU 2 [Drive Mode] desired mode

- Press / on the control wheel to select the desired setting when selecting a mode with its own setting values.

| (Single Shooting) | The camera shoots a single image without using the self-timer.
| (Cont. Shooting) | The camera shoots continuous images while the shutter button is pressed.
| (Spd Priority Cont.) | Shoots images continuously at high speed while you press and hold down the shutter button. Focus and brightness settings of the first shot are used for the following shots.
| (Self-timer) | Sets the self-timer to a 10-second or 2-second delay. When you press the shutter button, the self-timer lamp flashes and a beep sounds until the shutter operates. To cancel, press / again.
| (Self-portrait) | Sets the self-timer to Self-portrait timer. When the camera detects the specified number of faces, a beep sounds, and the shutter operates 2 seconds later.
| (Self-timer(Cont)) | The camera shoots continuous frames 10 seconds later after you press the shutter button. Select the number of frames from three or five.
| (Bracket: Cont.) | Shoots three images, each with different degrees of brightness. You can set the value of bracket deviation (steps).
| (WB bracket) | Shoots three images, each with different degrees of brightness according to the selected settings of white balance, color temperature and color filter. You can select the value of bracket deviation (steps) from [Lo] or [Hi].

Related Topic
Drive Mode
Still shooting menu items not available in some REC modes
Back to top