Cyber-shot User Guide
Print
Top page > Shooting > Using shooting functions > Exposure Comp.

## Exposure Comp.

You can adjust the exposure manually in 1/3 EV steps in a range of –3.0 EV to +3.0 EV.

1. Press the / (Exposure Comp.) on the control wheel.

1. Select the desired value using the control wheel.

Adjusting the exposure for better looking images
A: Overexposure (too much light)
B: Correct exposure
C: Underexposure (too little light)

- When the image shot is overexposed, adjust [Exposure Comp.] to the minus side.

- When the image shot is underexposed, adjust [Exposure Comp.] to the plus side.

Notes

- If you shoot a subject in extremely bright or dark conditions, or when you use the flash, the exposure adjustment may not be effective.

Related Topic
Functions not available in some REC modes
Back to top