Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > MENU items (Shooting) > Cont. Shooting Settings

## Cont. Shooting Settings

The camera shoots up to 10 continuous frames in one burst when you hold down the shutter button.

1. MENU (Cont. Shooting Settings) desired mode

| (Off) | Records a single image.
| (High) | Shoots up to 10 images per second in succession.
| (Low) | Shoots up to 2 images per second in succession.

Notes

- [Flash] is set to [Off].

- When recording with the self-timer, a series of up to 10 images is recorded.

- The recording interval becomes longer, depending on the setting for the image size.

- [Focus], [White Balance], and [EV] are adjusted for the first image, and these settings are also used for the other images.

- When the [Cont. Shooting Settings] is set to [High] or [Low], up to ISO800 can be selected for ISO speed.

- [VGA] image size will be set while recording on internal memory.

- When the battery level is low, or when the internal memory or a memory card is full, the burst stops.

- In slow shutter speed conditions, the burst of shots per second may be decreased.

- You may not be able to set some MENU items depending on the selected REC mode. For details, see “MENU items not available in some REC modes.” [Details]

Back to top