Cyber-shot User Guide
Print
Top page > Precautions / About this camera > Precautions > Battery charger

## Battery charger

- Only NP-BN1 type battery packs (and no others) can be charged in the battery charger (supplied). Batteries other than the specified kind may leak, overheat, or explode if you attempt to charge them, posing a risk of injury from electrocution and burns.

- Remove the charged battery pack from the battery charger. If you leave the charged battery pack in the charger, battery life may be shortened.

- The CHARGE lamp of the supplied battery charger flashes in either way:

- Fast flashing: Turns the light on and off repeatedly at the interval of approximately 0.15 seconds.

- Slow flashing: Turns the light on and off repeatedly at the interval of approximately 1.5 seconds.

- When the CHARGE lamp flashes fast, remove the battery pack being charged, and then insert the same battery pack into the battery charger securely again. When the CHARGE lamp flashes fast again, this may indicate a battery error or that a battery pack other than the specified type has been inserted. Check that the battery pack is the specified type. If the battery pack is the specified type, remove the battery pack, replace it with a new one or another one and check if the battery charger operates correctly. If the battery charger operates correctly, a battery error may have occurred.

- When the CHARGE lamp flashes slowly, it indicates that the battery charger stops charging temporarily on standby. The battery charger stops charging and enters the standby status automatically when the temperature is outside of the recommended operating temperature. When the temperature gets back within the appropriate range, the battery charger resumes charging and the CHARGE lamp lights up again. We recommend charging the battery pack in an ambient temperature of between 10°C to 30°C (50°F to 86°F).

Back to top