Cyber-shot User Guide
Print
Top page > Shooting > Using shooting functions > Burst/Bracket

## Burst/Bracket

You can select Single (single-image), Burst or Bracket as the shooting mode.

1. Press (Burst Settings) on the control wheel.

1. Select the desired mode with the control wheel.

| (Single) | The camera shoots a single image.
| (Burst) | The camera shoots 10 continuous frames in one burst when you hold down the shutter button.
| (Bracket) | The camera shoots a series of 3 images each with a different setting.

Notes

- [Flash] is set to [Off].

- When recording with the self-timer, a series of 10 images is recorded if [Burst] is selected and a series of 3 images, each with different settings, is recorded if [Bracket] is selected.

- When [Burst] is selected, [Focus], [White Balance], and [EV ] are adjusted for the first image, and these settings are also used for the other images.

- When the battery level is low, or when the internal memory or a memory card is full, the burst stops.

- [VGA] image size will be set while recording on internal memory.

- You may not be able to set some functions or MENU items depending on the selected REC mode. For details, see “Functions not available in some REC modes” [Details] and “MENU items not available in some REC modes.” [Details]

Related Topic
Burst Shooting Interval
Bracket Setting
Back to top