Cyber-shot User Guide
Print
Top page > Shooting > Using shooting functions > Cont. Shooting Settings

## Cont. Shooting Settings

You can select Single (single-image) or Burst as the shooting mode.

1. Press (Cont. Shooting Settings) on the control wheel.

1. Select the desired mode with the control wheel.

| (Single Shooting) | The camera shoots a single image.
| (Continuous Shooting) | The camera shoots up to 10 continuous frames in one burst when you hold down the shutter button.

Notes

- [Flash] is set to [Off].

- When recording with the self-timer, a series of up to 10 images is recorded.

- [Focus], [White Balance], and [EV] are adjusted for the first image, and these settings are also used for the other images.

- When the battery level is low, or when the internal memory or a memory card is full, the burst stops.

- [VGA] image size will be set while recording on internal memory.

Related Topic
Cont. Shooting Interval
Functions not available in some REC modes
MENU items not available in some REC modes
Back to top