# How to Use

# IC Recorder ICD-PX333/PX333F

## Tuning in an FM radio station automatically (automatic scanning) (ICD-PX333F only)

The headphone cord of headphones is an FM antenna, therefore, connect headphones to the (headphone) jack when listening to the FM radio.

#### Note

- During FM reception, the DPC function and noise cut function do not work.

1. In the stop mode, select DISP/MENU - “FM Radio,” and then press PLAY/STOP・ENTER.

   The IC recorder enters the FM radio mode.

2. Press DISP/MENU briefly to move the cursors (, ) to both sides of the frequency display on the upper line in the display window.

   The IC recorder is now ready for tuning in a station by scanning frequencies.

3. Press and hold – or + until the frequency digits begin to change on the display.
   The IC recorder automatically scans the radio frequencies and stops when it finds a clear station.
4. Press (stop) to turn the FM radio off.

#### Hint

- If you cannot tune in a station, press – or + repeatedly to change the frequency step by step.

### Related Topic

- Switching the FM radio output between speaker and headphones (ICD-PX333F only)
- Tuning in an FM radio station manually (manual scanning) (ICD-PX333F only)