# How to Use

# IC Recorder ICD-PX333/PX333F

## Selecting the microphone sensitivity (Mic Sensitivity)

You can set the microphone sensitivity for the built-in microphone. Set this menu item before you start recording.

1. In the stop or recording mode, select DISP/MENU - “Detail Menu” - “Mic Sensitivity,” and then press PLAY/STOP・ENTER.

2. Press – or + to select the desired level of the microphone sensitivity, and then press PLAY/STOP・ENTER.
3. Press (stop) to exit the menu mode.

#### Descriptions of menu items

You can select one of the menu items available.

High:

To record a sound far away from the IC recorder or a low sound, such as recording in a spacious room.

Medium:

To record the sound of a normal conversation or meeting, such as recording in a meeting space or during interview.

(Initial setting)

Low:

To record dictation with a microphone in front of your mouth, a sound near the IC recorder, or a loud sound.

#### Note

- During FM recording, the Mic Sensitivity setting is disabled (ICD-PX333F only).

### Related Topic

- Recording FM radio broadcasts (ICD-PX333F only)