# How to Use

# IC Recorder ICD-PX333/PX333F

## Menu list

The list below shows the menu items and in which operation mode the IC recorder can make changes to the menus.

- Add/Overwrite: Stop mode
  - Add: Adding a recording to a previously recorded file (Add)
  - Overwrite: Adding an overwrite recording during playback (Overwrite)
- VOR: Stop mode, Recording mode

  Starting to record automatically in response to sound – the VOR function

- DPC(Speed Control): Stop mode, Playback mode

  Adjusting the playback speed – the DPC (Digital Pitch Control) function

- Easy Search: Stop mode, Playback mode

  Searching the desired point quickly (Easy Search)

- Alarm: Stop mode

  Playing back a file at a desired time with an alarm

- AVLS: Stop mode, Playback mode

  Turning the AVLS function on or off (European models only)

- Protect: Stop mode

  Protecting a file

- Divide: Stop mode
  - Divide Current Position: Stop mode

    Dividing a file at the current position

  - Divide All Track Marks: Stop mode

    Dividing a file at all the track mark positions

- Move & Copy: Stop mode
  - Move File: Stop mode

    Moving a file to a different folder

  - File Copy: Stop mode

    Copying a file to the other memory

- Delete: Stop mode
  - Erase Track Mark: Stop mode

    Erasing a track mark

  - Erase All Track Marks: Stop mode

    Erasing all the track marks in the selected file at one time

  - Erase All: Stop mode

    Erasing all files in a folder

- Select Memory: Stop mode

  Selecting the memory

- FM Radio(*): Stop mode

  Tuning in an FM radio station manually (manual scanning) (ICD-PX333F only)

- Auto Preset(*): FM radio reception mode(*)

  Presetting FM radio stations automatically (ICD-PX333F only)

- DX/LOCAL(*): FM radio reception mode(*), FM radio recording mode(*)

  Switching the receiver sensitivity of the FM radio (ICD-PX333F only)

- Scan Sensitivity(*): FM radio reception mode(*)

  Switching the scanning sensitivity (ICD-PX333F only)

- Audio Output(*): FM radio reception mode(*), FM radio recording mode(*)

  Switching the FM radio output between speaker and headphones (ICD-PX333F only)

- Detail Menu: Stop mode, Playback mode, Recording mode
  - REC Mode:

    Selecting the recording mode (REC Mode)

  - Mic Sensitivity: Stop mode, Recording mode

    Selecting the microphone sensitivity (Mic Sensitivity)

  - LCF(Low Cut): Stop mode, Recording mode

    Reducing noise when recording (LCF(Low Cut))

  - Select Input: Stop mode

    Selecting the input mode (Select Input)

  - Continuous Play: Stop mode, Playback mode

    Playing back a file repeatedly

  - Noise Cut Level: Stop mode, Playback mode

    Reducing noise in the playback sound and making the human voice clearer – the noise cut function

  - LED: Stop mode

    Turning the operation indicator on or off (LED)

  - Language: Stop mode

    Setting the display language

  - Date&Time: Stop mode

    Setting the clock using the menu

  - Time Display: Stop mode

    Selecting the clock display (Time Display)

  - Beep: Stop mode

    Turning the beep sound on or off (Beep)

  - Auto Power Off: Stop mode

    Setting the time period for the IC recorder to turn off (Auto Power Off)

  - Format: Stop mode

    Formatting the memory (Format)

* For ICD-PX333F only