# How to Use

# IC Recorder ICD-PX333/PX333F

## Adjusting the playback speed – the DPC (Digital Pitch Control) function

You can adjust the playback speed in a range from 0.50 times to 2.00 times. The file is played back in natural tones by means of a digital processing function.

1. In the stop or playback mode, select DISP/MENU - “DPC(Speed Control),” and then press PLAY/STOP・ENTER.

2. Press – or + to select “ON,” and then press PLAY/STOP・ENTER.
3. During playback, press – or + to adjust the playback speed.

   The speed decreases by 0.05 times (from ×0.50 to ×1.00).

   The speed increases by 0.10 times (from ×1.00 to ×2.00).

   When you press and hold each button, you can change the speed continuously.

   The playback speed is set to “×0.70” when you purchase the IC recorder.

#### Note

- The noise cut function does not work if you set “DPC(Speed Control)” to “ON.”

#### Hint

- To resume normal playback speed, select “OFF” in step 2.