# How to Use

# IC Recorder ICD-PX333/PX333F

## Reducing noise when recording (LCF(Low Cut))

You can set the LCF (Low Cut Filter) function to cut a low frequency to reduce the roaring noise from wind; therefore you can record a file more clearly.

1. In the stop or recording mode, select DISP/MENU - “Detail Menu”-“LCF(Low Cut),” and then press PLAY/STOP・ENTER.

2. Press – or + to select “ON” or “OFF,” and then press PLAY/STOP・ENTER.
3. Press (stop) to exit the menu mode.

#### Descriptions of menu items

You can select one of the menu items available.

ON:

The LCF function is activated.

OFF:

The LCF function is canceled.

(Initial setting)

#### Note

- During FM recording, the LCF function does not work (ICD-PX333F only).

#### Hint

- Select “OFF” in step 2 to cancel the LCF function.

### Related Topic

- Recording FM radio broadcasts (ICD-PX333F only)