# How to Use

# IC Recorder ICD-PX333/PX333F

## Monitoring sound while recording

If you connect headphones to the (headphone) jack, you can monitor the recording.

1. Connect headphones to the (headphone) jack.
2. Press VOL -/+ to adjust the monitoring volume.
   Monitoring volume does not affect to the recording level.

#### Note

- When the cord of headphones touches the IC recorder while you are monitoring the recording, the IC recorder may record a rustling noise. The rustling noise can be reduced by holding the cord away from the IC recorder.

### Related Topic

- Recording sound from the built-in microphones