# How to Use

# IC Recorder ICD-PX333/PX333F

## Display when the HOLD function is set

#### Note

- The window shown above displays indications, numbers or items for explanatory purposes. The actual window may differ from those displayed here.

1. Message displayed when the HOLD function is set to “ON.”

   “HOLD” appears for approximately 3 seconds when you slide the HOLD・POWER ON/OFF switch in the direction of “HOLD.”

### Related Topic

- Preventing unintentional operations (HOLD)
- Releasing the HOLD function