# How to Use

# IC Recorder ICD-PX333/PX333F

## Playing back the recorded sound

1. Slide the HOLD・POWER ON/OFF switch in the direction of “POWER ON/OFF” to turn on the IC recorder, or towards the center to release the IC recorder from the HOLD status.
   The stop mode window appears.
2. Select the desired file to be played back.
   If you do not select a file, the file just recorded will be played back.
3. Press PLAY/STOP・ENTER.

   Playback starts, and the operation indicator () will light in green.

4. Press VOL –/+ to adjust the volume.

#### Note

- For the customers in Europe only:

  When “AVLS” is set to “ON” in the menu and the “AVLS” indicator lights, you cannot adjust the volume to a level that exceeds the AVLS-specified level. If you want to turn off the function and play back files at the original volume, use the menu to set “AVLS” to “OFF.”

#### Hint

- Press (stop) to stop playback.

### Related Topic

- Turning the power on
- Releasing the HOLD function
- Selecting a folder and a file
- Various operations while playing