# How to Use

# IC Recorder ICD-PX333/PX333F

## Reducing noise in the playback sound and making the human voice clearer – the noise cut function

The noise cut function reduces ambient noise other than the human voice, which makes the human voice clearer when you listen to the playback sound.

1. In the stop or playback mode, slide the NOISE CUT switch to“ON.”
2. Select DISP/MENU - “Detail Menu” - “Noise Cut Level,” and then press PLAY/STOP・ENTER.

3. Press – or + to select “Maximum” or “Medium,” and then press PLAY/STOP・ENTER.
4. Press (stop) to exit the menu mode.

#### Descriptions of menu items

You can select one of the menu items available.

Maximum:

The noise cut level will be higher.

(Initial setting)

Medium:

The noise cut level will be lowered. Select this item when you cannot hear the sound clearly by setting the noise cut function to “Maximum.”

#### Note

- The effect of the noise cut function may be different depending on the condition of the recorded voice.
- When playing back files using the built-in speaker or recording an FM radio broadcast (ICD-PX333F only), the noise cut function does not work.
- When you are using the built-in speaker, the noise cut function does not work.

#### Hint

- To cancel the noise cut function, slide the NOISE CUT switch to “OFF.”

### Related Topic

- Recording FM radio broadcasts (ICD-PX333F only)