# How to Use

# IC Recorder ICD-PX333/PX333F

## Design and specifications

#### Capacity (User available capacity)

4 GB (approx. 3.60 GB = 3,865,470,566 Byte)

A small amount of the internal memory is used for file management and therefore not available for user storage.

#### Maximum number of folders (for a drive)

400 folders

#### Maximum number of files (for a folder)

199 files

#### Maximum number of files (for a drive)

4,074 files (When 21 folders are contained in a drive.)

#### Frequency range

SHQ: 75 Hz - 20,000 Hz

HQ: 75 Hz - 17,000 Hz

SP: 75 Hz - 14,000 Hz

LP: 75 Hz - 3,500 Hz

#### Compatible file formats

MP3 (*1)

Bit rate: 32 kbps - 320 kbps (Supports variable bit rate (VBR))

Sampling frequencies: 16/22.05/24/32/44.1/48 kHz

File extension: .mp3

#### Sampling frequencies and bit rates for MP3 files recorded in each recording mode

SHQ: 44.1kHz, 192kbps

HQ: 44.1kHz, 128kbps

SP: 44.1kHz, 48kbps

LP: 11.025kHz, 8kbps

#### Frequency range for the FM radio reception (*2)

87.50 MHz - 108.00 MHz

IF 128 kHz

#### FM antenna (*2)

Stereo headphone cord antenna

#### Speaker

Approx. 28 mm (1 1/8 in.) dia.

#### Input/Output

Microphone jack (minijack, stereo)

input for plug in power, minimum input level 0.6 mV

Headphone jack (minijack, stereo)

output for 8 Ω - 300 Ω impedance headphones

USB connector (USB Mini-B jack)

High-Speed USB compatible

Memory Stick Micro™(M2™)/microSD memory card slot

#### Playback speed control (DPC)

2.00 times - 0.50 times

#### Power output

300 mW

#### Power requirements

Two LR03 (size AAA) alkaline batteries (supplied): 3.0 V DC

Two NH-AAA-B2KN/NH-AAA-B2EN rechargeable batteries (not supplied): 2.4 V DC

#### Operating temperature

5 °C - 35 °C (41 °F to 95 °F)

#### Dimensions (w/h/d) (not incl. projecting parts and controls) (JEITA) (*3)

Approx. 37.5 mm × 114.0 mm × 20.9 mm (1 1/2 in. × 4 1/2 in. × 27/32 in.)

#### Mass (JEITA) (*3)

Approx. 74 g (2 5/8 oz) including two LR03 alkaline batteries

#### Supplied accessories

See “Quick Start Guide” supplied with your IC recorder.

Design and specifications are subject to change without notice.

*1 The playback of MP3 files recorded using the IC recorder is also supported. Not all encoders are supported.

*2 ICD-PX333F only

*3 Measured value by the standard of JEITA (Japan Electronics and Information Technology Industries Association)

### Maximum recording time (*1)(*2)

The maximum recording time of all the folders is as follows.

#### 192kbps(MONO)(SHQ)(///)

Built-in memory

44 h. 40 m.

Memory card

2 GB: 22 h. 20 m.

4 GB: 44 h. 40 m.

8 GB: 89 h. 25 m.

16 GB: 178 h.

32 GB: 357 h.

#### 128kbps(MONO)(HQ)()

Built-in memory

67 h. 5 m.

Memory card

2 GB: 33 h. 30 m.

4 GB: 67 h. 5 m.

8 GB: 134 h.

16 GB: 268 h.

32 GB: 536 h.

#### 48kbps(MONO)(SP)

Built-in memory

178 h.

Memory card

2 GB: 89 h. 25 m.

4 GB: 178 h.

8 GB: 357 h.

16 GB: 715 h.

32 GB: 1,431 h.

#### 8kbps(MONO)(LP)

Built-in memory

1,073 h.

Memory card

2 GB: 536 h.

4 GB: 1,073 h.

8 GB: 2,147 h.

16 GB: 4,294 h.

32 GB: 8,589 h.

(h.: hours/m.: minutes)

*1 When you are going to record continuously for a long time, you may have to replace the batteries with new ones in the midst of recording. For details on the battery life, see “Battery life”.

*2 The maximum recording time in this topic for your reference only, and may differ depending on the card specifications.