# Troubleshooting

# IC Recorder ICD-PX333/PX333F

## Sound comes from only one channel.

- When audio output of an external device connected to the IC recorder is monaural and the recording mode is set to “192kbps(MONO)” (SHQ) or “128kbps(MONO)” (HQ), sounds are recorded only in one channel. In this case, set the recording mode to “48kbps(MONO)” (SP) or “8kbps(MONO)” (LP) in the menu.

### Related Topic

- Selecting the recording mode (REC Mode)