# How to Use

# IC Recorder ICD-PX333/PX333F

## Switching the receiver sensitivity of the FM radio (ICD-PX333F only)

You can set the receiver sensitivity when listening to the FM radio.

1. In the FM radio reception mode, select DISP/MENU - “DX/LOCAL,” and then press PLAY/STOP・ENTER.

2. Press – or + to select “DX” or “LOCAL,” and then press PLAY/STOP・ENTER.
3. Press (stop) to exit the menu mode.

#### Description of menu items

You can select one of the menu items available.

DX:

Normally, select this setting.

(Initial setting)

LOCAL:

When there is interference or collapsing caused by a intense electric field around the transmitting antenna of the broadcasting station, etc., select this setting.

#### Note

- Select “DX” when the IC recorder reception status is not good due to a weak signal.