;; Realtek RTL8139/810x/8169(S/SB)/8110(S/SB) all in one NDIS Driver
;;
;; Copyright 2004, Realtek Semiconductor Corporation
;;
;; .this release is primarily for OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                               
CatalogFile.NT    = netrtOEM.cat
DriverVer      = 12/02/2004,5.620.1202.2004

[Manufacturer]
%Realtek%   = Realtek, NT.5.1

[ControlFlags]
ExcludeFromSelect = PCI\VEN_10EC&DEV_8139
ExcludeFromSelect = PCI\VEN_10EC&DEV_8169
;ExcludeFromSelect = PCI\VEN_10EC&DEV_8168

[Realtek]
; DisplayName            Section            DeviceID
; -----------            -------            --------
%RTL8169.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8169
%RTL8139.DeviceDesc%    = RTL8139.ndi,      PCI\VEN_10EC&DEV_8139&REV_10
%RTL8139P.DeviceDesc%   = RTL8139P.ndi,     PCI\VEN_10EC&DEV_8139&REV_20
%RTL8169.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
%RTL8139.DeviceDesc%    = RTL8139.ndi,      PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_10
%RTL8139P.DeviceDesc%   = RTL8139P.ndi,     PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_20
%RTL8139.DeviceDesc% = RTL8139_TOS.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00011179
%RTL8139.DeviceDesc% = RTL8139_TOS.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00021179
%RTL8139Panasonic.DeviceDesc% = RTL8139.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_834310F7
;%RTL8168.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8168
;%RTL8168.DeviceDesc%    = RTL8169.ndi,      PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC

;;========================================================================================

[Realtek.NT.5.1]; This section will only be installed by Windows XP
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8169
%RTL8169.DeviceDesc%    = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
%RTL8139.DeviceDesc%    = RTL8139x.ndi,     PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_10
%RTL8139P.DeviceDesc%   = RTL8139Px.ndi,    PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_20
;%RTL8168.DeviceDesc%   = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8168
;%RTL8168.DeviceDesc%   = RTL8169x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC
;IDs for GBE
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_81CB104D ;ASUS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60201915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60211915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60221915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60231915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_60241915 ;Acorp
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_202F161F ;Arima
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F7A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F8A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03F9A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03FAA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0405A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0406A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_040CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_041CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0449A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_044AA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045BA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045EA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_045FA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0460A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0461A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0462A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_046DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_046EA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0477A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049CA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049EA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_049FA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A0A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A1A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A2A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CAA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CBA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CCA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04CDA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0526A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0528A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_052AA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0542A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0543A0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054BA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054DA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_054FA0A0 ;Aopen
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_23031565 ;Biostar
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_23041565 ;Biostar
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_F446270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2793270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_272B270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_273B270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_F644270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_7842270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_7860270F ;Chaintech
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00031854 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_07041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_09041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08051558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08061558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08071558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08081558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_08091558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05001558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05031558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05041558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05051558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05061558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05071558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05081558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05091558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_05701558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04701558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04761558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04801558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_04A01558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_47011558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_47021558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03751558 ;Clevo
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00361025 ;Compal
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_001214C0 ;Compal
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_001714C0 ;Compal
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00711025 ;Compal
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3085103C ;Compal
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_100A15BD ;DFI
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B111019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18651019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18731019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18741019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18531019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_18031019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B081019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_1B101019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F271019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F471019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F521019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0F561019 ;ECS
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_90221695 ;Epox
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_28211509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92171509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92181509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92201509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92221509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92231509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92261509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_921F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92671509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92691509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_926F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92701509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92731509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92741509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92751509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92761509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92771509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92781509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_92791509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927A1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927B1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927C1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927D1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927E1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_927F1509 ;FIC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C06105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C07105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C08105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C09105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C0F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C10105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C11105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C12105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C13105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C14105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C15105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C16105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C17105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C18105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C19105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C1F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C41105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C42105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C43105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C44105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C45105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C46105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C47105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C48105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C49105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C4F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C51105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C52105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C53105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C54105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C55105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C56105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C57105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C58105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C59105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C20105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C21105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C22105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C23105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C24105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C25105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C26105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C27105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C28105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C29105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C2F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C30105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C31105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C32105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C33105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C34105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C35105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C36105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C37105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C38105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C39105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C3F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5A105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5B105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5C105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5D105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5E105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C5F105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C60105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C61105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C62105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C63105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C64105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C65105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C70105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C71105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C72105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C73105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C74105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C75105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C80105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C81105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C82105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C83105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C84105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C85105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C90105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C91105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C92105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C93105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C94105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0C95105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA0105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA1105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA2105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA3105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA4105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA5105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA6105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA7105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA8105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CA9105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAA105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAB105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAC105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAD105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAE105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0CAF105B ;Foxconn
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0001458 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0091631 ;GIGABYTE
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00071170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_000A1170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_000B1170 ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500417FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500517FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_500617FF ;Inventec
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_10EC16F3 ;Jetway
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_811016F3 ;Jetway
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01241071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01711071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80501071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_83171071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_80661071 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_C0081631 ;Mitac
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_01611462 ;MS-1016
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_702C1462 ;MS-6702
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_728C1462 ;MS-6728
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_758C1462 ;MS-6758
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_771C1462 ;MS-6771
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_788C1462 ;MS-6788
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_799C1462 ;MS-6799
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_003C1462 ;MS-7003
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006C1462 ;MS-7006
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_008C1462 ;MS-7008
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_2A17103C ;MS-7025
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_033C1462 ;MS-7033
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E00F1631 ;MS-7069
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_E0111631 ;MS-7069
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_82971033 ;NEC
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_82B61033 ;NEC(Compal)
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_833810F7 ;Panasonic
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0729152D ;Quanta
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0730152D ;Quanta
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058A17FF ;Quanta
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_058B17FF ;Quanta
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_107D1734 ;Quanta
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_308F103C ;Quanta
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_31558452 ;Topstar
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_5003148C ;TUL
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020B14FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020E14FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020F14FF ;Twinhead
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_020E103C ;Twinhead
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_51081584 ;Uniwill
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_003317C0 ;Wistron
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_006E1025 ;Wistron
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_00791025 ;Wistron
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_105317C0 ;Wistron
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_109417C0 ;Wistron
%RTL8169.DeviceDesc% = RTL8169x.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_3081103C ;Wistron
;IDs for FE
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10451043 ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_17651043 ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80261043 ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_802F1043 ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_805B1043 ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80B31043 ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80DA104D ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80EA104D ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_B031144D ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_C00C144D ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_D0071631 ;ASUS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1000147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1002147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1004147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1005147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1006147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1400147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1401147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1800147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1C00147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7402147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7403147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7404147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7405147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7406147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A401147B ;Abit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60001915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60011915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60021915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60031915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60041915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60101915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60111915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60121915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60131915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60141915 ;Acorp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01771468 ;Ambit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00201468 ;Ambit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00301468 ;Ambit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00501468 ;Ambit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00601468 ;Ambit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_102113BD ;Ambit
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_36021961 ;AMOI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101110FD ;Andev
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_007CA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00B9A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00BAA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00C9A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00CCA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00CEA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00D1A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00D9A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_015FA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0173A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0174A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0175A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0176A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0177A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0178A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0179A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_017AA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_017BA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_017CA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_017DA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_017EA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_017FA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0180A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0181A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0182A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0183A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0184A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0185A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0186A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_019BA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_019CA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01A9A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01AAA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01B3A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01B4A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01B7A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01DBA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01DCA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01DDA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01DEA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01DFA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01E0A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01E1A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01E2A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01F5A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0204A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_020DA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0212A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_021AA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_022AA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_022BA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_022DA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0243A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0244A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0245A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_025FA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0260A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_026BA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_026CA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_026DA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_026EA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_026FA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0291A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0292A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0293A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0294A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0295A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0296A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0297A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02A0A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02A3A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02A4A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02A5A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02A6A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02A7A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02A8A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02A9A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02AAA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02ABA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02ACA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02ADA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02BBA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0376A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0377A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0378A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0393A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0394A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03DDA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03DEA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03DFA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03E0A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03EDA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03EEA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03F7A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03F8A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03F9A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03FAA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0405A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0406A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_040CA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_041CA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_045BA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_045CA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_045DA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_045EA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0477A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_047BA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0495A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0496A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0497A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0498A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0499A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_049AA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_049BA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04A6A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04A7A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04A8A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04A9A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04AAA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04ABA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04ACA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04CEA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04D4A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0524A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0525A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0527A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0529A0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_052BA0A0 ;Aopen
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00201468 ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0122107B ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2016161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2025161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2026161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2027161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2028161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_6102161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_202A161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_202C161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_202D161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_202F161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2030161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2031161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2033161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2034161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2035161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2039161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_203A161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_203B161F ;Arima
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3089103C ;Arima(HP)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_B900156D ;Alphatop
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_B901156D ;AlPhatop
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_B730156D ;AlPhatop
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_AB1C17EB ;APLUX
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10021816 ;AZZA
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10041816 ;AZZA
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_20021816 ;AZZA
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_30011816 ;AZZA
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_020114CB ;Billionton
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00121565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00381565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00391565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00A21565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00A31565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00C01565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00C41565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00F01565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00F21565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_23001565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_23041565 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01021793 ;Biostar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_72601265 ;CASIO
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A162270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A66A270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A666270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7176270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7842270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3105270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_270C270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_270D270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_270E270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_270F270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A165270F ;Chaintech
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00651025 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_006B103C ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_006D103C ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0012103C ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_001214C0 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_001514C0 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_001714C0 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0020103C ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00711025 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100A1734 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10338193 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10338139 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_104E1734 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_111C10CF ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1179FF00 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_200017AA ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3085103C ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_FF001179 ;Compal
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00031854 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01201558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02851558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02871558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02951558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03501558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03601558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04011558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04021558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04031558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04201558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04701558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_04801558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05011558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05021558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05031558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05041558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05051558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05061558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05071558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05081558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05091558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08011558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08021558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08031558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08041558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08051558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08061558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08071558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08081558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08091558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_19001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_20001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_22631558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_30001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_42011558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_56001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_72601558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_85861558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_88001558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_88801558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_05701558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_47021558 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_72601265 ;Clevo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00031FC2 ;DCC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100115BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100315BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100415BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100515BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100615BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100715BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100815BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100915BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100A15BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100F15BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101115BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101315BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_500C15BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_500D15BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_500E15BD ;DFI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_000114C2 ;DTK
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_23428139 ;Dr.Kaiser Systemhaus
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_09621019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_09701019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_09731019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_09751019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A011019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A201019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A251019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A261019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A361019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A371019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A381019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A391019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A401019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A411019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A421019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A431019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A441019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A451019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A461019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A471019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A481019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A491019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A511019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A521019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A531019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A541019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A551019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A561019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A571019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A581019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A591019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A601019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A611019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A621019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A631019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A641019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A651019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A661019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A671019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A681019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A691019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A701019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A711019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A721019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A731019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A741019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A751019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A761019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A771019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A781019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A791019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A801019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A811019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A821019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A831019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A841019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A851019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0A861019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0F201019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0F221019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0F271019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0F431019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0101019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0111019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0121019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0131019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0141019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0201019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0211019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0221019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0231019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0241019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0301019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0311019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0321019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0331019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0341019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_B5511019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0F031019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18011019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18021019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18031019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18041019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18051019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18061019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18071019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18081019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18091019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18101019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18111019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18121019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18131019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18141019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18151019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18161019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18171019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18181019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18191019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18201019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18311019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18321019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18331019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18341019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18351019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18361019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18371019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18381019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18391019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18401019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18411019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18421019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18431019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18441019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18451019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18461019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18471019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18481019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18491019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18501019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18511019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18521019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18531019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18541019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18551019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18561019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18571019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18581019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18591019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18601019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18611019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18621019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18631019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18641019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18651019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18661019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18671019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18681019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18691019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18701019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18711019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18721019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18731019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18741019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18751019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18761019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18771019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18781019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18791019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18801019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18811019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18821019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18831019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18841019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18851019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18861019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18871019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18881019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18891019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18901019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18911019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B011019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B021019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B031019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B041019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B051019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B061019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B071019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B081019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B091019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B101019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B111019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B121019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B131019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B141019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B151019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B161019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B171019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B181019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B191019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1B201019 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_215714A4 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_215814A4 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_215914A4 ;ECS
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90011695 ;EPoX
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_40011695 ;EPoX
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01021664 ;Fastfame
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_22201509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_23201509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_24201509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_24211509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_24221509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_24231509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_28211509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90031509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90041509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90051509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90061509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_900C1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_900D1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_900E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_900F1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90101509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90121509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90141509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90161509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90191509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_901A1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_901B1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_901C1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_901E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_901F1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90201509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90211509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90221509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90231509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90271509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_902A1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_902B1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90301509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90311509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90331509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90351509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90361509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90371509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90381509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90391509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90401509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90411509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90421509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90431509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90441509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90491509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_904A1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90501509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90531509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90551509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90561509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90581509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90591509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_905E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_90601509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92021509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92061509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92071509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92091509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_920A1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_920B1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_920D1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_920E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_920F1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92101509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92121509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92131509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92141509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92151509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92161509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92171509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92181509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92191509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_921A1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_921B1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_921C1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_921D1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_921E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_921F1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92201509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92211509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92221509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92231509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92241509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92251509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92261509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92271509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92281509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92291509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_922A1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_922B1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_922C1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_922D1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_922E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_922F1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92301509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92311509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92321509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92331509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92341509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92351509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92361509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92371509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92381509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92391509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_923A1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_923B1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_923C1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_923D1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_923E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_923F1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92401509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92411509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92421509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92431509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92441509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92451509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92461509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92471509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92481509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92491509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_924A1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_924B1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_924C1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_924D1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_924E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_924F1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92671509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92691509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_926B1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_926E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_926F1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92701509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92731509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92741509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92751509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92761509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92771509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92781509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_92791509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_927A1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_927B1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_927C1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_927D1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_927E1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_927F1509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_99161509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_99181509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_99191509 ;FIC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10F110CF ;Fujitsu(Quanta)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10F310CF ;Fujitsu
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_11BD10CF ;Fujitsu
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_121310CF ;Fujitsu
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_12CE10CF ;Fujitsu
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_201410CF ;Fujitsu
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00311025 ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00411025 ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C06105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C07105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C08105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C09105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C0A105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C0B105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C0C105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C0D105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C0E105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C0F105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C10105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C11105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C12105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C13105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C14105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C15105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C16105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C17105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C18105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C19105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C1A105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C1B105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C1C105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C1D105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C1E105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C1F105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C41105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C42105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C43105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C44105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C45105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C46105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C47105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C48105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C49105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C4A105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C4B105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C4C105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C4D105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C4E105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C4F105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C51105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C52105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C53105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C54105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C55105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C56105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C57105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C58105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C59105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C20105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C21105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C22105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C23105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C24105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C25105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C26105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C27105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C28105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C29105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C2A105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C2B105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C2C105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C2D105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C2E105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C2F105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C30105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C31105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C32105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C33105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C34105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C35105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C36105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C37105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C38105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C39105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C3A105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C3B105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C3C105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C3D105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C3E105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C3F105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C5A105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C5B105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C5C105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C5D105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C5E105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C5F105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C60105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C61105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C62105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C63105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C64105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C65105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C70105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C71105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C72105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C73105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C74105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C75105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C80105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C81105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C82105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C83105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C84105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C85105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C90105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C91105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C92105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C93105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C94105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0C95105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA0105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA1105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA2105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA3105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA4105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA5105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA6105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA7105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA8105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CA9105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CAA105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CAB105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CAC105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CAD105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CAE105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0CAF105B ;FOXCONN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_102A1734 ;FSC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_103C1734 ;FSC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_15001752 ;GBM
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_03001014 ;GIGABYTE
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_32001458 ;GIGABYTE
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_E0001458 ;GIGABYTE
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_E0001940 ;GIGABYTE
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_66661458 ;GIGABYTE
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_70031631 ;GIGABYTE
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_E0091631 ;GIGABYTE
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2A01103C ;HPD
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2A0B103C ;HP
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_802F1043 ;HPD
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_300E103C ;HP_Q
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2A20103C ;HP_CPC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_2A16103C ;HP
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3189109F ;HP
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00061170 ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00071170 ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00081170 ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_000A1170 ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_000B1170 ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_083C0E11 ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_500417FF ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_500517FF ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_500617FF ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_FF101179 ;Inventec
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_16681636 ;JEAN
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10EC16F3 ;Jetway
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_810016F3 ;Jetway
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3800191B ;JMP Systems
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_000315FE ;Kinpo
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00021854 ;LGE
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_215314A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_215414A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_215714A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_215814A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_215914A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_216314A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_216514A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_216614A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_216814A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_217214A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_218914A4 ;LITEON
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_000D0E11 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_000E0E11 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_001F0E11 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_100B13BD ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101413BD ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101613BD ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101C13BD ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10551734 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10791734 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00951071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01471071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01651071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01711071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10951071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_11471071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_11711071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01241071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_67841071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_68161071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_70201071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_70251071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_71701071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_72331071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_77221071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80111071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80501071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80511071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80521071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80601071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_81701071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_81751071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A3201071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A7601071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_C0021631 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_C0031631 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_C0051631 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA001071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA011071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA021071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA031071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA041071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA051071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA061071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA071071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA081071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_DA091071 ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_F6F113BD ;Mitac
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_200017FF ;MSI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00101462 ;MSI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00311462 ;MS-1003
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01011462 ;MS-1010
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01211462 ;MS-1012
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01311462 ;MS-1013
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02011462 ;MS-1020
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_02911462 ;MS-1029
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01611462 ;MS-1016
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_368C1462 ;MS-6368
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_378C1462 ;MS-6378
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_382C1462 ;MS-6382
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_390C1462 ;MS-6390
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_399C1462 ;MS-6399
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_505C1462 ;MS-6505
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_507C1462 ;MS-6507
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_513C1462 ;MS-6513
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_526C1462 ;MS-6526
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_532C1462 ;MS-6532
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_535C1462 ;MS-6535
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_536C1462 ;MS-6536
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_537C1462 ;MS-6537
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_524C1462 ;MS-6524
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_533C1462 ;MS-6533
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_552C1462 ;MS-6552
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_557C1462 ;MS-6557
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_558C1462 ;MS-6558
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_567C1462 ;MS-6567
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_568C1462 ;MS-6568
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_572C1462 ;MS-6572
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_573C1462 ;MS-6573
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_575C1462 ;MS-6575E
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_577C1462 ;MS-6577
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_579C1462 ;MS-6579
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_590C1462 ;MS-6590
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_701C1462 ;MS-6701
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_706C1462 ;MS-6706
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_707C1462 ;MS-6707
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_710C1462 ;MS-6710
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_714C1462 ;MS-6714
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_732C1462 ;MS-6732
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_733C1462 ;MS-6733
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_771C1462 ;MS-6771
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_788C1462 ;MS-6788
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_003C1462 ;MS-7003
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_006C1462 ;MS-7006
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_031C1462 ;MS-7031
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_033C1462 ;MS-7033
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_036C1462 ;MS-7036
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_037C1462 ;MS-7037
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_038C1462 ;MS-7038
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_057C1462 ;MS-7057
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_058C1462 ;MS-7058
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_82971033 ;MS-7069
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_072C1462 ;MS-7072
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_088C1462 ;MS-7088
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_067C1462 ;MSI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_082C1462 ;MSI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_097C1462 ;MSI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_120C1462 ;MSI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_816A1033 ;NEC(Arima)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_81931033 ;NEC(Arima)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_81C91033 ;NEC(Arima)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_81E71033 ;NEC(Arima)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_82031033 ;NEC(Arima)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_81921033 ;NEC(Quanta)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_82491033 ;NEC(Quanta)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_82B61033 ;NEC(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_824A1033 ;NEC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_826E1033 ;NEC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_82701033 ;NEC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_827A1033 ;NEC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_82A61033 ;NEC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_82AE1033 ;NEC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_82C61033 ;NEC
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_833810F7 ;Panasonic
%RTL8139Panasonic.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_834310F7 ;Panasonic
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0027103C ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3080103C ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3082103C ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3084103C ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_308F103C ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_006A0E11 ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_006A103C ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0089110A ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_01001265 ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_058917FF ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_058A17FF ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_058B17FF ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0705152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0707152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0720152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0724152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0726152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0728152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0729152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0730152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0731152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0734152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101810BD ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101910BD ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7701152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_8901152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_9904152D ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_FF311179 ;Quanta
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_76193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_561A3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_56193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_53193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_4D193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_4D1E3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_4D1A3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_4D1B3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_4D1D3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_4D1F3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_4D213411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_52193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_521F3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_4D263411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_521B3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_521C3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_521D3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_52203411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_52213411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_52223411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_52243411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_53193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_69193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_6A193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_6A1B3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_6A1D3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_6A1C3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_6E1A3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_6E193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_6D193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_6B193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_75193411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_630E3411 ;QDI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_315C109F ;Semitron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7142109F ;Semitron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_7148109F ;Semitron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3184109F ;Semitron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_102613BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_102913BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_102B13BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_103313BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_103713BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_103913BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_103A13BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_103B13BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_103E13BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_104213BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_104513BD ;Sharp
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80E3104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80EA104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80EC104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_80F6104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_810F104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_8110104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_8143104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_814D104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_8158104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_8168104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_8175104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_8177104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_8194104D ;SONY
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A40210FD ;SOYO
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A40510FD ;SOYO
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A40710FD ;SOYO
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A70310FD ;SOYO
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A70610FD ;SOYO
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_B30210FD ;SOYO
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_B30310FD ;SOYO
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_B70310FD ;SOYO
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_18656245 ;Surwin
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_838315D5 ;TATUNG
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_31528452 ;Topstar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_31538452 ;Topstar
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_31548452 ;Topstar
%RTL8139.DeviceDesc% = RTL8139_TOSx.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00011179 ;Toshiba
%RTL8139.DeviceDesc% = RTL8139_TOSx.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00021179 ;Toshiba
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3186109F ;Trigem
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3187109F ;Trigem
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_714A109F ;Trigem
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_5004148C ;TUL
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101D13BD ;Twinhead
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_1C0413BD ;Twinhead
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_300214FF ;Twinhead
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_300114FF ;Twinhead
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_020514FF ;Twinhead
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_020B14FF ;Twinhead
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_020B103C ;Twinhead
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_209710F1 ;Tyan
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_97001584 ;Uniwill
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_C0011631 ;Uniwill
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_103113BD ;USI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_0B7C17AA ;Vector
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0011106 ;VIA
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_A0021106 ;VIA
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_C0011106 ;VIA
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00191025 ;Wistron(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_001A1025 ;Wistron(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00211025 ;Wistron(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_002B1025 ;Wistron(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00361025 ;Wistron(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_003A1025 ;Wistron(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_003C1025 ;Wistron(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_003D1025 ;Wistron(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_005A1025 ;Wistron(Compal)
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00181025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00391025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00521025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_005F1025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00791025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101B1025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_101D1025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10241025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10261025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10271025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_10291025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_102B1025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_102C1025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_102D1025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_105317C0 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_3081103C ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_89251025 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_81391054 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_70051631 ;Wistron
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60251668 ;MC100RPMI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60291668 ;MC100RMmI
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60481668 ;MP100R
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60611668 ;MC400TR
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60631668 ;MC400VR
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60781668 ;PE100R
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_60801668 ;PE100R-2
%RTL8139.DeviceDesc% = RTL8139x.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_000118D8 ;
;IDs for CPFE
%RTL8139P.DeviceDesc% = RTL8139Px.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00560E11&REV_20 ;Arima
%RTL8139P.DeviceDesc% = RTL8139Px.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_00B00E11&REV_20 ;Arima
%RTL8139P.DeviceDesc% = RTL8139Px.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_08600E11&REV_20 ;Compal

;;****************************************************************************
;; Windows 98/ME
;;****************************************************************************
[rtl8139.ndi]
DriverVer       = 12/02/2004,620
AddReg          = rtl8139.id.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
CopyFiles       = Rtlnic.CopyFiles9x

[rtl8139P.ndi]
DriverVer       = 12/02/2004,620
AddReg          = rtl8139.id.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
CopyFiles       = Rtlnic.CopyFiles9x

[rtl8169.ndi]
DriverVer       = 12/02/2004,620
AddReg          = rtl8169.id.reg, RTLnic.all.reg, RTL8169.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

[RTL8139_TOS.ndi]
DriverVer       = 12/02/2004,620
AddReg          = rtl8139.id.reg, RTLnic.all.reg, RTL8139TOS.common.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;; Windows 2000
;;****************************************************************************
[RTL8139.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8139P.ndi.NT]
DelReg          = CpPreParams.DelReg
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL39.common.reg, RTL39p.only.reg, RTL39p.w2k.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139P.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8169.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL8169.common.reg, RTL8169.W2K.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8169.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8139_TOS.ndi.NT]
DelReg          = PreParams.DelReg           
AddReg          = RTL8023.reg, RTLnic.all.reg, RTL8139TOS.common.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139_TOS.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[Rtlnic.CopyFiles]
Rtlnic.sys,,,2

[Rtlnic.CopyFiles9x]
Rtlnic.sys,,,2

;;****************************************************************************
;; Windows XP
;;****************************************************************************
;----------------
; RTL8139 Family
;----------------
[RTL8139x.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL39.common.reg, RTL39.only.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8139x.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

[RTL8139_TOSx.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL8139TOS.common.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8139_TOSx.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

;-----------
; RTL8139c+
;-----------
[RTL8139Px.ndi.NT]
DelReg          = CpPreParams.DelReg
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL39.common.reg, RTL39p.only.reg, RTL39p.w2k.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8139Px.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

;---------
; RTL8169
;---------
[RTL8169x.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8023xp.reg, RTLnic.all.reg, RTL8169.common.reg, RTL8169.W2K.reg
CopyFiles       = Rtlnic.CopyFilesXP

[RTL8169x.ndi.NT.Services]
AddService = RTL8023xp, 2, rtsntxp.Service, common.EventLog

[Rtlnic.CopyFilesXP]
Rtlnicxp.sys,,,2

;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8139.id.reg]
HKR,,                 MediaType,          0,    1
HKR,,                 AdapterType,        0,    5
HKR,,                 BusType,            0,    5
HKR,,                 DevLoader,          0,    "*ndis"
HKR,,                 DeviceVxDs,         0,    "Rtlnic.sys"
HKR,,                 EnumPropPages,      0,    "netdi.dll,EnumPropPages"
HKR,NDIS,             MajorNdisVersion,   1,    03
HKR,NDIS,             MinorNdisVersion,   1,    0A
HKR,NDIS,             LogDriverName,      0,    "RTL8023"
HKR,Ndi,              DeviceID,           0,    "PCI\VEN_10EC&DEV_8139"
HKR,Ndi\Install,      ndis3,              0,    "rtl139.ndis5"
HKR,Ndi\Interfaces,   DefLower,            ,    "ethernet"
HKR,Ndi\Interfaces,   LowerRange,          ,    "ethernet"
HKR,Ndi\Interfaces,   DefUpper,            ,    "ndis3"
HKR,Ndi\Interfaces,   UpperRange,          ,    "ndis3"

[rtl8169.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtlnic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTL8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8169"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

;;****************************************************************************
;; common parameters
;;****************************************************************************
[RTLnic.all.reg]
HKR,Ndi\params\NetworkAddress,  ParamDesc,      0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,  type,           0, "edit"
HKR,Ndi\params\NetworkAddress,  default,        0, "000000000000"
HKR,Ndi\params\NetworkAddress,  LimitText,      0, "12"
HKR,Ndi\params\NetworkAddress,  UpperCase,      0, "1"
HKR,Ndi\params\NetworkAddress,  Optional,       0, "1"

[RTL39.common.reg]
HKR,Ndi\params\DuplexMode,        ParamDesc,   0, %SpeedDuplexMode%
HKR,Ndi\params\DuplexMode,        type,        0, "enum"
HKR,Ndi\params\DuplexMode,        default,     0, "1"
HKR,Ndi\params\DuplexMode\enum,   1,           0, %auto_nego%
HKR,Ndi\params\DuplexMode\enum,   2,           0, %sd10half%
HKR,Ndi\params\DuplexMode\enum,   3,           0, %sd10full%
HKR,Ndi\params\DuplexMode\enum,   4,           0, %sd100half%
HKR,Ndi\params\DuplexMode\enum,   5,           0, %sd100full%

HKR,Ndi\params\OptimalPerf,      ParamDesc,  0, %OptimalPerf%
HKR,Ndi\params\OptimalPerf,      default,    0, "0"
HKR,Ndi\params\OptimalPerf,      type,       0, "enum"
HKR,Ndi\params\OptimalPerf\enum, "1",        0, "Enable"
HKR,Ndi\params\OptimalPerf\enum, "0",        0, "Disable"

HKR,Ndi\params\WakeUpFrame,     ParamDesc,      0, %WOLCapability%
HKR,Ndi\params\WakeUpFrame,     default,        0, "1"
HKR,Ndi\params\WakeUpFrame,     type,           0, "enum"
HKR,Ndi\params\WakeUpFrame\enum,"0",            0, "Disable"
HKR,Ndi\params\WakeUpFrame\enum,"1",            0, "Enable"
HKR,,WakeUpFrame, 0, "1"

HKR,Ndi\params\LinkUp,           ParamDesc, 0, "WakeUp on Link Change"
HKR,Ndi\params\LinkUp,           default,   0, "0"
HKR,Ndi\params\LinkUp,           type,      0, "enum"
HKR,Ndi\params\LinkUp\enum,      "1",       0, "Enable"
HKR,Ndi\params\LinkUp\enum,      "0",       0, "Disable"

HKR,Ndi\params\EnableLDPS,       ParamDesc, 0, "Link Down Power Saving"
HKR,Ndi\params\EnableLDPS,       default,   0, "0"
HKR,Ndi\params\EnableLDPS,       type,      0, "enum"
HKR,Ndi\params\EnableLDPS\enum,  "1",       0, "Enable"
HKR,Ndi\params\EnableLDPS\enum,  "0",       0, "Disable"

[RTL39.only.reg]
HKR,Ndi\params\RxBufLen,         ParamDesc, 0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,         type,      0, "enum"
HKR,Ndi\params\RxBufLen,         default,   0, "3"
HKR,Ndi\params\RxBufLen\enum,    "0",       0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,    "1",       0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,    "2",       0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,    "3",       0, "64K bytes"

HKR,Ndi\params\RTPME,            ParamDesc, 0, "WakeUp using APM Mode"
HKR,Ndi\params\RTPME,            default,   0, "0"
HKR,Ndi\params\RTPME,            type,      0, "enum"
HKR,Ndi\params\RTPME\enum,       "1",       0, "Enable"
HKR,Ndi\params\RTPME\enum,       "0",       0, "Disable"

[RTL39p.only.reg]
HKR,Ndi\Params\NumCoalesce,       ParamDesc,  0, "Number of Tx Coalesce Buffer"
HKR,Ndi\Params\NumCoalesce,       Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,       Default,    0, "16"
HKR,Ndi\Params\NumCoalesce,       Min,        0, "0"
HKR,Ndi\Params\NumCoalesce,       Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,       Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,       Base,       0, "10"

[PreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[CpPreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\RTPME
HKR,,RTPME
HKR,Ndi\Params\RxBufLen
HKR,,RxBufLen
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[GigPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid

[RTL39p.w2k.reg]
HKR,Ndi\params\Offload,           ParamDesc,  0, "Task Offload"
HKR,Ndi\params\Offload,           default,    0, "1"
HKR,Ndi\params\Offload,           type,       0, "enum"
HKR,Ndi\params\Offload\enum,      "0",        0, "All Disable"
HKR,Ndi\params\Offload\enum,      "1",        0, "Checksum"
HKR,Ndi\params\Offload\enum,      "2",        0, "Chksum & TCP_Segment"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

[RTL8139TOS.common.reg]
HKR,Ndi\params\RxBufLen,          ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,          type,       0, "enum"
HKR,Ndi\params\RxBufLen,          default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,     "0",        0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,     "1",        0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,     "2",        0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,     "3",        0, "64K bytes"

HKR,Ndi\params\LinkUp,            ParamDesc,  0, "WakeUp on Link Change"
HKR,Ndi\params\LinkUp,            default,    0, "0"
HKR,Ndi\params\LinkUp,            type,       0, "enum"
HKR,Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR,Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR,Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp on ARP/PING"         
HKR,Ndi\params\WakeUpFrame,       default,    0, "1"                          
HKR,Ndi\params\WakeUpFrame,       type,       0, "enum"                       
HKR,Ndi\params\WakeUpFrame\enum,  "1",        0, "Enable"                     
HKR,Ndi\params\WakeUpFrame\enum,  "0",        0, "Disable"                    

HKR,Ndi\params\RTPME,             ParamDesc,  0, "WakeUp using APM Mode"      
HKR,Ndi\params\RTPME,             default,    0, "0"                          
HKR,Ndi\params\RTPME,             type,       0, "enum"                      
HKR,Ndi\params\RTPME\enum,        "1",        0, "Enable"                     
HKR,Ndi\params\RTPME\enum,        "0",        0, "Disable"                   

HKR,Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR,Ndi\params\EnableLDPS,        default,    0, "1"
HKR,Ndi\params\EnableLDPS,        type,       0, "enum"
HKR,Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"
HKR,Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"

HKR,Ndi\params\TxMaxDMABurst,     ParamDesc,  0, "Transmit DMA burst size"  
HKR,Ndi\params\TxMaxDMABurst,     type,       0, "enum"                           
HKR,Ndi\params\TxMaxDMABurst,     default,    0, "6"                           
HKR,Ndi\params\TxMaxDMABurst\enum,0,          0, "16 bytes"                  
HKR,Ndi\params\TxMaxDMABurst\enum,1,          0, "32 bytes"        
HKR,Ndi\params\TxMaxDMABurst\enum,2,          0, "64 bytes"         
HKR,Ndi\params\TxMaxDMABurst\enum,3,          0, "128 bytes"         
HKR,Ndi\params\TxMaxDMABurst\enum,4,          0, "256 bytes"        
HKR,Ndi\params\TxMaxDMABurst\enum,5,          0, "512 bytes"            
HKR,Ndi\params\TxMaxDMABurst\enum,6,          0, "1024 bytes"             
HKR,Ndi\params\TxMaxDMABurst\enum,7,          0, "2048 bytes"             

HKR,Ndi\params\RxMaxDMABurst,     ParamDesc,  0, "Receive DMA burst size"  
HKR,Ndi\params\RxMaxDMABurst,     type,       0, "enum"
HKR,Ndi\params\RxMaxDMABurst,     default,    0, "6"                      
HKR,Ndi\params\RxMaxDMABurst\enum,0,          0, "16 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,1,          0, "32 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum,2,          0, "64 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum,3,          0, "128 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,4,          0, "256 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,5,          0, "512 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,6,          0, "1024 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum,7,          0, "unlimitted"               

HKR,Ndi\params\EarlyRxThreshold,  ParamDesc,  0, "Receive FIFO threshold"   
HKR,Ndi\params\EarlyRxThreshold,  type,       0, "enum"
HKR,Ndi\params\EarlyRxThreshold,  default,    0, "2"
HKR,Ndi\params\EarlyRxThreshold\enum,0,       0, "16 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,1,       0, "32 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,2,       0, "64 bytes"
HKR,Ndi\params\EarlyRxThreshold\enum,3,       0, "128 bytes"
HKR,Ndi\params\EarlyRxThreshold\enum,4,       0, "256 bytes"
HKR,Ndi\params\EarlyRxThreshold\enum,5,       0, "512 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,6,       0, "1024 bytes" 
HKR,Ndi\params\EarlyRxThreshold\enum,7,       0, "No threshold"

HKR,,EnableLDPS,        0,   "1"
HKR,,WakeUpFrame,       0,   "1"          
HKR,,RTPME,             0,   "0"         
HKR,,LinkUp,            0,   "0"
HKR,,RxBufLen,          0,   "3"
HKR,,EarlyRxThreshold,  0,   "2"
HKR,,RxMaxDMABurst,     0,   "6"
HKR,,TxMaxDMABurst,     0,   "6" 

[RTL8169.common.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%

;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"

;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"

HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, "Disable"
HKR,Ndi\params\Jumboframe\enum,   "1",        0, "2KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "2",        0, "3KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "3",        0, "4KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "4",        0, "5KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "5",        0, "6KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "6",        0, "7KB MTU"

HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, "Disable"
HKR,Ndi\params\FlowControl\enum, "1",        0, "Enable"
HKR,,FlowControl,0,"1" 

[RTL8169.W2K.reg]
HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, "Disable"
HKR,Ndi\params\CksOffload\enum,   "1",        0, "Tx/Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "3",        0, "Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "4",        0, "Tx Checksum"

HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "1"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "1",        0, "Enable"
HKR,Ndi\params\Largesend\enum,    "0",        0, "Disable"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

;HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
;HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
;HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
;HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
;HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
;HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
;HKR,Ndi\Params\RegVlanid,   Base,       0, "10"

;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"

HKR,,CksOffload,0,"1" 
HKR,,Largesend,0,"1" 

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8023.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8023"

[rtsnt.Service]
DisplayName     = %Rtlnic.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtlnic.sys
LoadOrderGroup  = NDIS

[RTL8023xp.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8023xp"

[rtsntxp.Service]
DisplayName     = %Rtlnicxp.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtlnicxp.sys
LoadOrderGroup  = NDIS

[common.EventLog]
Addreg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
Rtlnic.CopyFiles           = 12
Rtlnic.CopyFilesXP         = 12
Rtlnic.CopyFiles9x         = 11
DefaultDestDir             = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
Rtlnic.sys   = 1
Rtlnicxp.sys  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek                 = "Realtek Semiconductor Corp."
VLanTagging             = "802.1Q/1p VLAN Tagging"
;VLanID                 = "802.1Q VLAN ID"
ChecksumOffload         = "Offload Checksum"
LargesendOffload        = "Offload TCP_LargeSend"
SpeedDuplexMode         = "Link Speed/Duplex Mode"
auto_nego               = "Auto Negotiation"
sd10half                = "10Mbps/Half Duplex"
sd10full                = "10Mbps/Full Duplex"
sd100half               = "100Mbps/Half Duplex"
sd100full               = "100Mbps/Full Duplex"
sd1000full              = "1000Mbps/Full Duplex"
NetworkAddress          = "Network Address"
JumboFrame              = "Jumbo Frame"
;TxDescNumber           = "Number of Tx Descriptor"
;RxDescNumber           = "Number of Rx Descriptor"
;TxHPQDescNumber        = "Number of High Priority Tx Descriptor"
WOLCapability           = "WakeUp on ARP/PING"
WOLLinkChange           = "WakeUp on Link Change"
LDPSCapability          = "Link Down Power Saving"
OptimalPerf             = "Optimal Performance"
FlowControl             = "Flow Control"

;;Source disk name
DISKNAME = "Realtek RTL8139/810x/8169/8110 all in one NDIS Driver"

;RTL8168.DeviceDesc        = "Realtek RTL8168 PCI-E Gigabit Ethernet NIC"
RTL8169.DeviceDesc        = "Realtek RTL8169/8110 Family Gigabit Ethernet NIC"
RTL8139.DeviceDesc        = "Realtek RTL8139/810x Family Fast Ethernet NIC"
RTL8139P.DeviceDesc       = "Realtek RTL8139C+ Fast Ethernet NIC"
RTL8139Panasonic.DeviceDesc = "(MOBILE ASSIST)Realtek RTL8139/810x Family Fast Ethernet NIC"

;;NT service name
Rtlnic.Service.DispName    = "Realtek RTL8139/810x/8169/8110 all in one NDIS NT Driver"
Rtlnicxp.Service.DispName    = "Realtek RTL8139/810x/8169/8110 all in one NDIS XP Driver"
