;*****************************************
; NETw4v32.INF
;
; Intel Wireless WiFi Link Adapters
; Installation Script for Windows Vista 32 bit
;
; Copyright (c) 2007 Intel, Inc. All Rights Reserved
;
;------------------------------------------------------------------------------

;******************************************************************************
; Version Section
;------------------------------------------------------------------------------
[version]
Signature   = "$Windows NT$"
Compatible  = 1
Class       = net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %PROVIDER_NAME%
DriverVer   = 06/20/2007,11.1.1.16 ;DATE HAS TO BE IN FOLLOWING FORMAT MM/DD/YYYY



CatalogFile = NETw4v32.cat


;*****************************************
; Manufacturer
;-----------------------------------------

[Manufacturer]
%COMPANY_NAME% = Device, NTx86.6.0

;[ControlFlags]
;ExcludeFromSelect = \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11008086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11018086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11028086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11038086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11048086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11058086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11068086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11078086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11008086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11018086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11028086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11038086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11048086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11058086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11068086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11078086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10008086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10018086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10028086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10038086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10048086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10058086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10068086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10078086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10008086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10018086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10028086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10038086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10048086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10008086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10018086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10028086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10038086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10048086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10308086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10318086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10328086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10338086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10058086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10348086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11108086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11118086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11128086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11138086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11148086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11158086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11168086 , \ 
;        PCI\VEN_8086&DEV_4233&SUBSYS_11178086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11108086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11118086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11128086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11138086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11148086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11158086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11168086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_11178086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10108086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10118086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10128086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10138086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10148086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10158086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10168086 , \ 
;        PCI\VEN_8086&DEV_4230&SUBSYS_10178086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10108086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10118086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10128086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10138086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10148086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11208086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11218086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11228086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11238086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11248086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11258086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11268086 , \ 
;        PCI\VEN_8086&DEV_422D&SUBSYS_11278086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11208086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11218086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11228086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11238086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11248086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11258086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11268086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_11278086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10208086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10218086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10228086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10238086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10248086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10258086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10268086 , \ 
;        PCI\VEN_8086&DEV_4229&SUBSYS_10278086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10208086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10218086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10228086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10238086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10248086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10208086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10218086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10228086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10238086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10248086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10408086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10418086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10428086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10438086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10448086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10408086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10418086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10428086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10438086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10448086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10508086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10518086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10528086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10538086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_10548086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10508086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10518086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10528086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10538086 , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_10548086 , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135B103C , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135C103C , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135D103C , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135E103C , \ 
;        PCI\VEN_8086&DEV_4228&SUBSYS_135F103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135B103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135C103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135D103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135E103C , \ 
;        PCI\VEN_8086&DEV_4222&SUBSYS_135F103C , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10108086 , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10118086 , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10128086 , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10138086 , \ 
;        PCI\VEN_8086&DEV_4227&SUBSYS_10148086 , \ 

;*****************************************
;Device
;-----------------------------------------

;*****************************************
;Device VISTA
;-----------------------------------------
[Device.NTx86.6.0]

; GEN_4965_AGN_C
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW1    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11008086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW2    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11018086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_RoW    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11028086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_JPN    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11038086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_KRA    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11048086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP1    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11058086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP2    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11068086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP3    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11078086 ; SP3

; GEN_4965_AGN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11008086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11018086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_RoW    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11028086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_JPN    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11038086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_KRA    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11048086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_SP1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11058086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_SP2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11068086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_GEN_4965_AGN_VISTA_SP3    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11078086 ; SP3

; GEN_4965_AG
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10008086 ; MOW1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10018086 ; MOW2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10028086 ; RoW
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10038086 ; JPN
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10048086 ; KRA
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_SP1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10058086 ; SP1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_SP2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10068086 ; SP2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_GEN_4965_AG_VISTA_SP3    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10078086 ; SP3

; GEN_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10008086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10018086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10028086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10038086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_GEN_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10048086 ; KRA

; GEN_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10008086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10018086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10028086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10038086 ; JPN
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10048086 ; KRA

; GEN_3945_ABG_SP1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_SP1_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10308086 ;

; GEN_3945_ABG_SP2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_SP2_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10318086 ;

; GEN_3945_ABG_SP3
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_SP3_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10328086 ;

; GEN_3945_ABG_SP4
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_GEN_3945_ABG_SP4_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10338086 ;

; GEN_3945_BG
%NIC_MPCIEX_3945BG% = Install_MPCIEX_GEN_3945_BG_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10058086 ;

; GEN_3945_BGX
%NIC_MPCIEX_3945BG% = Install_MPCIEX_GEN_3945_BGX_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10348086 ;

; Lenovo_4965_AGN_C
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11108086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11118086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_RoW    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11128086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_JPN    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11138086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_KRA    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11148086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP1    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11158086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP2    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11168086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP3    ,   PCI\VEN_8086&DEV_4233&SUBSYS_11178086 ; SP3

; Lenovo_4965_AGN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11108086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11118086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_RoW    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11128086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_JPN    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11138086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_KRA    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11148086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP1    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11158086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP2    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11168086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP3    ,   PCI\VEN_8086&DEV_4230&SUBSYS_11178086 ; SP3

; Lenovo_4965_AG
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10108086 ; MOW1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10118086 ; MOW2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10128086 ; RoW
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10138086 ; JPN
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10148086 ; KRA
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_SP1    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10158086 ; SP1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_SP2    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10168086 ; SP2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Lenovo_4965_AG_VISTA_SP3    ,   PCI\VEN_8086&DEV_4230&SUBSYS_10178086 ; SP3

; Lenovo_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10108086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10118086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10128086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10138086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Lenovo_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10148086 ; KRA

; Dell_4965_AGN_C
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW1    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11208086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW2    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11218086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_RoW    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11228086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_JPN    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11238086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_KRA    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11248086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP1    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11258086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP2    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11268086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP3    ,   PCI\VEN_8086&DEV_422D&SUBSYS_11278086 ; SP3

; Dell_4965_AGN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11208086 ; MOW1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11218086 ; MOW2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_RoW    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11228086 ; RoW
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_JPN    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11238086 ; JPN
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_KRA    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11248086 ; KRA
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_SP1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11258086 ; SP1
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_SP2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11268086 ; SP2
%NIC_MPCIEX_4965AGN% = Install_MPCIEX_Dell_4965_AGN_VISTA_SP3    ,   PCI\VEN_8086&DEV_4229&SUBSYS_11278086 ; SP3

; Dell_4965_AG
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10208086 ; MOW1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10218086 ; MOW2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10228086 ; RoW
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10238086 ; JPN
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10248086 ; KRA
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_SP1    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10258086 ; SP1
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_SP2    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10268086 ; SP2
%NIC_MPCIEX_4965AG% = Install_MPCIEX_Dell_4965_AG_VISTA_SP3    ,   PCI\VEN_8086&DEV_4229&SUBSYS_10278086 ; SP3

; Dell_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10208086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10218086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10228086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10238086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Dell_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10248086 ; KRA

; Dell_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10208086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10218086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10228086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10238086 ; JPN
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Dell_3945_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10248086 ; KRA

; Toshiba_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10408086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10418086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10428086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10438086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Toshiba_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10448086 ; KRA

; Toshiba_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10408086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10418086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Toshiba_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10428086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Toshiba_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10438086 ; JPN

; Toshiba_3945_BGX
%NIC_MPCIEX_3945BG% = Install_MPCIEX_Toshiba_3945_BGX_VISTA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10448086 ;

; Sony_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10508086 ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10518086 ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10528086 ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10538086 ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_Sony_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_10548086 ; KRA

; Sony_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10508086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10518086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10528086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10538086 ; JPN
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_Sony_3945_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_10548086 ; KRA

; HP_3965_ABG
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135B103C ; MOW1
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135C103C ; MOW2
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135D103C ; RoW
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135E103C ; JPN
%NIC_MPCIEX_3965ABG% = Install_MPCIEX_HP_3965_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4228&SUBSYS_135F103C ; KRA

; HP_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135B103C ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135C103C ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135D103C ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135E103C ; JPN
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_HP_3945_ABG_VISTA_KRA    ,   PCI\VEN_8086&DEV_4222&SUBSYS_135F103C ; KRA

; IBM_3945_ABG
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_IBM_3945_ABG_VISTA_MOW1    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10108086 ; MOW1
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_IBM_3945_ABG_VISTA_MOW2    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10118086 ; MOW2
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_IBM_3945_ABG_VISTA_RoW    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10128086 ; RoW
%NIC_MPCIEX_3945ABG% = Install_MPCIEX_IBM_3945_ABG_VISTA_JPN    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10138086 ; JPN

; IBM_3945_BG
%NIC_MPCIEX_3945BG% = Install_MPCIEX_IBM_3945_BG_VISTA    ,   PCI\VEN_8086&DEV_4227&SUBSYS_10148086 ;



;*****************************************
;INSTALL VISTA
;-----------------------------------------

;-----------------------------------------
; Intel  4965AGN VISTA GEN_4965_AGN_C
;-----------------------------------------

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN_C, Reg_GEN_4965_AGN_C_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_C_VISTA_SP3.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  4965AGN VISTA GEN_4965_AGN
;-----------------------------------------

[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_SP1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_SP2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AGN, Reg_GEN_4965_AGN_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AGN_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AGN_VISTA_SP3.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  4965AG VISTA GEN_4965_AG
;-----------------------------------------

[Install_MPCIEX_GEN_4965_AG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_MOW1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_MOW2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_RoW, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_JPN, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_KRA, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_SP1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_SP1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_SP2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_SP2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_4965_AG_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_4965_AG, Reg_GEN_4965_AG_SP3, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_4965_AG_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_4965_AG_VISTA_SP3.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3965ABG VISTA GEN_3965_ABG
;-----------------------------------------

[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3965_ABG, Reg_GEN_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3965_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA GEN_3945_ABG
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_GEN_3945_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG, Reg_GEN_3945_ABG_KRA, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_GEN_3945_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA GEN_3945_ABG_SP1
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_SP1_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG_SP1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_SP1_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_ABG_SP1_VISTA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA GEN_3945_ABG_SP2
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_SP2_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG_SP2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_SP2_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_ABG_SP2_VISTA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA GEN_3945_ABG_SP3
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_SP3_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG_SP3, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_SP3_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_ABG_SP3_VISTA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA GEN_3945_ABG_SP4
;-----------------------------------------

[Install_MPCIEX_GEN_3945_ABG_SP4_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_ABG_SP4, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_ABG_SP4_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_ABG_SP4_VISTA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945BG VISTA GEN_3945_BG
;-----------------------------------------

[Install_MPCIEX_GEN_3945_BG_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_BG, Reg_MPCIEX_3945BG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_BG_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_BG_VISTA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945BG VISTA GEN_3945_BGX
;-----------------------------------------

[Install_MPCIEX_GEN_3945_BGX_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_GEN_3945_BGX, Reg_MPCIEX_3945BG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3945_BGX_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_GEN_3945_BGX_VISTA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  4965AGN VISTA Lenovo_4965_AGN_C
;-----------------------------------------

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN_C, Reg_Lenovo_4965_AGN_C_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_C_VISTA_SP3.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  4965AGN VISTA Lenovo_4965_AGN
;-----------------------------------------

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AGN, Reg_Lenovo_4965_AGN_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AGN_VISTA_SP3.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  4965AG VISTA Lenovo_4965_AG
;-----------------------------------------

[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_MOW1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_MOW2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_RoW, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_JPN, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_KRA, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_SP1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_SP2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_4965_AG, Reg_Lenovo_4965_AG_SP3, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Lenovo_4965_AG_VISTA_SP3.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3965ABG VISTA Lenovo_3965_ABG
;-----------------------------------------

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Lenovo_3965_ABG, Reg_Lenovo_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Lenovo_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Lenovo_3965_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  4965AGN VISTA Dell_4965_AGN_C
;-----------------------------------------

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN_C, Reg_Dell_4965_AGN_C_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_C_VISTA_SP3.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  4965AGN VISTA Dell_4965_AGN
;-----------------------------------------

[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_MOW1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_MOW2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_RoW, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_JPN, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_KRA, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_SP1, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_SP1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_SP2, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_SP2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AGN, Reg_Dell_4965_AGN_SP3, Reg_MPCIEX_4965AGN, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AGN_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AGN_VISTA_SP3.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  4965AG VISTA Dell_4965_AG
;-----------------------------------------

[Install_MPCIEX_Dell_4965_AG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_MOW1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_MOW2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_RoW, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_JPN, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_KRA, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_SP1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_SP1, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_SP1.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_SP1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_SP2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_SP2, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_SP2.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_SP2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_4965_AG_VISTA_SP3]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_4965_AG, Reg_Dell_4965_AG_SP3, Reg_MPCIEX_4965AG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_KDR, Reg_NDI, Reg_NDI_KDR
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_4965_AG_VISTA_SP3.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Dell_4965_AG_VISTA_SP3.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3965ABG VISTA Dell_3965_ABG
;-----------------------------------------

[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3965_ABG, Reg_Dell_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3965_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA Dell_3945_ABG
;-----------------------------------------

[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Dell_3945_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Dell_3945_ABG, Reg_Dell_3945_ABG_KRA, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Dell_3945_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Dell_3945_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3965ABG VISTA Toshiba_3965_ABG
;-----------------------------------------

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3965_ABG, Reg_Toshiba_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3965_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA Toshiba_3945_ABG
;-----------------------------------------

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_ABG, Reg_Toshiba_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_ABG, Reg_Toshiba_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3945_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_ABG, Reg_Toshiba_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3945_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_ABG, Reg_Toshiba_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Toshiba_3945_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945BG VISTA Toshiba_3945_BGX
;-----------------------------------------

[Install_MPCIEX_Toshiba_3945_BGX_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Toshiba_3945_BGX, Reg_MPCIEX_3945BG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Toshiba_3945_BGX_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_Toshiba_3945_BGX_VISTA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3965ABG VISTA Sony_3965_ABG
;-----------------------------------------

[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3965_ABG, Reg_Sony_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3965_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA Sony_3945_ABG
;-----------------------------------------

[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_Sony_3945_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_Sony_3945_ABG, Reg_Sony_3945_ABG_KRA, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_Sony_3945_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_Sony_3945_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3965ABG VISTA HP_3965_ABG
;-----------------------------------------

[Install_MPCIEX_HP_3965_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_MOW1, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3965_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_MOW2, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3965_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_RoW, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3965_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_JPN, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3965_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3965_ABG, Reg_HP_3965_ABG_KRA, Reg_MPCIEX_3965ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3965_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3965_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA HP_3945_ABG
;-----------------------------------------

[Install_MPCIEX_HP_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_HP_3945_ABG_VISTA_KRA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_HP_3945_ABG, Reg_HP_3945_ABG_KRA, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_HP_3945_ABG_VISTA_KRA.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_HP_3945_ABG_VISTA_KRA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945ABG VISTA IBM_3945_ABG
;-----------------------------------------

[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW1]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_ABG, Reg_IBM_3945_ABG_MOW1, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW1.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW1.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW2]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_ABG, Reg_IBM_3945_ABG_MOW2, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW2.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_IBM_3945_ABG_VISTA_MOW2.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_IBM_3945_ABG_VISTA_RoW]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_ABG, Reg_IBM_3945_ABG_RoW, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_ABG_VISTA_RoW.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_IBM_3945_ABG_VISTA_RoW.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Install_MPCIEX_IBM_3945_ABG_VISTA_JPN]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_ABG, Reg_IBM_3945_ABG_JPN, Reg_MPCIEX_3945ABG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_ABG_VISTA_JPN.HW]
AddReg      = MSI_NDIS.reg
Include     = machine.inf
Needs       = PciASPMOptIn


[Install_MPCIEX_IBM_3945_ABG_VISTA_JPN.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

;-----------------------------------------
; Intel  3945BG VISTA IBM_3945_BG
;-----------------------------------------

[Install_MPCIEX_IBM_3945_BG_VISTA]
AddReg         = Reg_Common, Reg_Common_VISTA, Reg_IBM_3945_BG, Reg_MPCIEX_3945BG, Reg_NDIS_VISTA, Reg_CoInstaller32, Reg_ALM, Reg_NDI, Reg_NDI_ALM
DelReg         = Reg_Loudon_Obsolete
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_VISTA, CopyFiles_NCPA32
*IfType = 71             ; IF_TYPE_IEEE80211
*MediaType = 16          ; NdisMediumNative802_11
*PhysicalMediaType = 9   ; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IBM_3945_BG_VISTA.HW]
AddReg      = MSI_NDIS.reg


[Install_MPCIEX_IBM_3945_BG_VISTA.Services]
AddService      = NETw4v32, 2, NIC_Service_VISTA, Common_EventLog_VISTA

[Reg_Loudon_Obsolete]
HKR,,RfKillSKU
HKR,,FixedSupportedRates
HKR,,PowerIndex
HKR,,PnPCapabilities

[Reg_Common]
HKR,,ModulationType,2,"2"
HKR,,RecommendedBeaconInterval,0x10001,0x64
HKR,,CardType,0x00010001,2
HKR,,ConnectionPriority,0,"2"
HKR,,DesiredPortType,0x10003,0x1
HKR,,ExternalImage,0x10001,0x0
HKR,,NdisEnvironment,0x10001,0
HKR,,NetType,0,"WLAN"
HKR,,Provider,0,%PROVIDER_NAME%
HKR,,PibssShortSlot,0x10001,0x1
HKR,,ConfigurationName,0,"PR0W1RELE55"
HKR,,DesiredAuthenticationMode,0x10003,0x0
HKR,,DesiredCipher,0x10003,0x1
HKR,,FixedLongPreamble,0x10001,0x0
HKR,,DesiredPSKey1,0x2,""
HKR,,DesiredPSKey2,0x2,""
HKR,,DesiredPSKey3,0x2,""
HKR,,DesiredPSKey4,0x2,""
HKR,,DesiredDefaultKeyId,0x10003,0x1
HKR,,RadioEnable,0x10003,0x1
HKR,,CCXv4FeatureSet,0x10003,0xFFFFFFFF
HKR,,WoWLanEnable,0x10001,0x1
HKR,,ApsdTriggerQueues,0x10001,0x0
HKR,,BcsSupport,0x10003,0x0
HKR,,DlsEnabled,0x10003,0x0
HKR,,DlsResponseTimeout,0x10003,0x0
HKR,,DlsTimeoutCounter,0x10003,0x0
HKR,,SlsEnabled,0x10003,0x0
HKR,,SlsEnabledOnRecipient,0x10003,0x0
HKR,,SlsForcedToDirect,0x10003,0x0
HKR,,SlsDecisionPeriod,0x10003,0x0

; following registry keys define the Advanced Property Page (NDI) values. they are common, and the defult values vary between the different reg sections.
[Reg_NDI]
HKR, Ndi\params\RecommendedChannel24,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL24_STR%
HKR, Ndi\params\RecommendedChannel24,      	Type,       0x00000002, "int"
HKR, Ndi\params\RecommendedChannel24,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel24,      	Min,	    0x00000002, "1"
HKR, Ndi\params\RecommendedChannel24,      	Step,	   	0x00000002, "1"

HKR, Ndi\Params\WirelessMode,               ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,               Type,       0, "enum",
HKR, Ndi\params\WirelessMode,      			    Default,   	0, "34" ;abg
HKR, Ndi\Params\WirelessMode,               Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 			    "17",       0, "1. 802.11a"
HKR, Ndi\params\WirelessMode\enum, 			    "0",        0, "2. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 			    "16",       0, "3. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 			    "32",       0, "4. 802.11b/g"
HKR, Ndi\params\WirelessMode\enum, 			    "18",       0, "5. 802.11a/g"
HKR, Ndi\params\WirelessMode\enum, 			    "34",       0, "6. 802.11a/b/g"

HKR, Ndi\params\IbssTxPower,      			    ParamDesc, 	0x00000000, %IBSS_TX_POWER_STR%
HKR, Ndi\params\IbssTxPower,      			    Type,      	0x00000002, "enum"
HKR, Ndi\params\IbssTxPower,      			    Default,   	0x00000002, "100"
HKR, Ndi\params\IbssTxPower,      			    Optional,  	0x00000002, "0"
HKR, Ndi\params\IbssTxPower\enum, 			    "0",       	0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "25",       0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "50",       0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "75",       0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\IbssTxPower\enum, 			    "100",      0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\RoamAggressiveness,     	  ParamDesc, 	0x00000000, %ROAMING_AGGRESSIVENESS_STR%
HKR, Ndi\params\RoamAggressiveness,     	  Type,      	0x00000002, "enum"
HKR, Ndi\params\RoamAggressiveness,     	  Default,   	0x00000002, "2"
HKR, Ndi\params\RoamAggressiveness,     	  Optional,  	0x00000002, "0"
HKR, Ndi\params\RoamAggressiveness\enum,	  "0",       	0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	  "1",       	0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	  "2",     	0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	  "3", 	    	0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\RoamAggressiveness\enum,    	  "4",          0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\RecommendedAtimWindow, 				ParamDesc, 	0x00000000, %ADHOC_POWER_MANAGEMENT_STR%
HKR, Ndi\params\RecommendedAtimWindow, 				Type,  			0x00000002, "enum"
HKR, Ndi\params\RecommendedAtimWindow, 				Default, 		0x00000002, "0"
HKR, Ndi\params\RecommendedAtimWindow, 				Optional,  	0x00000002, "0"
HKR, Ndi\params\RecommendedAtimWindow\enum,  	"0", 				0x00000000, %DISABLED_STR%
HKR, Ndi\params\RecommendedAtimWindow\enum,  	"3", 				0x00000000, %MAXIMUM_POWER_SAVING_STR%
HKR, Ndi\params\RecommendedAtimWindow\enum,  	"10", 			0x00000000, %NOISY_ENVIRONMENT_STR%

HKR, Ndi\params\IbssQosEnabled,			  ParamDesc, 	0x00000000, %ADHOC_QOS_MODE_STR%
HKR, Ndi\params\IbssQosEnabled,			  Type,  			0x00000002, "enum"
HKR, Ndi\params\IbssQosEnabled,			  Default, 		0x00000002, "0"
HKR, Ndi\params\IbssQosEnabled,			  Optional,  	0x00000002, "0"
HKR, Ndi\params\IbssQosEnabled\enum,  "0",  			0x00000000, %WMM_DISABLED_STR%
HKR, Ndi\params\IbssQosEnabled\enum,  "1",  			0x00000000, %WMM_ENABLED_STR%

HKR, Ndi\params\CtsToItself,		  ParamDesc, 			0x00000000, %MIXED_MODE_PROTECTION_STR%
HKR, Ndi\params\CtsToItself,		  Type,  					0x00000002, "enum"
HKR, Ndi\params\CtsToItself,		  Default, 				0x00000002, "1"
HKR, Ndi\params\CtsToItself,		  Optional,  			0x00000002, "0"
HKR, Ndi\params\CtsToItself\enum, "0",  					0x00000000, %RTS_CTS_ENABLED_STR%
HKR, Ndi\params\CtsToItself\enum, "1",  					0x00000000, %CTS_TO_SELF_ENABLED_STR%

HKR, Ndi\params\PropPacketBurstEnabled,		ParamDesc, 	0x00000000, %THROUGHPUT_ENHANCEMENT_STR%
HKR, Ndi\params\PropPacketBurstEnabled,		Type,  			0x00000002, "enum"
HKR, Ndi\params\PropPacketBurstEnabled,		Default, 		0x00000002, "0"
HKR, Ndi\params\PropPacketBurstEnabled,		Optional,  	0x00000002, "0"
HKR, Ndi\params\PropPacketBurstEnabled\enum, "0", 		0x00000000, %DISABLED_STR%
HKR, Ndi\params\PropPacketBurstEnabled\enum, "1", 		0x00000000, %ENABLED_STR%

; Kedron specific NDI values
[Reg_NDI_KDR]
HKR,,CLSGUID,0,"{4E82578B-20D2-4709-B663-CC9C3EA9C74A}"


[Reg_NDI_ALM]
HKR,,CLSGUID,0,"{AA7636EC-77CB-4e5a-9C1C-43950899EAAA}"


[Reg_NDIS_VISTA]
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5,wifipro"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet,wlan"
HKR, Ndi,             Service,      0, "NETw4v32"

; Registry settings by HW
; =========================

[Reg_KDR]
HKR,,ScanMode,0x10001,0x18
HKR,,WatchDogEnabled,0x10001,0x1
HKR,,CalibrationActive,0x10001,0x0000197F
HKR,,rlcChainSettings,0x10001,0x0
HKR,,ScanChainSelection,0x10001,0x37

[Reg_ALM]
HKR,,CalibrationActive,0x10001,0x0000001F
HKR,,IEEE11nMode,0x00000002,0x0
HKR,,BTEnableFlags,0x10001,0x3

; Registry settings by OS
; =========================

[Reg_Common_VISTA]
HKR,,TGeEnableBits,0x10001,0x27
HKR,,FeatureSet,0x10001,0xA1920001

; Registry settings by SKU
; =========================

[Reg_GEN_4965_AGN]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth,				ParamDesc, 	0, %CHANNELWIDTH%
HKR, Ndi\params\ChannelWidth,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_4965_AGN_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_GEN_4965_AGN_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x1
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_4965_AGN_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_4965_AGN_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AGN_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_4965_AGN_C]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth,				ParamDesc, 	0, %CHANNELWIDTH%
HKR, Ndi\params\ChannelWidth,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_GEN_4965_AGN_C_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_GEN_4965_AGN_C_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x1
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AGN_C_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AGN_C_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AGN_C_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	    0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_GEN_4965_AG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_GEN_4965_AG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_GEN_4965_AG_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	    0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_GEN_4965_AG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_GEN_4965_AG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_4965_AG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_GEN_3965_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_GEN_3965_ABG_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	     	0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_GEN_3965_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"



[Reg_GEN_3965_ABG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_3965_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_GEN_3945_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_GEN_3945_ABG_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_3945_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	    	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_GEN_3945_ABG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_3945_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_GEN_3945_BG]
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_GEN_3945_BGX]
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"Intel 802.11 Default SSID"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Lenovo_4965_AGN]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth,				ParamDesc, 	0, %CHANNELWIDTH%
HKR, Ndi\params\ChannelWidth,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_4965_AGN_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Lenovo_4965_AGN_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x1
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Lenovo_4965_AGN_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	     	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Lenovo_4965_AGN_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_C]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,  	Default,  0x00000002, "11"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,  	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default, 	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",  0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",  0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth,				ParamDesc, 	0, %CHANNELWIDTH%
HKR, Ndi\params\ChannelWidth,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Lenovo_4965_AGN_C_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Lenovo_4965_AGN_C_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,  	Default,  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,  	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,  	Type, 0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,  	Optional, 0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	  0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	 	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	 	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	 	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x1
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_C_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,  	Default,  0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,  	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,  	Type, 0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,  	Optional, 0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	 	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	  0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	  0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	 	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	 	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_C_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,  	Default,  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,  	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,  	Type, 0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,  	Optional, 0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	 	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	  0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	 	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	 	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AGN_C_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,  	Default,  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,  	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,  	Type, 0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,  	Optional, 0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	 	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	  0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	  0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	 	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	 	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	  0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	  0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	 	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	 	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24, Max,	  0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Lenovo_4965_AG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Lenovo_4965_AG_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	    	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_4965_AG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Lenovo_4965_AG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Lenovo_3965_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Lenovo_3965_ABG_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_3965_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	     	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Lenovo_3965_ABG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Lenovo_3965_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth,				ParamDesc, 	0, %CHANNELWIDTH%
HKR, Ndi\params\ChannelWidth,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_4965_AGN_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Dell_4965_AGN_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x1
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_C]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"
HKR, Ndi\params\IEEE11nMode,				ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,				Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,				Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,				Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 			"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 			"1",        0, %ENABLED_STR%

HKR, Ndi\params\ChannelWidth,				ParamDesc, 	0, %CHANNELWIDTH%
HKR, Ndi\params\ChannelWidth,				Type,      	0, "enum"
HKR, Ndi\params\ChannelWidth,				Default,   	0, "1"
HKR, Ndi\params\ChannelWidth,				Optional,  	0, "0"
HKR, Ndi\params\ChannelWidth\enum, 			"0",       0, %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth\enum, 			"1",       0, %CHANNELWIDTHAUTO%

HKR, Ndi\params\FatChannelIntolerant, 	    ParamDesc,		0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 		0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,		0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 		0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%

[Reg_Dell_4965_AGN_C_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Dell_4965_AGN_C_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x1
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_C_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_C_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AGN_C_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR,,ForceDuplicateDcr,0x10001,0x0
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"

[Reg_Dell_4965_AG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Dell_4965_AG_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Dell_4965_AG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_4965_AG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"

[Reg_Dell_3965_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Dell_3965_ABG_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3965_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Dell_3965_ABG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3965_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"101"
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "1"

[Reg_Dell_3945_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Dell_3945_ABG_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3945_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Dell_3945_ABG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Dell_3945_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "10"

[Reg_Toshiba_3965_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Toshiba_3965_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3965_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Toshiba_3965_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3965_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "10"

[Reg_Toshiba_3945_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Toshiba_3945_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3945_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Toshiba_3945_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Toshiba_3945_BGX]
HKR,,BandType,0x10003,0x0
HKR,,LedMode,0x10001,0x1
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "10"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Sony_3965_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Sony_3965_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"

[Reg_Sony_3965_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3965_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	    	0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Sony_3965_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3965_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_Sony_3945_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_Sony_3945_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3945_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_Sony_3945_ABG_JPN]
HKR,,JPNLegacyChannels,0x10003,0x1
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_Sony_3945_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_HP_3965_ABG]
HKR,,LedMode,0x10001,0x2
HKR,,BandType,0x10003,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_HP_3965_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_HP_3965_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3965_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3965_ABG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 	0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3965_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,LedMode,0x10001,0x2
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_HP_3945_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_HP_3945_ABG_MOW2]
HKR,,JPNLegacyChannels,0x10003,0x0
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11" 
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3945_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_HP_3945_ABG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_HP_3945_ABG_KRA]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	     	0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,       Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_IBM_3945_ABG]
HKR,,BandType,0x10003,0x2
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"

[Reg_IBM_3945_ABG_MOW1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_IBM_3945_ABG_MOW2]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_IBM_3945_ABG_RoW]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"149",	    0x00000002, "149"
HKR, Ndi\params\RecommendedChannel52\enum, 	"153",	    0x00000002, "153"
HKR, Ndi\params\RecommendedChannel52\enum, 	"157",	   	0x00000002, "157"
HKR, Ndi\params\RecommendedChannel52\enum, 	"161",	   	0x00000002, "161"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"


[Reg_IBM_3945_ABG_JPN]
HKR,,IEEE11dMode,0x10001,0x0
HKR,,JPNLegacyChannels,0x10003,0x1
HKR, Ndi\params\RecommendedChannel52,      	Default,    0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL52_STR%
HKR, Ndi\params\RecommendedChannel52,      	Type,       0x00000002, "enum"
HKR, Ndi\params\RecommendedChannel52,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel52\enum, 	"0",	   	  0x00000000, %AUTO_STR%
HKR, Ndi\params\RecommendedChannel52\enum, 	"36",	      0x00000002, "36"
HKR, Ndi\params\RecommendedChannel52\enum, 	"40",	      0x00000002, "40"
HKR, Ndi\params\RecommendedChannel52\enum, 	"44",	   	  0x00000002, "44"
HKR, Ndi\params\RecommendedChannel52\enum, 	"48",	   	  0x00000002, "48"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "13"
HKR, Ndi\params\RecommendedBand, 				ParamDesc,	0x00000000, %RECOMMENDED_BAND%
HKR, Ndi\params\RecommendedBand, 				Type,	 			0x00000002, "enum"
HKR, Ndi\params\RecommendedBand, 				Default,	  0x00000002, "0" ;b/g
HKR, Ndi\params\RecommendedBand, 				Optional, 	0x00000002, "0"
HKR, Ndi\params\RecommendedBand\enum,  	"0",	  		0x00000002, "0. 802.11b/g"
HKR, Ndi\params\RecommendedBand\enum,  	"1",	  		0x00000002, "1. 802.11a"

[Reg_IBM_3945_BG]
HKR,,BandType,0x10003,0x0
HKR,,DesiredSsid,0x00000002,"WXYZ"
HKR,,LedMode,0x10001,0x3
HKR, Ndi\params\RecommendedChannel24,      	Default,    0x00000002, "11"
HKR, Ndi\params\RecommendedChannel24,      	Max,	      0x00000002, "11"

[Reg_MPCIEX_3965ABG]
HKR,,Diversity11a,0x10003,0x3
HKR,,Diversity11b,0x10003,0x3
HKR,,Diversity11g,0x10003,0x3
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_3965ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_3965ABG%

[Reg_MPCIEX_3945ABG]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_3945ABG%
HKR,,DriverDesc,0,%NIC_DriverDesc_3945ABG%

[Reg_MPCIEX_3945BG]
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_3945BG%
HKR,,DriverDesc,0,%NIC_DriverDesc_3945BG%

[Reg_MPCIEX_4965AGN] 
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0 
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_4965AGN%
HKR,,DriverDesc,0,%NIC_DriverDesc_4965AGN%

[Reg_MPCIEX_4965AG] 
HKR,,Diversity11a,0x10003,0x0
HKR,,Diversity11b,0x10003,0x0
HKR,,Diversity11g,0x10003,0x0 
HKR,,AdapterModel,0,%NIC_MPCIEX_AdapterModel_4965AG%
HKR,,DriverDesc,0,%NIC_DriverDesc_4965AG%


; Registry settings for Binding
; =============================

[Reg_CoInstaller32]
HKR,,CoInstallers32,0x00010000,"NETw4c32.dll,ClassCoInstallerEntryPoint"

[MSI_NDIS.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1


; Registry settings for EventLogs
; ===============================

[Common_EventLog_VISTA]
AddReg = Reg_CommonAddEventLog_VISTA

[Reg_CommonAddEventLog_VISTA]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\NETw4v32.sys"
HKR,, TypesSupported,   0x00010001, 7

[Reg_GEN_3945_ABG_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_3945_ABG_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_3945_ABG_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_3945_ABG_SP4]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_4965_AGN_C_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_GEN_4965_AGN_C_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_GEN_4965_AGN_C_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_GEN_4965_AGN_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_GEN_4965_AGN_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_GEN_4965_AGN_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_GEN_4965_AG_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_4965_AG_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_GEN_4965_AG_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Lenovo_4965_AGN_C_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Lenovo_4965_AGN_C_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Lenovo_4965_AGN_C_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Lenovo_4965_AGN_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Lenovo_4965_AGN_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Lenovo_4965_AGN_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Lenovo_4965_AG_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Lenovo_4965_AG_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Lenovo_4965_AG_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Dell_4965_AGN_C_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Dell_4965_AGN_C_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Dell_4965_AGN_C_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Dell_4965_AGN_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Dell_4965_AGN_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Dell_4965_AGN_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"
HKR,,ForceDuplicateDcr,0x10001,0x0

[Reg_Dell_4965_AG_SP1]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Dell_4965_AG_SP2]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"

[Reg_Dell_4965_AG_SP3]
HKR,,IEEE11dMode,0x10001,0x0
HKR, Ndi\params\RecommendedChannel24,  	Max,	  0x00000002, "11"


[NIC_Service_VISTA]
DisplayName = %NIC_Service_DispName_VISTA%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\NETw4v32.sys
LoadOrderGroup  = NDIS

[Common_EventLog_VISTA]
AddReg = Reg_CommonAddEventLog_VISTA

;-----------------------------------------
; DestinationDirs

[CopyFiles_Driver_VISTA]
NETw4v32.sys,,,2


[CopyFiles_NCPA32]
NETw4c32.dll,,,2
NETw4r32.dll,,,2

[SourceDisksNames]
1=%SOURCEDISK1%,,

[SourceDisksFiles]
NETw4v32.sys   = 1,,
NETw4c32.dll = 1,,
NETw4r32.dll = 1,,

[DestinationDirs]
DefaultDestDir            = 11 ; Windows\System32
CopyFiles_Driver_VISTA=12;Windows\System32\Drivers
CopyFiles_NCPA32          = 11 ; Windows\System32

[Strings]
PROVIDER_NAME                        = "Intel"
COMPANY_NAME                         = "Intel Corporation"

NIC_MPCIEX_3945ABG                 = "Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  = "Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 = "Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  = "Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 = "Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  = "Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    = "Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     = "Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    = "Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     = "Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    = "Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     = "Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               = "Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         = "Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   = "Intel(R) Wireless WiFi Link 3945ABG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                = "Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    = "Intel(R) Wireless WiFi Link 3945BG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               = "Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   = "Intel(R) Wireless WiFi Link 3965ABG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                = "Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    = "Intel(R) Wireless WiFi Link 3965BG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               = "Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   = "Intel(R) Wireless WiFi Link 4965AGN Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 = "Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    = "Intel(R) Wireless WiFi Link 4965AG Adapter Driver for Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           = "Intel(R) Wireless WiFi Link Adapter Driver for Windows Vista 32 Bit"

SOURCEDISK1                          = "Intel(R) Wireless WiFi Link 4965AGN Install Disk"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	= "Ad Hoc Channel 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	= "Ad Hoc Channel 802.11 a"
RECOMMENDED_BAND          	= "Ad Hoc Default Wireless Mode"
IBSS_TX_POWER_STR           = "Transmit Power"
ROAMING_AGGRESSIVENESS_STR	= "Roaming Aggressiveness"
ADHOC_POWER_MANAGEMENT_STR	= "Ad Hoc Power Management"
ADHOC_QOS_MODE_STR          = "Ad Hoc QoS Mode"
MIXED_MODE_PROTECTION_STR   = "Mixed Mode Protection"
THROUGHPUT_ENHANCEMENT_STR  = "Throughput Enhancement"
WIRELESS_MODE_STR           = "Wireless Mode"
CHANNELWIDTH                = "802.11n Channel Width"
TGnMode                     = "802.11n Mode"
FAT_CHANNEL_TOLERANT		= "Fat Channel Intolerant"

LOWEST_STR					= "Lowest"
MEDIUM_LOW_STR				= "Medium-low"
MEDIUM_STR					= "Medium"
MEDIUM_HIGH_STR				= "Medium-High"
HIGHEST_STR					= "Highest"
DISABLED_STR				= "Disabled"
ENABLED_STR 				= "Enabled"
MAXIMUM_POWER_SAVING_STR	= "Maximum Power Savings"
NOISY_ENVIRONMENT_STR		= "Noisy Environment"
WMM_STR                     = "WMM "
CTS_TO_SELF_ENABLED_STR     = "CTS-to-self Enabled"
RTS_CTS_ENABLED_STR         = "RTS/CTS Enabled"
AUTO_STR                    = "Auto"
CHANNELWIDTH20ONLY          = "20 MHz Only"
CHANNELWIDTHAUTO            = "Auto"
WMM_DISABLED_STR            = "WMM Disabled"
WMM_ENABLED_STR             = "WMM Enabled"


[Strings.0401] ; Arabic (Saudi Arabia)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Wireless WiFi Link 3945ABG áäÙÇã Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Wireless WiFi Link 3945BG áäÙÇã Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Wireless WiFi Link 3965ABG áäÙÇã Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Wireless WiFi Link 3965BG áäÙÇã Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Wireless WiFi Link 4965AGN áäÙÇã Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Wireless WiFi Link 4965AG áäÙÇã Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="ÈÑäÇãÌ ÊÔÛíá ãÍæá Intel(R) Wireless WiFi Link áäÙÇã Windows Vista 32 Bit"

SOURCEDISK1                          ="ÞÑÕ ÊËÈíÊ Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="ÞäÇÉ ÇáÃÞÑÇä 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="ÞäÇÉ ÇáÃÞÑÇä 802.11a"
RECOMMENDED_BAND          	="æÖÚ ÇááÇÓáßí ÇáÇÝÊÑÇÖí ááÃÞÑÇä"
IBSS_TX_POWER_STR           ="ØÇÞÉ ÇáÅÑÓÇá"
ROAMING_AGGRESSIVENESS_STR	="äÔÇØ ÇáÊÌæÇá"
ADHOC_POWER_MANAGEMENT_STR	="ÅÏÇÑÉ ØÇÞÉ ÇáÃÞÑÇä"
ADHOC_QOS_MODE_STR          ="ÇáæÖÚ QoS ááÃÞÑÇä"
MIXED_MODE_PROTECTION_STR   ="ÍãÇíÉ ÇáæÖÚ ÇáãÎÊáØ"
THROUGHPUT_ENHANCEMENT_STR  ="ÊÍÓíä ÇáÎÑÌ"
WIRELESS_MODE_STR           ="æÖÚ ÇááÇÓáßí"
CHANNELWIDTH                ="ÚÑÖ ÞäÇÉ 802.11n"
TGnMode                     ="æÖÚ 802.11n"
FAT_CHANNEL_TOLERANT		="ÛíÑ ãÊæÇÝÞ ãÚ ÞäÇÉ 40 ãíÌÇåíÑÊÒ"

LOWEST_STR					="ÇáÃÏäì"
MEDIUM_LOW_STR				="ãÊæÓØ-ãäÎÝÖ"
MEDIUM_STR					="ãÊæÓØ"
MEDIUM_HIGH_STR				="ãÊæÓØ-ãÑÊÝÚ"
HIGHEST_STR					="ÇáÃÚáì"
DISABLED_STR				="ãÚØá"
ENABLED_STR 				="ããßøóä"
MAXIMUM_POWER_SAVING_STR	="ÃÞÕì ÊæÝíÑ ááØÇÞÉ"
NOISY_ENVIRONMENT_STR		="ÈíÆÉ ÇáÖæÖÇÁ"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="Êãßíä CTS ÇáÐÇÊí"
RTS_CTS_ENABLED_STR         ="Êãßíä RTS/CTS"
AUTO_STR                    ="ÊáÞÇÆí"
CHANNELWIDTH20ONLY          ="20 ãíÌÇåíÑÊÒ ÝÞØ"
CHANNELWIDTHAUTO            ="ÊáÞÇÆí"
WMM_DISABLED_STR            ="ãÚØá WMM"
WMM_ENABLED_STR             ="ããßøóä WMM"


[Strings.0804] ; Chinese (Simplified)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Intel(R) Wireless WiFi Link 3945ABG ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows Vista 32 Î»£©"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Intel(R) Wireless WiFi Link 3945BG ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows Vista 32 Î»£©"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Intel(R) Wireless WiFi Link 3965ABG ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows Vista 32 Î»£©"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Intel(R) Wireless WiFi Link 3965BG ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows Vista 32 Î»£©"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Intel(R) Wireless WiFi Link 4965AGN ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows Vista 32 Î»£©"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Intel(R) Wireless WiFi Link 4965AG ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows Vista 32 Î»£©"

NIC_Service_DispName_VISTA           ="Intel(R) Wireless WiFi Link ÊÊÅäÆ÷Çý¶¯³ÌÐò£¨ÊÊÓÃÓÚ Windows Vista 32 Î»£©"

SOURCEDISK1                          ="Intel(R) Wireless WiFi Link 4965AGN °²×°ÅÌ"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad Hoc ÐÅµÀ 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	="Ad Hoc ÐÅµÀ 802.11a"
RECOMMENDED_BAND          	="Ad Hoc Ä¬ÈÏÎÞÏßÄ£Ê½"
IBSS_TX_POWER_STR           ="·¢ÉäµçÔ´"
ROAMING_AGGRESSIVENESS_STR	="ÂþÓÎÖ÷¶¯ÐÔ"
ADHOC_POWER_MANAGEMENT_STR	="Ad Hoc µçÔ´¹ÜÀí"
ADHOC_QOS_MODE_STR          ="Ad Hoc QoS Ä£Ê½"
MIXED_MODE_PROTECTION_STR   ="»ìºÏÄ£Ê½±£»¤"
THROUGHPUT_ENHANCEMENT_STR  ="ÍÌÍÂÁ¿ÔöÇ¿"
WIRELESS_MODE_STR           ="ÎÞÏßÄ£Ê½"
CHANNELWIDTH                ="802.11n ÐÅµÀ¿í¶È"
TGnMode                     ="802.11n Ä£Ê½"
FAT_CHANNEL_TOLERANT		="Óë 40Mhz ÐÅµÀ²»¼æÈÝ"

LOWEST_STR					="×îµÍÖµ"
MEDIUM_LOW_STR				="ÖÐµÍ"
MEDIUM_STR					="ÖÐ¼ä"
MEDIUM_HIGH_STR				="ÖÐ¸ß"
HIGHEST_STR					="×î¸ßÖµ"
DISABLED_STR				="ÒÑ½ûÓÃ"
ENABLED_STR 				="ÒÑÆôÓÃ"
MAXIMUM_POWER_SAVING_STR	="×î´óºÄµçÁ¿½ÚÄÜ"
NOISY_ENVIRONMENT_STR		="àÐÔÓ»·¾³"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS ÖÁ×ÔÉíÆôÓÃ"
RTS_CTS_ENABLED_STR         ="RTS/CTS ÆôÓÃ"
AUTO_STR                    ="×Ô¶¯"
CHANNELWIDTH20ONLY          ="½ö 20 MHz"
CHANNELWIDTHAUTO            ="×Ô¶¯"
WMM_DISABLED_STR            ="WMM ÒÑ½ûÓÃ"
WMM_ENABLED_STR             ="WMM ÒÑÆôÓÃ"


[Strings.0404] ; Chinese (Traditional)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 3945ABG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 3945BG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 3965ABG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 3965BG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 4965AGN ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 4965AG ¤¶­±¥dÅX°Êµ{¦¡"

NIC_Service_DispName_VISTA           ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link ¤¶­±¥dÅX°Êµ{¦¡"

SOURCEDISK1                          ="Intel(R) Wireless WiFi Link 4965AGN ¦w¸ËºÏºÐ"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="ÂI¹ïÂI (ad hoc) ³q¹D 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="ÂI¹ïÂI (ad hoc) ³q¹D 802.11a"
RECOMMENDED_BAND          	="ÂI¹ïÂI (ad hoc) ¹w³]µL½u¼Ò¦¡"
IBSS_TX_POWER_STR           ="¶Ç¿é¹q·½"
ROAMING_AGGRESSIVENESS_STR	="º©¹C¿n·¥«×"
ADHOC_POWER_MANAGEMENT_STR	="ÂI¹ïÂI (ad hoc) ¹q·½ºÞ²z"
ADHOC_QOS_MODE_STR          ="ÂI¹ïÂI (ad hoc) QoS ¼Ò¦¡"
MIXED_MODE_PROTECTION_STR   ="²V¦X¼Ò¦¡«OÅ@"
THROUGHPUT_ENHANCEMENT_STR  ="¿é°e¶q¼W±j¥\¯à"
WIRELESS_MODE_STR           ="µL½u¼Ò¦¡"
CHANNELWIDTH                ="802.11n ³q¹D¼e«×"
TGnMode                     ="802.11n ¼Ò¦¡"
FAT_CHANNEL_TOLERANT		="¤£®e¤j¶q³q¹D"

LOWEST_STR					="³Ì§C"
MEDIUM_LOW_STR				="¤¤§C"
MEDIUM_STR					="¤¤"
MEDIUM_HIGH_STR				="¤¤°ª"
HIGHEST_STR					="³Ì°ª"
DISABLED_STR				="°±¥Î"
ENABLED_STR 				="±Ò¥Î"
MAXIMUM_POWER_SAVING_STR	="³Ì¬Ù¹q"
NOISY_ENVIRONMENT_STR		="¾¸­µÀô¹Ò"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="±Ò¥Î CTS-to-self"
RTS_CTS_ENABLED_STR         ="±Ò¥Î RTS/CTS"
AUTO_STR                    ="¦Û°Ê"
CHANNELWIDTH20ONLY          ="¶È­­©ó 20 MHz"
CHANNELWIDTHAUTO            ="¦Û°Ê"
WMM_DISABLED_STR            ="WMM °±¥Î"
WMM_ENABLED_STR             ="WMM ±Ò¥Î"


[Strings.0405] ; Czech (Czech Republic)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Ovladaè adaptéru Intel(R) Wireless WiFi Link 3945ABG pro systém Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Ovladaè adaptéru Intel(R) Wireless WiFi Link 3945BG pro systém Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Ovladaè adaptéru Intel(R) Wireless WiFi Link 3965ABG pro systém Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Ovladaè adaptéru Intel(R) Wireless WiFi Link 3965BG pro systém Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Ovladaè adaptéru Intel(R) Wireless WiFi Link 4965AGN pro systém Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Ovladaè adaptéru Intel(R) Wireless WiFi Link 4965AG pro systém Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="Ovladaè adaptéru Intel(R) Wireless WiFi Link pro systém Windows Vista 32 Bit"

SOURCEDISK1                          ="Instalaèní disk adaptéru Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Kanál ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Kanál ad hoc 802.11a"
RECOMMENDED_BAND          	="Výchozí bezdrátový režim ad hoc"
IBSS_TX_POWER_STR           ="Vysílací energie"
ROAMING_AGGRESSIVENESS_STR	="Agresivita roamingu"
ADHOC_POWER_MANAGEMENT_STR	="Správa napájení ad hoc"
ADHOC_QOS_MODE_STR          ="Režim Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   ="Ochrana smíšeného režimu"
THROUGHPUT_ENHANCEMENT_STR  ="Zlepšení propustnosti"
WIRELESS_MODE_STR           ="Bezdrátový režim"
CHANNELWIDTH                ="Šíøka kanálu 802.11n"
TGnMode                     ="Režim 802.11n"
FAT_CHANNEL_TOLERANT		="Nekompatibilní s šíøkou kanálu 40 MHz"

LOWEST_STR					="Nejnižší"
MEDIUM_LOW_STR				="Støednì nízký"
MEDIUM_STR					="Støední"
MEDIUM_HIGH_STR				="Støednì vysoký"
HIGHEST_STR					="Nejvyšší"
DISABLED_STR				="Zakázáno"
ENABLED_STR 				="Povoleno"
MAXIMUM_POWER_SAVING_STR	="Maximální úspora energie"
NOISY_ENVIRONMENT_STR		="Prostøedí s velkým šumem"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-to-self povoleno"
RTS_CTS_ENABLED_STR         ="RTS/CTS povoleno"
AUTO_STR                    ="Automaticky"
CHANNELWIDTH20ONLY          ="Pouze 20 MHz"
CHANNELWIDTHAUTO            ="Automaticky"
WMM_DISABLED_STR            ="WMM zakázáno"
WMM_ENABLED_STR             ="WMM povoleno"


[Strings.0406] ; Danish (Denmark)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Intel(R) Wireless WiFi Link 3945BG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Intel(R) Wireless WiFi Link 3965ABG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Intel(R) Wireless WiFi Link 3965BG Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Intel(R) Wireless WiFi Link 4965AGN Adapter Driver for Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Intel(R) Wireless WiFi Link 4965AG Adapter Driver for Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="Intel(R) Wireless WiFi Link Adapter Driver for Windows Vista 32 Bit"

SOURCEDISK1                          ="Intel(R) Wireless WiFi Link 4965AGN Install Disk"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad hoc-kanal 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	="Ad hoc-kanal 802.11 a"
RECOMMENDED_BAND          	="Ad hoc standard trådløs tilstand"
IBSS_TX_POWER_STR           ="Sendeeffekt"
ROAMING_AGGRESSIVENESS_STR	="Roaming-aggressivitet"
ADHOC_POWER_MANAGEMENT_STR	="Ad Hoc-strømstyring"
ADHOC_QOS_MODE_STR          ="Ad Hoc QoS-tilstand"
MIXED_MODE_PROTECTION_STR   ="Beskyttelse i blandet miljø"
THROUGHPUT_ENHANCEMENT_STR  ="Forbedring af ydelse"
WIRELESS_MODE_STR           ="Trådløs tilstand"
CHANNELWIDTH                ="802.11n kanalbredde"
TGnMode                     ="802.11n tilstand"
FAT_CHANNEL_TOLERANT		="40Mhz kanal intolerant"

LOWEST_STR					="Laveste"
MEDIUM_LOW_STR				="Mellem-lav"
MEDIUM_STR					="Mellem"
MEDIUM_HIGH_STR				="Mellem-høj"
HIGHEST_STR					="Højeste"
DISABLED_STR				="Deaktiveret"
ENABLED_STR 				="Aktiveret"
MAXIMUM_POWER_SAVING_STR	="Maks. strømbesparelse"
NOISY_ENVIRONMENT_STR		="Støjfyldt miljø"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-to-self activeret "
RTS_CTS_ENABLED_STR         ="RTS/CTS aktiveret "
AUTO_STR                    ="Auto"
CHANNELWIDTH20ONLY          ="Kun 20 MHz"
CHANNELWIDTHAUTO            ="Auto"
WMM_DISABLED_STR            ="WMM deaktiveret"
WMM_ENABLED_STR             ="WMM aktiveret"


[Strings.0407] ; German (Germany)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Intel(R) Wireless WiFi Link 3945ABG Adaptertreiber für Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Intel(R) Wireless WiFi Link 3945BG Adaptertreiber für Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Intel(R) Wireless WiFi Link 3965ABG Adaptertreiber für Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Intel(R) Wireless WiFi Link 3965BG Adaptertreiber für Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Intel(R) Wireless WiFi Link 4965AGN Adaptertreiber für Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Intel(R) Wireless WiFi Link 4965AG Adaptertreiber für Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="Intel(R) Wireless WiFi Link Adaptertreiber für Windows Vista 32 Bit"

SOURCEDISK1                          ="Intel(R) Wireless WiFi Link 4965AGN Installationsdisk"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad-Hoc-Kanal 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	="Ad-Hoc-Channel 802.11 a"
RECOMMENDED_BAND          	="Standard-WLAN-Modus für Ad-hoc"
IBSS_TX_POWER_STR           ="Übertragungsleistung"
ROAMING_AGGRESSIVENESS_STR	="Roaming-Dynamik"
ADHOC_POWER_MANAGEMENT_STR	="Ad-Hoc-Energieverwaltung"
ADHOC_QOS_MODE_STR          ="Ad-Hoc QoS-Modus"
MIXED_MODE_PROTECTION_STR   ="Schutz f. gemischte Umgebungen"
THROUGHPUT_ENHANCEMENT_STR  ="Durchsatzverbesserung"
WIRELESS_MODE_STR           ="Drahtloser Modus"
CHANNELWIDTH                ="802.11n Kanalbreite"
TGnMode                     ="802.11n Modus"
FAT_CHANNEL_TOLERANT		="Nur 20-MHz-Kanal"

LOWEST_STR					="Niedrig"
MEDIUM_LOW_STR				="Mittel-niedrig"
MEDIUM_STR					="Mittel"
MEDIUM_HIGH_STR				="Mittel-hoch"
HIGHEST_STR					="Hoch"
DISABLED_STR				="Deaktiviert"
ENABLED_STR 				="Aktiviert"
MAXIMUM_POWER_SAVING_STR	="Maximale Energieersparnis"
NOISY_ENVIRONMENT_STR		="Laute Umgebung"
WMM_STR                     ="WMM"
CTS_TO_SELF_ENABLED_STR     ="'CTS-to-self' aktiviert"
RTS_CTS_ENABLED_STR         ="RTS/CTS aktiviert"
AUTO_STR                    ="Auto"
CHANNELWIDTH20ONLY          ="nur 20 MHz"
CHANNELWIDTHAUTO            ="Auto"
WMM_DISABLED_STR            ="WMM deaktiviert"
WMM_ENABLED_STR             ="WMM aktiviert"


[Strings.0408] ; Greek (Greece)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Wireless WiFi Link 3945ABG ãéá Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Wireless WiFi Link 3945BG ãéá Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Wireless WiFi Link 3965ABG ãéá Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Wireless WiFi Link 3965BG ãéá Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Wireless WiFi Link 4965AGN ãéá Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Wireless WiFi Link 4965AG ãéá Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="Ðñüãñáììá ïäÞãçóçò ðñïóáñìïãÝá Intel(R) Wireless WiFi Link ãéá Windows Vista 32 Bit"

SOURCEDISK1                          ="ÄéóêÝôá åãêáôÜóôáóçò Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="ÊáíÜëé ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="ÊáíÜëé ad hoc 802.11a"
RECOMMENDED_BAND          	="ÐñïåðéëåãìÝíç áóýñìáôç ëåéôïõñãßá ad hoc"
IBSS_TX_POWER_STR           ="ÌåôÜäïóç éó÷ýïò"
ROAMING_AGGRESSIVENESS_STR	="Äõíáìéêüôçôá ðåñéáãùãÞò"
ADHOC_POWER_MANAGEMENT_STR	="Äéá÷åßñéóç éó÷ýïò ad hoc"
ADHOC_QOS_MODE_STR          ="Ôñüðïò ëåéôïõñãßáò Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   ="Ðñïóôáóßá ìåéêôÞò ëåéôïõñãßáò"
THROUGHPUT_ENHANCEMENT_STR  ="Âåëôßùóç éêáíüôçôáò ìåôÜäïóçò"
WIRELESS_MODE_STR           ="Áóýñìáôç êáôÜóôáóç"
CHANNELWIDTH                ="Åýñïò êáíáëéïý 802.11n"
TGnMode                     ="Ëåéôïõñãßá 802.11n"
FAT_CHANNEL_TOLERANT		="Ìç óõìâáôü ìå éó÷õñÜ êáíÜëéá"

LOWEST_STR					="×áìçëüôåñç"
MEDIUM_LOW_STR				="Ìåóáßá-×áìçëÞ"
MEDIUM_STR					="Ìåóáßá"
MEDIUM_HIGH_STR				="Ìåóáßá-ÕøçëÞ"
HIGHEST_STR					="Õøçëüôåñç"
DISABLED_STR				="Áðåíåñãïðïßçóç"
ENABLED_STR 				="ÅíåñãïðïéçìÝíç"
MAXIMUM_POWER_SAVING_STR	="ÌÝãéóôåò åîïéêïíïìÞóåéò éó÷ýïò"
NOISY_ENVIRONMENT_STR		="Èïñõâþäåò ðåñéâÜëëïí"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="ÅíåñãïðïéçìÝíï CTS-to-self"
RTS_CTS_ENABLED_STR         ="ÅíåñãïðïéçìÝíï RTS/CTS"
AUTO_STR                    ="Áõôüìáôá"
CHANNELWIDTH20ONLY          ="Ìüíï 20 MHz"
CHANNELWIDTHAUTO            ="Áõôüìáôá"
WMM_DISABLED_STR            ="Áðåíåñãïðïßçóç WMM"
WMM_ENABLED_STR             ="ÅíåñãïðïéçìÝíç WMM"


[Strings.0C0A] ; Spanish (Spain)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Controlador del adaptador Intel(R) Wireless WiFi Link 3945ABG para Windows Vista de 32 bits"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Controlador del adaptador Intel(R) Wireless WiFi Link 3945BG para Windows Vista de 32 bits"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Controlador del adaptador Intel(R) Wireless WiFi Link 3965ABG para Windows Vista de 32 bits"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Controlador del adaptador Intel(R) Wireless WiFi Link 3965BG para Windows Vista de 32 bits"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Controlador del adaptador Intel(R) Wireless WiFi Link 4965AGN para Windows Vista de 32 bits"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Controlador del adaptador Intel(R) Wireless WiFi Link 4965AG para Windows Vista de 32 bits"

NIC_Service_DispName_VISTA           ="Controlador del adaptador Intel(R) Wireless WiFi Link para Windows Vista de 32 bits"

SOURCEDISK1                          ="Disco de instalación de Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canal Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Canal Ad Hoc 802.11a"
RECOMMENDED_BAND          	="Modo inalámbrico predeterminado Ad Hoc"
IBSS_TX_POWER_STR           ="Potencia de transmisión"
ROAMING_AGGRESSIVENESS_STR	="Agresividad de itinerancia"
ADHOC_POWER_MANAGEMENT_STR	="Administración de energía Ad Hoc"
ADHOC_QOS_MODE_STR          ="Modo QoS Ad Hoc"
MIXED_MODE_PROTECTION_STR   ="Protección de modo mixto"
THROUGHPUT_ENHANCEMENT_STR  ="Optimización de la capacidad de proceso"
WIRELESS_MODE_STR           ="Modo inalámbrico"
CHANNELWIDTH                ="Ancho de canal 802.11n"
TGnMode                     ="Modo 802.11n"
FAT_CHANNEL_TOLERANT		="No compatible con canal de 40 Mhz"

LOWEST_STR					="Mínimo"
MEDIUM_LOW_STR				="Bajo"
MEDIUM_STR					="Mediano"
MEDIUM_HIGH_STR				="Alto"
HIGHEST_STR					="Máximo"
DISABLED_STR				="Desactivado"
ENABLED_STR 				="Activado"
MAXIMUM_POWER_SAVING_STR	="Máximo ahorro de energía"
NOISY_ENVIRONMENT_STR		="Entorno ruidoso"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-to-self activado"
RTS_CTS_ENABLED_STR         ="RTS/CTS activado"
AUTO_STR                    ="Automático"
CHANNELWIDTH20ONLY          ="Sólo 20 MHz"
CHANNELWIDTHAUTO            ="Automático"
WMM_DISABLED_STR            ="WMM desactivado"
WMM_ENABLED_STR             ="WMM activado"


[Strings.040B] ; Finnish (Finland)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Intel(R) Wireless WiFi Link 3945ABG -sovitinohjain Windows Vista 32-bit -käyttöjärjestelmään"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Intel(R) Wireless WiFi Link 3945BG -sovitinohjain Windows Vista 32-bit -käyttöjärjestelmään"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Intel(R) Wireless WiFi Link 3965ABG -sovitinohjain Windows Vista 32-bit -käyttöjärjestelmään"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Intel(R) Wireless WiFi Link 3965ABG -sovitinohjain Windows Vista 32-bit -käyttöjärjestelmään"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Intel(R) Wireless WiFi Link 4965ABG -sovitinohjain Windows Vista 32-bit -käyttöjärjestelmään"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Intel(R) Wireless WiFi Link 4965AG -sovitinohjain Windows Vista 32-bit -käyttöjärjestelmään"

NIC_Service_DispName_VISTA           ="Intel(R) Wireless WiFi Link -sovitinohjain Windows Vista 32-bit -käyttöjärjestelmään"

SOURCEDISK1                          ="Intel(R) Wireless WiFi Link 4965AGN -asennuslevy"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad Hoc -kanava 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Ad Hoc -kanava 802.11a "
RECOMMENDED_BAND          	="Langaton Ad Hoc -oletustila"
IBSS_TX_POWER_STR           ="Lähetysteho"
ROAMING_AGGRESSIVENESS_STR	="Solukonpäivitysaktiivisuus"
ADHOC_POWER_MANAGEMENT_STR	="Ad Hoc -virranhallinta"
ADHOC_QOS_MODE_STR          ="Ad Hoc QoS -tila"
MIXED_MODE_PROTECTION_STR   ="Sekatilasuojaus"
THROUGHPUT_ENHANCEMENT_STR  ="Läpimenon parantaminen"
WIRELESS_MODE_STR           ="Langaton tila"
CHANNELWIDTH                ="802.11n-kanavaleveys"
TGnMode                     ="802.11n-tila"
FAT_CHANNEL_TOLERANT		="Fat Channel -esto"

LOWEST_STR					="Pienin"
MEDIUM_LOW_STR				="Kohtalainen-pieni"
MEDIUM_STR					="Kohtalainen"
MEDIUM_HIGH_STR				="Kohtalainen-suuri"
HIGHEST_STR					="Suurin"
DISABLED_STR				="Poissa käytöstä"
ENABLED_STR 				="Käytössä"
MAXIMUM_POWER_SAVING_STR	="Suurin virransäästö"
NOISY_ENVIRONMENT_STR		="Häiriöllinen ympäristö"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS itselle käytössä"
RTS_CTS_ENABLED_STR         ="RTS/CTS käytössä"
AUTO_STR                    ="Automaattinen"
CHANNELWIDTH20ONLY          ="Vain 20 MHz"
CHANNELWIDTHAUTO            ="Automaattinen"
WMM_DISABLED_STR            ="WMM poissa käytöstä"
WMM_ENABLED_STR             ="WMM käytössä"


[Strings.040C] ; French (France)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Pilote de carte Intel(R) Wireless WiFi Link 3945ABG pour Windows Vista 32 bits"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Pilote de carte Intel(R) Wireless WiFi Link 3945BG pour Windows Vista 32 bits"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Pilote de carte Intel(R) Wireless WiFi Link 3965ABG pour Windows Vista 32 bits"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Pilote de carte Intel(R) Wireless WiFi Link 3965BG pour Windows Vista 32 bits"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Pilote de carte Intel(R) Wireless WiFi Link 4965AGN pour Windows Vista 32 bits"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Pilote de carte Intel(R) Wireless WiFi Link 4965AG pour Windows Vista 32 bits"

NIC_Service_DispName_VISTA           ="Pilote de carte Intel(R) Wireless WiFi Link pour Windows Vista 32 bits"

SOURCEDISK1                          ="Disque d'installation de la carte Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canal ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Canal ad hoc 802.11a"
RECOMMENDED_BAND          	="Mode ad hoc sans fil par défaut"
IBSS_TX_POWER_STR           ="Puissance de transmission"
ROAMING_AGGRESSIVENESS_STR	="Agressivité de l'itinérance"
ADHOC_POWER_MANAGEMENT_STR	="Gestion de l'alimentation ad hoc"
ADHOC_QOS_MODE_STR          ="Mode QS ad hoc"
MIXED_MODE_PROTECTION_STR   ="Protection en mode mixte"
THROUGHPUT_ENHANCEMENT_STR  ="Optimisation du débit"
WIRELESS_MODE_STR           ="Mode Sans fil"
CHANNELWIDTH                ="Largeur de canal 802.11n"
TGnMode                     ="Mode 802.11n"
FAT_CHANNEL_TOLERANT		="Non compatible avec les canaux de 40 MHz"

LOWEST_STR					="Min."
MEDIUM_LOW_STR				="Faible"
MEDIUM_STR					="Moyenne"
MEDIUM_HIGH_STR				="Élevée"
HIGHEST_STR					="Max."
DISABLED_STR				="Désactivée"
ENABLED_STR 				="Activée"
MAXIMUM_POWER_SAVING_STR	="Économie d'énergie max."
NOISY_ENVIRONMENT_STR		="Environnement bruyant"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="Auto-CTS activée"
RTS_CTS_ENABLED_STR         ="RTS/CTS activée"
AUTO_STR                    ="Auto"
CHANNELWIDTH20ONLY          ="20 MHz uniquement"
CHANNELWIDTHAUTO            ="Auto"
WMM_DISABLED_STR            ="WMM désactivée"
WMM_ENABLED_STR             ="WMM activée"


[Strings.040D] ; Hebrew (Israel)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="îðäì äú÷ï ùì îúàí Intel(R) Wireless WiFi Link 3945ABG òáåø Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="îðäì äú÷ï ùì îúàí Intel(R) Wireless WiFi Link 3945BG òáåø Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="îðäì äú÷ï ùì îúàí Intel(R) Wireless WiFi Link 3965ABG òáåø Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="îðäì äú÷ï ùì îúàí Intel(R) Wireless WiFi Link 3965BG òáåø Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="îðäì äú÷ï ùì îúàí Intel(R) Wireless WiFi Link 4965AGN òáåø Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="îðäì äú÷ï ùì îúàí Intel(R) Wireless WiFi Link 4965AG òáåø Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="îðäì äú÷ï ùì îúàí Intel(R) Wireless WiFi Link  òáåø Windows Vista 32 Bit"

SOURCEDISK1                          ="ãéñ÷ äú÷ðä ùì Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="òøåõ àã äå÷ 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="òøåõ àã äå÷ 802.11a"
RECOMMENDED_BAND          	="îöá àìçåèé áøéøú îçãì ùì àã äå÷"
IBSS_TX_POWER_STR           ="øîú ùéãåø"
ROAMING_AGGRESSIVENESS_STR	="úå÷ôðåú ðãéãä"
ADHOC_POWER_MANAGEMENT_STR	="ðéäåì öøéëú çùîì àã äå÷"
ADHOC_QOS_MODE_STR          ="îöá Ad Hoc Qos"
MIXED_MODE_PROTECTION_STR   ="äâðú îöá îòåøá"
THROUGHPUT_ENHANCEMENT_STR  ="ùéôåø ÷öá äòáøä"
WIRELESS_MODE_STR           ="îöá àìçåèé"
CHANNELWIDTH                ="øåçá òøåõ 802.11n"
TGnMode                     ="îöá 802.11n"
FAT_CHANNEL_TOLERANT		="ìà úåàí ìòøåõ 40Mhz"

LOWEST_STR					="ðîåê áéåúø"
MEDIUM_LOW_STR				="áéðåðé-ðîåê"
MEDIUM_STR					="áéðåðé"
MEDIUM_HIGH_STR				="áéðåðé-âáåä"
HIGHEST_STR					="âáåä áéåúø"
DISABLED_STR				="îðåèøì"
ENABLED_STR 				="æîéï"
MAXIMUM_POWER_SAVING_STR	="çéñëåï îøáé áçùîì"
NOISY_ENVIRONMENT_STR		="ñáéáä øåòùú"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="îàåôùø CTS-àì-òöîå (CTS-to-self)"
RTS_CTS_ENABLED_STR         ="îàåôùø RTS/CTS"
AUTO_STR                    ="àåèåîèé"
CHANNELWIDTH20ONLY          ="ý20 MHz áìáã"
CHANNELWIDTHAUTO            ="àåèåîèé"
WMM_DISABLED_STR            ="îðåèøì WMM"
WMM_ENABLED_STR             ="æîéï WMM"


[Strings.040E] ; Hungarian (Hungary)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Intel(R) Wireless WiFi Link 3945ABG adapter illesztõprogram 32 bites Windows Vistához"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Intel(R) Wireless WiFi Link 3945BG adapter illesztõprogram 32 bites Windows Vistához"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Intel(R) Wireless WiFi Link 3965ABG adapter illesztõprogram 32 bites Windows Vistához"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Intel(R) Wireless WiFi Link 3965BG adapter illesztõprogram 32 bites Windows Vistához"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Intel(R) Wireless WiFi Link 4965AGN adapter illesztõprogram 32 bites Windows Vistához"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Intel(R) Wireless WiFi Link 4965AG adapter illesztõprogram 32 bites Windows Vistához"

NIC_Service_DispName_VISTA           ="Intel(R) Wireless WiFi Link adapter illesztõprogram 32 bites Windows Vistához"

SOURCEDISK1                          ="Intel(R) Wireless WiFi Link 4965AGN telepítõ lemez"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Alkalmi csatorna 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	="Alkalmi csatorna 802.11 a"
RECOMMENDED_BAND          	="Alkalmi kapcsolat alapértelmezett vezeték nélküli üzemmódja"
IBSS_TX_POWER_STR           ="Sugárzási teljesítmény"
ROAMING_AGGRESSIVENESS_STR	="A barangolás intenzitása"
ADHOC_POWER_MANAGEMENT_STR	="Energiagazdálkodás alkalmi hálózatokon"
ADHOC_QOS_MODE_STR          ="Alkalmi QoS üzemmód"
MIXED_MODE_PROTECTION_STR   ="Vegyes üzemmódú védelem"
THROUGHPUT_ENHANCEMENT_STR  ="Az átviteli kapacitás növelése"
WIRELESS_MODE_STR           ="Vezeték nélküli üzemmód"
CHANNELWIDTH                ="802.11n csatorna-sávszélesség"
TGnMode                     ="802.11n üzemmód"
FAT_CHANNEL_TOLERANT		="Csökkentett sávszélességen mûködik"

LOWEST_STR					="Legalacsonyabb"
MEDIUM_LOW_STR				="Közepes - alacsony"
MEDIUM_STR					="Közepes"
MEDIUM_HIGH_STR				="Közepes - magas"
HIGHEST_STR					="Legmagasabb"
DISABLED_STR				="Letiltva"
ENABLED_STR 				="Engedélyezve"
MAXIMUM_POWER_SAVING_STR	="Max. energiatakarékosság"
NOISY_ENVIRONMENT_STR		="Zajos környezet"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-to-self engedélyezve"
RTS_CTS_ENABLED_STR         ="RTS/CTS engedélyezve"
AUTO_STR                    ="Auto"
CHANNELWIDTH20ONLY          ="Csak 20 MHz"
CHANNELWIDTHAUTO            ="Auto"
WMM_DISABLED_STR            ="WMM letiltva"
WMM_ENABLED_STR             ="WMM engedélyezve"


[Strings.0410] ; Italian (Italy)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Driver scheda Intel(R) Wireless WiFi Link 3945ABG per Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Driver scheda Intel(R) Wireless WiFi Link 3945BG per Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Driver scheda Intel(R) Wireless WiFi Link 3965ABG per Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Driver scheda Intel(R) Wireless WiFi Link 3965BG per Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Driver scheda Intel(R) Wireless WiFi Link 4965AGN per Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Driver scheda Intel(R) Wireless WiFi Link 4965AG per Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="Driver scheda Intel(R) Wireless WiFi Link per Windows Vista 32 Bit"

SOURCEDISK1                          ="Disco di installazione per Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canale Ad Hoc 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	="Canale Ad Hoc 802.11 a"
RECOMMENDED_BAND          	="Modalità wireless predefinita Ad Hoc"
IBSS_TX_POWER_STR           ="Potenza di trasmissione"
ROAMING_AGGRESSIVENESS_STR	="Efficacia roaming"
ADHOC_POWER_MANAGEMENT_STR	="Risparmio energia ad hoc"
ADHOC_QOS_MODE_STR          ="Modalità Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   ="Protezione modalità protetta"
THROUGHPUT_ENHANCEMENT_STR  ="Miglioramento velocità"
WIRELESS_MODE_STR           ="Modalità wireless"
CHANNELWIDTH                ="Larghezza canale 802.11n"
TGnMode                     ="Modalità 802.11n "
FAT_CHANNEL_TOLERANT		="Non compatibile con canale ad ampia larghezza"

LOWEST_STR					="Minimo"
MEDIUM_LOW_STR				="Medio-basso"
MEDIUM_STR					="Medio"
MEDIUM_HIGH_STR				="Medio-alto"
HIGHEST_STR					="Massimo"
DISABLED_STR				="Disattivata"
ENABLED_STR 				="Attivata"
MAXIMUM_POWER_SAVING_STR	="Massimo risparmio energetico"
NOISY_ENVIRONMENT_STR		="Ambienti rumorosi"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="Attivato da CTS a sé"
RTS_CTS_ENABLED_STR         ="Attivato RTS/CTS"
AUTO_STR                    ="Auto"
CHANNELWIDTH20ONLY          ="Soltanto 20 MHz"
CHANNELWIDTHAUTO            ="Auto"
WMM_DISABLED_STR            ="WMM disattivata"
WMM_ENABLED_STR             ="WMM attivata"


[Strings.0411] ; Japanese (Japan)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Windows Vista 32 ƒrƒbƒg—pƒCƒ“ƒeƒ‹(R) Wireless WiFi Link 3945ABG ƒAƒ_ƒvƒ^ ƒhƒ‰ƒCƒo"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Windows Vista 32 ƒrƒbƒg—pƒCƒ“ƒeƒ‹(R) Wireless WiFi Link 3945BG ƒAƒ_ƒvƒ^ ƒhƒ‰ƒCƒo"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Windows Vista 32 ƒrƒbƒg—pƒCƒ“ƒeƒ‹(R) Wireless WiFi Link 3965ABG ƒAƒ_ƒvƒ^ ƒhƒ‰ƒCƒo"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Windows Vista 32 ƒrƒbƒg—pƒCƒ“ƒeƒ‹(R) Wireless WiFi Link 3965BG ƒAƒ_ƒvƒ^ ƒhƒ‰ƒCƒo"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Windows Vista 32 ƒrƒbƒg—pƒCƒ“ƒeƒ‹(R) Wireless WiFi Link 4945AGN ƒAƒ_ƒvƒ^ ƒhƒ‰ƒCƒo"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Windows Vista 32 ƒrƒbƒg—pƒCƒ“ƒeƒ‹(R) Wireless WiFi Link 4945AG ƒAƒ_ƒvƒ^ ƒhƒ‰ƒCƒo"

NIC_Service_DispName_VISTA           ="Windows Vista 32 ƒrƒbƒg—pƒCƒ“ƒeƒ‹(R) Wireless WiFi Link ƒAƒ_ƒvƒ^ ƒhƒ‰ƒCƒo"

SOURCEDISK1                          ="ƒCƒ“ƒeƒ‹(R) Wireless WiFi Link 4965AGN ƒCƒ“ƒXƒg�[ƒ‹ ƒfƒBƒXƒN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="ƒAƒhƒzƒbƒN ƒ`ƒƒƒlƒ‹ 802.11b/g "
RECOMMENDED_CHANNEL52_STR 	="ƒAƒhƒzƒbƒN ƒ`ƒƒƒlƒ‹ 802.11a"
RECOMMENDED_BAND          	="ƒAƒhƒzƒbƒN ƒfƒtƒHƒ‹ƒg ƒ�ƒCƒ„ƒŒƒX ƒ‚�[ƒh"
IBSS_TX_POWER_STR           ="‘—�Mƒpƒ��["
ROAMING_AGGRESSIVENESS_STR	="ƒ��[ƒ~ƒ“ƒO‚Ì�Ï‹É�«"
ADHOC_POWER_MANAGEMENT_STR	="ƒAƒhƒzƒbƒN“dŒ¹ŠÇ—�"
ADHOC_QOS_MODE_STR          ="ƒAƒhƒzƒbƒN QoS ƒ‚�[ƒh"
MIXED_MODE_PROTECTION_STR   ="�¬�Ýƒ‚�[ƒh•ÛŒì"
THROUGHPUT_ENHANCEMENT_STR  ="ƒXƒ‹�[ƒvƒbƒg‚Ì‘�‰Á"
WIRELESS_MODE_STR           ="ƒ�ƒCƒ„ƒŒƒX ƒ‚�[ƒh"
CHANNELWIDTH                ="802.11n ƒ`ƒƒƒlƒ‹•�"
TGnMode                     ="802.11n ƒ‚�[ƒh"
FAT_CHANNEL_TOLERANT		="40Mhz ƒ`ƒƒƒlƒ‹•�”ñŒÝŠ·"

LOWEST_STR					="�Å’á"
MEDIUM_LOW_STR				="’†’á"
MEDIUM_STR					="’†"
MEDIUM_HIGH_STR				="’†�‚"
HIGHEST_STR					="�Å�‚"
DISABLED_STR				="–³Œø"
ENABLED_STR 				="—LŒø"
MAXIMUM_POWER_SAVING_STR	="�Å‘å�ß“d"
NOISY_ENVIRONMENT_STR		="ŽG‰¹‚Ì‘½‚¢ŠÂ‹«"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="ŒÂ•Ê CTS —LŒø"
RTS_CTS_ENABLED_STR         ="RTS/CTS —LŒø"
AUTO_STR                    ="Ž©“®"
CHANNELWIDTH20ONLY          ="20MHz �ê—p"
CHANNELWIDTHAUTO            ="Ž©“®"
WMM_DISABLED_STR            ="WMM –³Œø"
WMM_ENABLED_STR             ="WMM —LŒø"


[Strings.0412] ; Korean (Korea)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Windows Vista 32ºñÆ®¿ë ÀÎÅÚ(R) ¹«¼± WiFi ¸µÅ© 3945ABG ¾î´ðÅÍ µå¶óÀÌ¹ö"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Windows Vista 32ºñÆ®¿ë ÀÎÅÚ(R) ¹«¼± WiFi ¸µÅ© 3945BG ¾î´ðÅÍ µå¶óÀÌ¹ö"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Windows Vista 32ºñÆ®¿ë ÀÎÅÚ(R) ¹«¼± WiFi ¸µÅ© 3965ABG ¾î´ðÅÍ µå¶óÀÌ¹ö"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Windows Vista 32ºñÆ®¿ë ÀÎÅÚ(R) ¹«¼± WiFi ¸µÅ© 3965BG ¾î´ðÅÍ µå¶óÀÌ¹ö"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Windows Vista 32ºñÆ®¿ë ÀÎÅÚ(R) ¹«¼± WiFi ¸µÅ© 4965AGN ¾î´ðÅÍ µå¶óÀÌ¹ö"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Windows Vista 32ºñÆ®¿ë ÀÎÅÚ(R) ¹«¼± WiFi ¸µÅ© 4965AG ¾î´ðÅÍ µå¶óÀÌ¹ö"

NIC_Service_DispName_VISTA           ="Windows Vista 32ºñÆ®¿ë ÀÎÅÚ(R) ¹«¼± WiFi ¸µÅ© ¾î´ðÅÍ µå¶óÀÌ¹ö"

SOURCEDISK1                          ="ÀÎÅÚ(R) ¹«¼± WiFi ¸µÅ© 4965AGN ¼³Ä¡ µð½ºÅ©"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad Hoc Ã¤³Î 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	="Ad Hoc Ã¤³Î 802.11 a"
RECOMMENDED_BAND          	="Ad Hoc ±âº» ¹«¼± ¸ðµå"
IBSS_TX_POWER_STR           ="Àü¼Û Àü¿ø"
ROAMING_AGGRESSIVENESS_STR	="·Î¹Ö ¼öÁØ"
ADHOC_POWER_MANAGEMENT_STR	="Ad Hoc Àü¿ø °ü¸®"
ADHOC_QOS_MODE_STR          ="Ad Hoc QoS ¸ðµå"
MIXED_MODE_PROTECTION_STR   ="È¥ÇÕ ¸ðµå º¸È£"
THROUGHPUT_ENHANCEMENT_STR  ="Ã³¸®·® °³¼±"
WIRELESS_MODE_STR           ="¹«¼± ¸ðµå"
CHANNELWIDTH                ="802.11n Ã¤³Î Æø"
TGnMode                     ="802.11n ¸ðµå"
FAT_CHANNEL_TOLERANT		="°úºÎÇÏ Ã¤³Î ºñÁö¿ø"

LOWEST_STR					="ÃÖÇÏ"
MEDIUM_LOW_STR				="º¸Åë-³·À½"
MEDIUM_STR					="º¸Åë"
MEDIUM_HIGH_STR				="º¸Åë-³ôÀ½"
HIGHEST_STR					="ÃÖ°í"
DISABLED_STR				="ºñÈ°¼ºÈ­"
ENABLED_STR 				="»ç¿ëÇÔ"
MAXIMUM_POWER_SAVING_STR	="ÃÖ´ë ÀýÀü"
NOISY_ENVIRONMENT_STR		="ÀâÀ½ È¯°æ"
WMM_STR                     ="WMM"
CTS_TO_SELF_ENABLED_STR     ="ÀÚÃ¼ CTS »ç¿ë"
RTS_CTS_ENABLED_STR         ="RTS/CTS »ç¿ë"
AUTO_STR                    ="ÀÚµ¿"
CHANNELWIDTH20ONLY          ="20 MHz Àü¿ë"
CHANNELWIDTHAUTO            ="ÀÚµ¿"
WMM_DISABLED_STR            ="WMM ºñÈ°¼ºÈ­"
WMM_ENABLED_STR             ="WMM »ç¿ëÇÔ"


[Strings.0413] ; Dutch (Netherlands)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Stuurprogramma voor Intel(R) Wireless WiFi Link 3945ABG Adapter onder Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Stuurprogramma voor Intel(R) Wireless WiFi Link 3945BG Adapter onder Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Stuurprogramma voor Intel(R) Wireless WiFi Link 3965ABG Adapter onder Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Stuurprogramma voor Intel(R) Wireless WiFi Link 3965BG Adapter onder Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Stuurprogramma voor Intel(R) Wireless WiFi Link 4965AGN Adapter onder Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Stuurprogramma voor Intel(R) Wireless WiFi Link 4965AG Adapter onder Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="Stuurprogramma voor Intel(R) Wireless WiFi Link Adapter onder Windows Vista 32 Bit"

SOURCEDISK1                          ="Installatieschijf voor Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad-hockanaal 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Ad-hockanaal 802.11a"
RECOMMENDED_BAND          	="Ad-hoc standaard draadloze modus"
IBSS_TX_POWER_STR           ="Verzendenergie"
ROAMING_AGGRESSIVENESS_STR	="Agressiviteit bij zwerven"
ADHOC_POWER_MANAGEMENT_STR	="Energiebeheer ad-hocverbindingen"
ADHOC_QOS_MODE_STR          ="Ad-hoc QoS-modus"
MIXED_MODE_PROTECTION_STR   ="Beveiliging van gemengde modus"
THROUGHPUT_ENHANCEMENT_STR  ="Verbetering van  doorvoer"
WIRELESS_MODE_STR           ="Draadloze modus"
CHANNELWIDTH                ="802.11n-kanaalbreedte"
TGnMode                     ="802.11n-modus"
FAT_CHANNEL_TOLERANT		="Niet compatibel met 40-Mhz kanaal"

LOWEST_STR					="Laagste"
MEDIUM_LOW_STR				="Laag"
MEDIUM_STR					="Normaal"
MEDIUM_HIGH_STR				="Hoog"
HIGHEST_STR					="Hoogste"
DISABLED_STR				="Uitgeschakeld"
ENABLED_STR 				="Ingeschakeld"
MAXIMUM_POWER_SAVING_STR	="Maximale energiebesparing"
NOISY_ENVIRONMENT_STR		="Omgeving met ruis"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-naar-zelf ingeschakeld"
RTS_CTS_ENABLED_STR         ="RTS/CTS ingeschakeld"
AUTO_STR                    ="Auto"
CHANNELWIDTH20ONLY          ="Alleen 20 MHz"
CHANNELWIDTHAUTO            ="Auto"
WMM_DISABLED_STR            ="WMM uitgeschakeld"
WMM_ENABLED_STR             ="WMM ingeschakeld"


[Strings.0414] ; Norwegian (Bokmål) (Norway)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Intel(R) Wireless WiFi Link 3945ABG  kortdriver for Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Intel(R) Wireless WiFi Link 3945BG kortdriver for Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Intel(R) Wireless WiFi Link 3965ABG kortdriver for Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Intel(R) Wireless WiFi Link 3965BG kortdriver for Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Intel(R) Wireless WiFi Link 4965AGN kortdriver for Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Intel(R) Wireless WiFi Link 4965AG kortdriver for Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="Intel(R) Wireless WiFi Link kortdriver for Windows Vista 32 Bit"

SOURCEDISK1                          ="Intel(R) Wireless WiFi Link 4965AGN Installasjonsdiskett"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad Hoc-kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Ad Hoc-kanal 802.11a"
RECOMMENDED_BAND          	="Ad hoc standard trådløsmodus"
IBSS_TX_POWER_STR           ="Overføringsstrøm"
ROAMING_AGGRESSIVENESS_STR	="Streifingsaggresjon"
ADHOC_POWER_MANAGEMENT_STR	="Ad Hoc strømstyring"
ADHOC_QOS_MODE_STR          ="Ad Hoc QoS modus"
MIXED_MODE_PROTECTION_STR   ="Blandet modus-beskyttelse"
THROUGHPUT_ENHANCEMENT_STR  ="Gjennomstrømningsutvidelse"
WIRELESS_MODE_STR           ="Trådløsmodus"
CHANNELWIDTH                ="802.11n Kanalbredde"
TGnMode                     ="802.11n-modus"
FAT_CHANNEL_TOLERANT		="Intolerant for kanal"

LOWEST_STR					="Laveste"
MEDIUM_LOW_STR				="Middels-lav"
MEDIUM_STR					="Middels"
MEDIUM_HIGH_STR				="Middels-høy"
HIGHEST_STR					="Høyeste"
DISABLED_STR				="Deaktivert"
ENABLED_STR 				="Aktivert"
MAXIMUM_POWER_SAVING_STR	="Maksimal strømsparing"
NOISY_ENVIRONMENT_STR		="Støyende miljø"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-til-selv aktivert"
RTS_CTS_ENABLED_STR         ="RTS/CTS-aktivert"
AUTO_STR                    ="Automatisk"
CHANNELWIDTH20ONLY          ="Kun 20 MHz "
CHANNELWIDTHAUTO            ="Automatisk"
WMM_DISABLED_STR            ="WMM deaktivert"
WMM_ENABLED_STR             ="WMM aktivert"


[Strings.0415] ; Polish (Poland)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Sterownik karty Intel(R) Wireless WiFi Link 3945ABG dla systemu Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Sterownik karty Intel(R) Wireless WiFi Link 3945BG dla systemu Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Sterownik karty Intel(R) Wireless WiFi Link 3965ABG dla systemu Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Sterownik karty Intel(R) Wireless WiFi Link 3965BG dla systemu Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Sterownik karty Intel(R) Wireless WiFi Link 4965AGN dla systemu Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Sterownik karty Intel(R) Wireless WiFi Link 4965AG dla systemu Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="Sterownik karty Intel(R) Wireless WiFi Link dla systemu Windows Vista 32 Bit"

SOURCEDISK1                          ="Dysk instalacyjny Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Kana³ ad hoc 802.11 b/g"
RECOMMENDED_CHANNEL52_STR 	="Kana³ ad hoc 802.11 a"
RECOMMENDED_BAND          	="Domyœlny tryb sieci bezprzewodowej ad hoc"
IBSS_TX_POWER_STR           ="Moc transmisji"
ROAMING_AGGRESSIVENESS_STR	="Agresywnoœæ mobilnoœci"
ADHOC_POWER_MANAGEMENT_STR	="Zarz¹dzanie energi¹ w sieci ad hoc"
ADHOC_QOS_MODE_STR          ="Tryb ad hoc QoS"
MIXED_MODE_PROTECTION_STR   ="Ochrona trybu mieszanego"
THROUGHPUT_ENHANCEMENT_STR  ="Rozszerzenie przep³ywnoœci"
WIRELESS_MODE_STR           ="Tryb bezprzewodowy"
CHANNELWIDTH                ="Szerokoœæ kana³u 802.11n"
TGnMode                     ="Tryb 802.11n"
FAT_CHANNEL_TOLERANT		="Brak tolerancji dla kana³u 40 MHz"

LOWEST_STR					="Najni¿sza"
MEDIUM_LOW_STR				="Œrednio-niska"
MEDIUM_STR					="Œrednia"
MEDIUM_HIGH_STR				="Œrednio-wysoka"
HIGHEST_STR					="Najwy¿sza"
DISABLED_STR				="Wy³¹czone"
ENABLED_STR 				="W³¹czono"
MAXIMUM_POWER_SAVING_STR	="Maksymalna oszczêdnoœæ energii"
NOISY_ENVIRONMENT_STR		="Œrodowisko z zak³óceniami"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="W³¹czony sygna³ zwrotny CTS"
RTS_CTS_ENABLED_STR         ="W³¹czony sygna³ RTS/CTS"
AUTO_STR                    ="Automatyczny"
CHANNELWIDTH20ONLY          ="Tylko 20 MHz"
CHANNELWIDTHAUTO            ="Automatyczny"
WMM_DISABLED_STR            ="Wy³¹czone WMM"
WMM_ENABLED_STR             ="W³¹czono WMM"


[Strings.0416] ; Portuguese (Brazil)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Driver do Adaptador Intel(R) Wireless WiFi Link 3945ABG para Windows Vista 32 bits"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Driver do Adaptador Intel(R) Wireless WiFi Link 3945BG para Windows Vista 32 bits"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Driver do Adaptador Intel(R) Wireless WiFi Link 3965ABG para Windows Vista 32 bits"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Driver do Adaptador Intel(R) Wireless WiFi Link 3965BG para Windows Vista 32 bits"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Driver do Adaptador Intel(R) Wireless WiFi Link 4965AGN para Windows Vista 32 bits"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Driver do Adaptador Intel(R) Wireless WiFi Link 4965AG para Windows Vista 32 bits"

NIC_Service_DispName_VISTA           ="Driver do Adaptador Intel(R) Wireless WiFi Link para Windows Vista 32 bits"

SOURCEDISK1                          ="Disco da instalação do Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canal ad-hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Canal ad-hoc 802.11a"
RECOMMENDED_BAND          	="Modo sem fio padrão ad-hoc"
IBSS_TX_POWER_STR           ="Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR	="Agressividade de roaming"
ADHOC_POWER_MANAGEMENT_STR	="Gerenciamento de energia ad-hoc"
ADHOC_QOS_MODE_STR          ="Modo QoS Ad-hoc"
MIXED_MODE_PROTECTION_STR   ="Proteção de modo misto"
THROUGHPUT_ENHANCEMENT_STR  ="Aumento da throughput"
WIRELESS_MODE_STR           ="Modo sem fio"
CHANNELWIDTH                ="Largura de canal 802.11n"
TGnMode                     ="Modo 802.11n"
FAT_CHANNEL_TOLERANT		="Sem tolerância a canal gordo"

LOWEST_STR					="Mais baixo"
MEDIUM_LOW_STR				="Média a baixa"
MEDIUM_STR					="Média"
MEDIUM_HIGH_STR				="Média a alta"
HIGHEST_STR					="Mais alto"
DISABLED_STR				="Desabilitado"
ENABLED_STR 				="Habilitado"
MAXIMUM_POWER_SAVING_STR	="Economia máx. de energia"
NOISY_ENVIRONMENT_STR		="Ambiente ruidoso"
WMM_STR                     ="WMM"
CTS_TO_SELF_ENABLED_STR     ="CTS em auto-ativação ativado"
RTS_CTS_ENABLED_STR         ="RTS/CTS ativado"
AUTO_STR                    ="Auto"
CHANNELWIDTH20ONLY          ="20 MHz apenas"
CHANNELWIDTHAUTO            ="Auto"
WMM_DISABLED_STR            ="WMM desabilitado"
WMM_ENABLED_STR             ="WMM habilitado"


[Strings.0816] ; Portuguese (Portugal)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Controlador do Adaptador da ligação sem fios Intel(R) 3945ABG para Windows Vista 32 Bits"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Controlador do Adaptador da ligação sem fios Intel(R) 3945BG para Windows Vista 32 Bits"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Controlador do Adaptador da ligação WiFi sem fios Intel(R) 3965ABG para Windows Vista 32 Bits"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Controlador do Adaptador da ligação sem fios Intel(R) 3965BG para Windows Vista 32 Bits"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Controlador do Adaptador da ligação WiFi sem fios Intel(R) 4965AGN para Windows Vista 32 Bits"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Controlador do Adaptador da ligação WiFi sem fios Intel(R) 4965AG para Windows Vista 32 Bits"

NIC_Service_DispName_VISTA           ="Controlador do Adaptador da ligação WiFi sem fios Intel(R) para Windows Vista 32 Bits"

SOURCEDISK1                          ="Disco de instalação da Ligação WiFi sem fios Intel(R) 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canal ad hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Canal ad hoc 802.11 a"
RECOMMENDED_BAND          	="Modo ad hoc sem fios predefinido"
IBSS_TX_POWER_STR           ="Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR	="Agressividade do roaming"
ADHOC_POWER_MANAGEMENT_STR	="Gestão de energia ad hoc"
ADHOC_QOS_MODE_STR          ="Modo Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   ="Protecção do modo misto"
THROUGHPUT_ENHANCEMENT_STR  ="Melhoria da produtividade"
WIRELESS_MODE_STR           ="Modo sem fios"
CHANNELWIDTH                ="Largura do canal 802.11n"
TGnMode                     ="Modo 802.11n"
FAT_CHANNEL_TOLERANT		="Canal de grandes volumes incompatível"

LOWEST_STR					="Menor"
MEDIUM_LOW_STR				="Média-baixa"
MEDIUM_STR					="Média"
MEDIUM_HIGH_STR				="Média-Elevada"
HIGHEST_STR					="Maior"
DISABLED_STR				="Desactivado"
ENABLED_STR 				="Activado"
MAXIMUM_POWER_SAVING_STR	="Máxima poupança de energia"
NOISY_ENVIRONMENT_STR		="Ambiente ruidoso"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-para-activação-automática"
RTS_CTS_ENABLED_STR         ="RTS/CTS Activado"
AUTO_STR                    ="Auto"
CHANNELWIDTH20ONLY          ="Apenas 20 MHz"
CHANNELWIDTHAUTO            ="Auto"
WMM_DISABLED_STR            ="WMM desactivado"
WMM_ENABLED_STR             ="WMM activado"


[Strings.0419] ; Russian (Russia)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Äðàéâåð àäàïòåðà Intel(R) Wireless WiFi Link 3945ABG äëÿ Windows Vista 32 Bit"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Äðàéâåð àäàïòåðà Intel(R) Wireless WiFi Link 3945BG äëÿ Windows Vista 32 Bit"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Äðàéâåð àäàïòåðà Intel(R) Wireless WiFi Link 3965ABG äëÿ Windows Vista 32 Bit"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Äðàéâåð àäàïòåðà Intel(R) Wireless WiFi Link 3965BG äëÿ Windows Vista 32 Bit"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Äðàéâåð àäàïòåðà Intel(R) Wireless WiFi Link 4965AGN äëÿ Windows Vista 32 Bit"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Äðàéâåð àäàïòåðà Intel(R) Wireless WiFi Link 4965AG äëÿ Windows Vista 32 Bit"

NIC_Service_DispName_VISTA           ="Äðàéâåð àäàïòåðà Intel(R) Wireless WiFi Link äëÿ Windows Vista 32 Bit"

SOURCEDISK1                          ="Óñòàíîâî÷íûé äèñê àäàïòåðà Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Êàíàë Ad Hoc 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Êàíàë Ad Hoc 802.11a"
RECOMMENDED_BAND          	="Ðåæèì áåñïðîâîäíîé ñåòè Ad Hoc ïî óìîë÷àíèþ"
IBSS_TX_POWER_STR           ="Ìîùíîñòü ïåðåäà÷è"
ROAMING_AGGRESSIVENESS_STR	="Àãðåññèâíîñòü ðîóìèíãà"
ADHOC_POWER_MANAGEMENT_STR	="Óïðàâëåíèå ìîùíîñòüþ ïåðåäà÷è Ad Hoc"
ADHOC_QOS_MODE_STR          ="Ðåæèì Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   ="Çàùèòà â ñìåøàííîì ðåæèìå"
THROUGHPUT_ENHANCEMENT_STR  ="Ïîâûøåííàÿ ïðîïóñêíàÿ ñïîñîáíîñòü Intel (Intel Throughput Enhancement)"
WIRELESS_MODE_STR           ="Ðåæèì áåñïðîâîäíîé ñåòè"
CHANNELWIDTH                ="Øèðèíà êàíàëà 802.11n"
TGnMode                     ="Ðåæèì 802.11n"
FAT_CHANNEL_TOLERANT		="Íåñîâìåñòèìîñòü ñ êàíàëîì 40 ÌÃö"

LOWEST_STR					="Ìèí"
MEDIUM_LOW_STR				="Ñðåäí-ìèí"
MEDIUM_STR					="Ñðåäí"
MEDIUM_HIGH_STR				="Ñðåäí-ìàêñ"
HIGHEST_STR					="Ìàêñ"
DISABLED_STR				="Âûêëþ÷åíî"
ENABLED_STR 				="Âêëþ÷åíî"
MAXIMUM_POWER_SAVING_STR	="Ìàêñèìàëüíàÿ ýêîíîìèÿ ýíåðãèè"
NOISY_ENVIRONMENT_STR		="Óñëîâèÿ ñ ïîìåõàìè"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-to-self âêëþ÷åíî"
RTS_CTS_ENABLED_STR         ="RTS/CTS âêëþ÷åíî"
AUTO_STR                    ="Àâòî"
CHANNELWIDTH20ONLY          ="Òîëüêî 20 ÌÃö"
CHANNELWIDTHAUTO            ="Àâòî"
WMM_DISABLED_STR            ="WMM Âûêëþ÷åíî"
WMM_ENABLED_STR             ="WMM Âêëþ÷åíî"


[Strings.041D] ; Swedish (Sweden)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Kortdrivrutin för Windows Vista 32-bitars för Intel(R) Wireless WiFi Link 3945ABG"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Kortdrivrutin för Windows Vista 32-bitars för Intel(R) Wireless WiFi Link 3945BG"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Kortdrivrutin för Windows Vista 32-bitars för Intel(R) Wireless WiFi Link 3965ABG"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Kortdrivrutin för Windows Vista 32-bitars för Intel(R) Wireless WiFi Link 3965BG"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Kortdrivrutin för Windows Vista 32-bitars för Intel(R) Wireless WiFi Link 4965AGN"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Kortdrivrutin för Windows Vista 32-bitars för Intel(R) Wireless WiFi Link 4965AG"

NIC_Service_DispName_VISTA           ="Kortdrivrutin för Windows Vista 32-bitars för Intel(R) Wireless WiFi Link"

SOURCEDISK1                          ="Installationsdisk för Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad hoc-kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Ad hoc-kanal 802.11a"
RECOMMENDED_BAND          	="Ad hoc Standard trådlöst läge"
IBSS_TX_POWER_STR           ="Överföringsenergi"
ROAMING_AGGRESSIVENESS_STR	="Roaming-aggressivitet"
ADHOC_POWER_MANAGEMENT_STR	="Energisparfunktioner för ad hoc"
ADHOC_QOS_MODE_STR          ="Ad Hoc QoS-läge"
MIXED_MODE_PROTECTION_STR   ="Skydd för blandat läge"
THROUGHPUT_ENHANCEMENT_STR  ="Genomflödesförbättring"
WIRELESS_MODE_STR           ="Trådlöst läge"
CHANNELWIDTH                ="802.11n-kanalbredd"
TGnMode                     ="802.11n-läge"
FAT_CHANNEL_TOLERANT		="Inkompatibel med 40 MHz-kanal"

LOWEST_STR					="Lägsta"
MEDIUM_LOW_STR				="Medel-låg"
MEDIUM_STR					="Medel"
MEDIUM_HIGH_STR				="Medel-hög"
HIGHEST_STR					="Högsta"
DISABLED_STR				="Inaktiverad"
ENABLED_STR 				="Aktiverad"
MAXIMUM_POWER_SAVING_STR	="Max. energibesparing"
NOISY_ENVIRONMENT_STR		="Miljö med störningar"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-till-själv aktiverat"
RTS_CTS_ENABLED_STR         ="RTS/CTS aktiverat"
AUTO_STR                    ="Auto"
CHANNELWIDTH20ONLY          ="Endast 20 MHz"
CHANNELWIDTHAUTO            ="Auto"
WMM_DISABLED_STR            ="WMM inaktiverad"
WMM_ENABLED_STR             ="WMM aktiverad"


[Strings.041E] ; Thai (Thailand)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Wireless WiFi Link 3945ABG ÊÓËÃÑº Windows Vista 32 ºÔµ"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Wireless WiFi Link 3945BG ÊÓËÃÑº Windows Vista 32 ºÔµ"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Wireless WiFi Link 3965ABG ÊÓËÃÑº Windows Vista 32 ºÔµ"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Wireless WiFi Link 3965BG ÊÓËÃÑº Windows Vista 32 ºÔµ"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Wireless WiFi Link 4965AGN ÊÓËÃÑº Windows Vista 32 ºÔµ"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Wireless WiFi Link 4965AG ÊÓËÃÑº Windows Vista 32 ºÔµ"

NIC_Service_DispName_VISTA           ="ä´ÃàÇÍÃìÍá´ç»àµÍÃì Intel(R) Wireless WiFi Link ÊÓËÃÑº Windows Vista 32 ºÔµ"

SOURCEDISK1                          ="´ÔÊ¡ìµÔ´µÑé§ Intel(R) Wireless WiFi Link 4965AGN"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="áª¹à¹Åà©¾ÒÐ¡Ô¨ 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="áª¹à¹Åà©¾ÒÐ¡Ô¨ 802.11a"
RECOMMENDED_BAND          	="âËÁ´äÃéÊÒÂàÃÔèÁµé¹áººà©¾ÒÐ¡Ô¨"
IBSS_TX_POWER_STR           ="¡ÒÃÊè§¼èÒ¹¾ÅÑ§§Ò¹"
ROAMING_AGGRESSIVENESS_STR	="¤ÇÒÁáÃ§ã¹¡ÒÃãªé§Ò¹¢éÒÁà¢µ"
ADHOC_POWER_MANAGEMENT_STR	="¡ÒÃ¨Ñ´¡ÒÃ¾ÅÑ§§Ò¹à©¾ÒÐ¡Ô¨"
ADHOC_QOS_MODE_STR          ="âËÁ´ QoS à©¾ÒÐ¡Ô¨"
MIXED_MODE_PROTECTION_STR   ="¡ÒÃ»éÍ§¡Ñ¹âËÁ´¼ÊÁ"
THROUGHPUT_ENHANCEMENT_STR  ="¡ÒÃà¾ÔèÁ»ÃÐÊÔ·¸ÔÀÒ¾ÍÑµÃÒÃÑºÊè§"
WIRELESS_MODE_STR           ="âËÁ´äÃéÊÒÂ"
CHANNELWIDTH                ="¢¹Ò´áª¹à¹Å 802.11n"
TGnMode                     ="âËÁ´ 802.11n"
FAT_CHANNEL_TOLERANT		="äÁèÊÒÁÒÃ¶ãªéáª¹á¹Å¢¹Ò´ãË­è"

LOWEST_STR					="µèÓÊØ´"
MEDIUM_LOW_STR				="»Ò¹¡ÅÒ§-µèÓ"
MEDIUM_STR					="»Ò¹¡ÅÒ§"
MEDIUM_HIGH_STR				="»Ò¹¡ÅÒ§-ÊÙ§"
HIGHEST_STR					="ÊÙ§ÊØ´"
DISABLED_STR				="Â¡àÅÔ¡ãªé§Ò¹"
ENABLED_STR 				="ãªé§Ò¹áÅéÇ"
MAXIMUM_POWER_SAVING_STR	="¡ÒÃ»ÃÐËÂÑ´¾ÅÑ§§Ò¹ÊÙ§ÊØ´"
NOISY_ENVIRONMENT_STR		="ÊÀÒ¾áÇ´ÅéÍÁ·ÕèÁÕàÊÕÂ§´Ñ§"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="ãªé§Ò¹ CTS-to-self áÅéÇ"
RTS_CTS_ENABLED_STR         ="ãªé§Ò¹ RTS/CTS"
AUTO_STR                    ="ÍÑµâ¹ÁÑµÔ"
CHANNELWIDTH20ONLY          ="20 MHz à·èÒ¹Ñé¹"
CHANNELWIDTHAUTO            ="ÍÑµâ¹ÁÑµÔ"
WMM_DISABLED_STR            ="Â¡àÅÔ¡ãªé§Ò¹ WMM"
WMM_ENABLED_STR             ="ãªé§Ò¹áÅéÇ WMM"


[Strings.041F] ; Turkish (Turkey)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="Windows Vista 32 Bit için Intel(R) Wireless WiFi Link 3945ABG Baðdaþtýrýcý Sürücüsü"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="Windows Vista 32 Bit için Intel(R) Wireless WiFi Link 3945BG Baðdaþtýrýcý Sürücüsü"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="Windows Vista 32 Bit için Intel(R) Wireless WiFi Link 3965ABG Baðdaþtýrýcý Sürücüsü"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="Windows Vista 32 Bit için Intel(R) Wireless WiFi Link 3965BG Baðdaþtýrýcý Sürücüsü"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="Windows Vista 32 Bit için Intel(R) Wireless WiFi Link 4965AGN Baðdaþtýrýcý Sürücüsü"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="Windows Vista 32 Bit için Intel(R) Wireless WiFi Link 4965AG Baðdaþtýrýcý Sürücüsü"

NIC_Service_DispName_VISTA           ="Windows Vista 32 Bit için Intel(R) Wireless WiFi Link Baðdaþtýrýcý Sürücüsü"

SOURCEDISK1                          ="Intel(R) Wireless WiFi Link 4965AGN Yükleme Diski"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Aygýttan Aygýta Kanal 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="Aygýttan Aygýta Kanal 802.11a"
RECOMMENDED_BAND          	="Aygýttan Aygýta Varsayýlan Kablosuz Baðlantý Modu"
IBSS_TX_POWER_STR           ="Yayýn gücü"
ROAMING_AGGRESSIVENESS_STR	="Gezinme Zorlamasý"
ADHOC_POWER_MANAGEMENT_STR	="Aygýttan Aygýta Güç Yönetimi"
ADHOC_QOS_MODE_STR          ="Aygýttan Aygýta QoS Modu"
MIXED_MODE_PROTECTION_STR   ="Karýþýk Mod Korumasý"
THROUGHPUT_ENHANCEMENT_STR  ="Veri Aktarým Geliþtirici"
WIRELESS_MODE_STR           ="Kablosuz Kip"
CHANNELWIDTH                ="802.11n Kanal Geniþliði"
TGnMode                     ="802.11n Modu"
FAT_CHANNEL_TOLERANT		="Geniþ Kanal için Uyumsuz"

LOWEST_STR					="En düþük"
MEDIUM_LOW_STR				="Düþük"
MEDIUM_STR					="Orta"
MEDIUM_HIGH_STR				="Yüksek"
HIGHEST_STR					="En yüksek"
DISABLED_STR				="Devre dýþý"
ENABLED_STR 				="Etkin"
MAXIMUM_POWER_SAVING_STR	="Azami Güç Tasarrufu"
NOISY_ENVIRONMENT_STR		="Gürültülü Ortam"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="CTS-to-self etkin"
RTS_CTS_ENABLED_STR         ="RTS/CTS etkin"
AUTO_STR                    ="Otomatik"
CHANNELWIDTH20ONLY          ="Yalnýzca 20 MHz"
CHANNELWIDTHAUTO            ="Otomatik"
WMM_DISABLED_STR            ="WMM devre dýþý"
WMM_ENABLED_STR             ="WMM etkin"


[Strings.0C04] ; Chinese (Hong Kong)
PROVIDER_NAME                        ="Intel"
COMPANY_NAME                         ="Intel Corporation"

NIC_MPCIEX_3945ABG                 ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_3945BG                  ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_3965ABG                 ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_3965BG                  ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_4965AGN                 ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_4965AG                  ="Intel(R) Wireless WiFi Link 4965AG"

NIC_MPCIEX_AdapterModel_3945ABG    ="Intel(R) PRO/Wireless 3945ABG Network Connection"
NIC_MPCIEX_AdapterModel_3945BG     ="Intel(R) PRO/Wireless 3945BG Network Connection"
NIC_MPCIEX_AdapterModel_3965ABG    ="Intel(R) PRO/Wireless 3965ABG Network Connection"
NIC_MPCIEX_AdapterModel_3965BG     ="Intel(R) PRO/Wireless 3965BG Network Connection"
NIC_MPCIEX_AdapterModel_4965AGN    ="Intel(R) Wireless WiFi Link 4965AGN"
NIC_MPCIEX_AdapterModel_4965AG     ="Intel(R) Wireless WiFi Link 4965AG"
NIC_DriverDesc_3945ABG               ="Intel(R) Wireless WiFi Link 3945ABG Driver"
NIC_Service_DispName_3945ABG         ="Intel(R) Wireless WiFi Link 3945ABG Adapter Driver"
NIC_Service_DispName_3945ABG_VISTA   ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 3945ABG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_3945BG                ="Intel(R) Wireless WiFi Link 3945BG Driver"
NIC_Service_DispName_3945BG_VISTA    ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 3945BG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_3965ABG               ="Intel(R) Wireless WiFi Link 3965ABG Driver"
NIC_Service_DispName_3965ABG_VISTA   ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 3965ABG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_3965BG                ="Intel(R) Wireless WiFi Link 3965BG Driver"
NIC_Service_DispName_3965BG_VISTA    ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 3965BG ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_4965AGN               ="Intel(R) Wireless WiFi Link 4965AGN Driver"
NIC_Service_DispName_4965AGN_VISTA   ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 4965AGN ¤¶­±¥dÅX°Êµ{¦¡"
NIC_DriverDesc_4965AG          		 ="Intel(R) Wireless WiFi Link 4965AG Driver"
NIC_Service_DispName_4965AG_VISTA    ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link 4965AG ¤¶­±¥dÅX°Êµ{¦¡"

NIC_Service_DispName_VISTA           ="¥Î©ó Windows Vista 32 Bit ªº Intel(R) Wireless WiFi Link ¤¶­±¥dÅX°Êµ{¦¡"

SOURCEDISK1                          ="Intel(R) Wireless WiFi Link 4965AGN ¦w¸ËºÏºÐ"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="ÂI¹ïÂI (ad hoc) ³q¹D 802.11b/g"
RECOMMENDED_CHANNEL52_STR 	="ÂI¹ïÂI (ad hoc) ³q¹D 802.11a"
RECOMMENDED_BAND          	="ÂI¹ïÂI (ad hoc) ¹w³]µL½u¼Ò¦¡"
IBSS_TX_POWER_STR           ="¶Ç¿é¹q·½"
ROAMING_AGGRESSIVENESS_STR	="º©¹C¿n·¥«×"
ADHOC_POWER_MANAGEMENT_STR	="ÂI¹ïÂI (ad hoc) ¹q·½ºÞ²z"
ADHOC_QOS_MODE_STR          ="ÂI¹ïÂI (ad hoc) QoS ¼Ò¦¡"
MIXED_MODE_PROTECTION_STR   ="²V¦X¼Ò¦¡«OÅ@"
THROUGHPUT_ENHANCEMENT_STR  ="¿é°e¶q¼W±j¥\¯à"
WIRELESS_MODE_STR           ="µL½u¼Ò¦¡"
CHANNELWIDTH                ="802.11n ³q¹D¼e«×"
TGnMode                     ="802.11n ¼Ò¦¡"
FAT_CHANNEL_TOLERANT		="¤£®e¤j¶q³q¹D"

LOWEST_STR					="³Ì§C"
MEDIUM_LOW_STR				="¤¤§C"
MEDIUM_STR					="¤¤"
MEDIUM_HIGH_STR				="¤¤°ª"
HIGHEST_STR					="³Ì°ª"
DISABLED_STR				="°±¥Î"
ENABLED_STR 				="±Ò¥Î"
MAXIMUM_POWER_SAVING_STR	="³Ì¬Ù¹q"
NOISY_ENVIRONMENT_STR		="¾¸­µÀô¹Ò"
WMM_STR                     ="WMM "
CTS_TO_SELF_ENABLED_STR     ="±Ò¥Î CTS-to-self"
RTS_CTS_ENABLED_STR         ="±Ò¥Î RTS/CTS"
AUTO_STR                    ="¦Û°Ê"
CHANNELWIDTH20ONLY          ="¶È­­©ó 20 MHz"
CHANNELWIDTHAUTO            ="¦Û°Ê"
WMM_DISABLED_STR            ="WMM °±¥Î"
WMM_ENABLED_STR             ="WMM ±Ò¥Î"

