; Copyright (c) 2007 Texas Instruments
; TI FlashMedia Installation file for Win2000/XP

[Version]
Signature=$CHICAGO$
Class=MTD
ClassGuid={4d36e970-e325-11ce-bfc1-08002be10318}
Provider=%MFGNAME%
CataLogFile=ti21sony.cat
DriverVer=04/23/2007,2.0.0.18

[Manufacturer]
%MFGNAME%=DeviceList,NTamd64

[ControlFlags]
ExcludeFromSelect=*

[DestinationDirs]
DefaultDestDir = 11
DriverCopyFiles = 12

[SourceDisksFiles]
ti21sony.sys=1

[SourceDisksNames]
1=%INSTDISK%,,,

[DeviceList]
%DESCRIPTION%=FMDriverInstall,PCI\VEN_104C&DEV_8033  ; xx21
%DESCRIPTION_xx12%=FMDriverInstall,PCI\VEN_104C&DEV_803B  ; xx12

[DeviceList.NTamd64]
%DESCRIPTION%=FMDriverInstall,PCI\VEN_104C&DEV_8033  ; xx21
%DESCRIPTION_xx12%=FMDriverInstall,PCI\VEN_104C&DEV_803B  ; xx12

;------------------------------------------------------------------------------
;  Windows 2000/XP Sections
;------------------------------------------------------------------------------

[FMDriverInstall.NT]
AddReg   = FMDriverInstall.AddReg
CopyFiles=DriverCopyFiles

[FMDriverInstall.NTamd64]
AddReg   = FMDriverInstall.AddReg
CopyFiles=DriverCopyFiles

[DriverCopyFiles]
ti21sony.sys,,,2

[FMDriverInstall.NT.Services]
AddService=ti21sony,2,DriverService

[FMDriverInstall.NTamd64.Services]
AddService=ti21sony,2,DriverService

[DriverService]
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%10%\system32\drivers\ti21sony.sys


[FMDriverInstall.nt.hw]
AddReg=FMDriverHwAddReg

[FMDriverInstall.NTamd64.hw]
AddReg=FMDriverHwAddReg

[FMDriverHwAddReg]
HKLM,"SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\FlashMedia#MemoryStickDevice2","NoSoftEject",0x00010001,0x00000001
HKLM,"SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\FlashMedia#MemoryStickDevice0","NoSoftEject",0x00010001,0x00000001
HKLM,"SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\FlashMedia#SDDevice3","NoSoftEject",0x00010001,0x00000001
HKLM,"SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\FlashMedia#SDDevice1","NoSoftEject",0x00010001,0x00000001

[FMDriverInstall.AddReg]
; DWORD will go to software branch
;HKR,,SecurityEnable,0x00010001,1
; Write to specified registry path
HKLM,System\CurrentControlSet\Services\ti21sony\Parameters,ShowRemoveDiagBox, 0x10001,0

; 0 - default. Switch to SDIO
; 1 - Switch to SD or SDIO
; 2 - switch to MMC or SDIO
; 3 - switch to SD or MMC or SDIO
HKLM,System\CurrentControlSet\Services\ti21sony\Parameters,SDSwitch, 0x10001,0

; 1 - SmartMedia enable
; 0 - SmartMedia disable
HKLM,System\CurrentControlSet\Services\ti21sony\Parameters,SMEnable, 0x10001,1

; 1 - MS Parallel Mode dedicated socket enable
; 0 - MS Parallel Mode dedicated socket disable
HKLM,System\CurrentControlSet\Services\ti21sony\Parameters,MSPEnable, 0x10001,1

; Enable Dbg Message by default is disable or 0
; 1 - enable debug message in release build
HKLM,System\CurrentControlSet\Services\ti21sony\Parameters,DbgMsgEnable, 0x10001,0

; 0 - Disable SM CIS check
; 1 - Enable Sm CIS check, set to 1 by default
HKLM,System\CurrentControlSet\Services\ti21sony\Parameters,SMCISEnable, 0x10001,1

; For xx12 device, use one LED as default: 1 - two LED used, 0 - one LED used
HKLM,System\CurrentControlSet\Services\ti21sony\Parameters,UseOneLED, 0x10001,0

; Which MFUNC to use for LED; default is MFUNC 5
; 0x02 - MFUNC 1
; 0x04 - MFUNC 2
; 0x08 - MFUNC 3
; 0x10 - MFUNC 4
; 0x20 - MFUNC 5
; 0x40 - MFUNC 6
HKLM,System\CurrentControlSet\Services\ti21sony\Parameters,UseMFUNC, 0x10001,0x20

; Support MemoryStick slot only: Disable is default as 0, 1 - enable.
;HKLM,System\CurrentControlSet\Services\ti21sony\Parameters,MSSlotOnly, 0x10001,0

; this flag is for W2K QFE "Delayed write fail"
HKLM,System\CurrentControlSet\Services\Disk,HotPlugAlwaysEnable, 0x00010000,"MemoryStick2","SD3"

;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------

[Strings]
MFGNAME="Texas Instruments Inc"
INSTDISK="TI Installation Disc"
DESCRIPTION="Texas Instruments PCI7411 Integrated FlashMedia Controller"
DESCRIPTION_xx12="Texas Instruments PCIxx12 Integrated FlashMedia Controller"
