;**************************************************************************
; Copyright (c) 2001, LAN-Express Wireless LAN Card for Windows 2K/XP
;**************************************************************************

[Version]
 DriverVer = 07/15/2002, 2.0.2
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
 CatalogFile         = NetWlan.cat
 ;MillenniumPreferred = .ME

; ---------------------------------------------------------------------------------

[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = "LAN-Express"
 VER_VENDOR_NAME_STR    = "LAN-Express"

 PRISM_SERVICE_DISPLAY  = "IEEE 802.11 Wireless NIC Driver"
 INSTALL_DISK_STR       = "LAN-Express IEEE 802.11 PCMCIA/PCI Driver Disk"

 ADHOC_DEMO_STR         = "Adhoc Demo Mode"
 SHORT_PREAM_STR        = "Preamble Mode"
 RTSTHRESH_STR          = "RTS Threshold"
 FRAGTHRESH_STR         = "Fragmentation Threshold"
 AUTHENT_TYPE_STR       = "Authentication Algorithm"
 LISTENINTERVAL_STR     = "Listen Interval"
 POWER_SAVE_STR         = "Power Save Mode"
 POWER_LEVEL_STR        = "Power Save Level"
 LOAD_FIRMWARE_STR      = "Firmware Download"

 PCMCIA_DESC_STR        = "LAN-Express IEEE 802.11 PCMCIA Card"
 PCI_DESC_STR           = "LAN-Express IEEE 802.11 PCI Adapter"

; ---------------------------------------------------------------------------------
[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = PCI\VEN_1260&DEV_3873&SUBSYS_02011468

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
%PCI_DESC_STR%     = PRISM_PCI,        PCI\VEN_1260&DEV_3873&SUBSYS_02011468
 
;==========================================
[PRISM_PCI]       ; Win9x
 AddReg         = PRISM_PCI.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy

[PRISM_PCI.NT]    ; Win2k
 AddReg         = PRISM_PCI.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCI.NT.Services]
 AddService     = PRISM, 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCI.reg]
 HKR,Ndi        ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS__PRISM_PCI_SUBSYSID_"
 HKR,           ,PlatformId,0,"32804"
 HKR,           ,VendorDesc,0,%PCI_DESC_STR%
 HKR,           ,LoadFirmware,0,"1"
 ;HKR, NDI\params\LoadFirmware,,0,1


;###############################################################################

[PRISM_DRIVER.Service]
 DisplayName    = %PRISM_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\EXPRESS.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_PCI.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM"
 HKR,NDI                ,CardType               ,0      ,"PCI"
 HKR,                   ,BusType                ,0      ,"5"
 HKR,                   ,DeviceVxDs             ,0      ,"EXPRESS.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,"01","00","00","00"
 HKR,                   ,IOBaseAddress          ,1      ,"02","00","00","00"
 HKR,                   ,InterruptNumber        ,1      ,"04","00","00","00"

[COMMON_NDIS.reg]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 ;HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 ;HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 ;HKR,NDI                ,NdiInstaller           ,0      ,"NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,1
 HKR,Ndi\params\PSMode,default,0,"1"
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,"enum"
 HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,"1"

;[COMMON_NDIS.reg.ME]
; HKR,                   ,RunningWin9X           ,0      ,"1"
; HKR,                   ,DevLoader              ,0      ,"*ndis"
 ;HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 ;HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 ;HKR,NDI                ,NdiInstaller           ,0      ,"NdiProc"
 ;HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 ;HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 ;HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 ;HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 ;HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 ;HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 ;HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 ;HKR,defaults,PSMode,0,1
 ;HKR,NDI\params\PSMode,,0,1
 ;HKR,Ndi\params\PSMode,default,0,"1"
 ;HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 ;HKR,NDI\params\PSMode,type,,"enum"
 ;HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
 ;HKR,NDI\params\PSMode\enum,1,,"Disable"
 ;HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 ;HKR,NDI\params\PSMode,optional,0,"1"

[COMMON_NDIS.reg.NT]
 ;HKR,                   ,EnumPropPages32        ,0      ,"PRISMCFG.cpl,NetPropPageProvider"
 ;HKR,                   ,EnumPropPages32        ,0      ,"NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

 HKR,defaults,PSMode,0,1
 HKR,Ndi\params\PSMode,default,0,"1"
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,"enum"
 HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
 HKR,NDI\params\PSMode,optional,0,"1"

[COMMON.reg]
 HKR,                   ,LanExpress             ,0      ,"1"    
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,defaults,ListenInterval,0,3
 HKR,Ndi\params\ListenInterval,default,0,"3"
 HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
 HKR,NDI\params\ListenInterval,type,,"int"
 HKR,NDI\params\ListenInterval,flag,1,"30","00","00","00"
 HKR,NDI\params\ListenInterval,min,0,"0"
 HKR,NDI\params\ListenInterval,max,0,"77"
 HKR,NDI\params\ListenInterval,step,0,"1"
 HKR,NDI\params\ListenInterval,optional,0,"1"

 HKR,defaults,RTSThresh,0,2432
 HKR,Ndi\params\RTSThresh,default,0,"2432"
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,"int"
 HKR,NDI\params\RTSThresh,flag,1,"20","00","00","00"
 HKR,NDI\params\RTSThresh,min,0,"0"
 HKR,NDI\params\RTSThresh,max,0,"2432"
 HKR,NDI\params\RTSThresh,step,0,"64"
 HKR,NDI\params\RTSThresh,optional,0,"1"

 HKR,defaults,FragThresh,0,2432
 HKR,Ndi\params\FragThresh,default,0,"2432"
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,"int"
 HKR,NDI\params\FragThresh,flag,1,"20","00","00","00"
 HKR,NDI\params\FragThresh,min,0,"256"
 HKR,NDI\params\FragThresh,max,0,"2432"
 HKR,NDI\params\FragThresh,step,0,"128"
 HKR,NDI\params\FragThresh,optional,0,"1"

 HKR,defaults,PreambleMode,0,1
 HKR,Ndi\params\PreambleMode,default,0,"1"
 HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
 HKR,NDI\params\PreambleMode,type,,"enum"
 HKR,NDI\params\PreambleMode,flag,1,"30","00","00","00"
 HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
 HKR,NDI\params\PreambleMode,optional,0,"1"

 HKR,defaults,AuthentAlg,0,65535
 HKR,NDI\params\AuthentAlg,default,0,"65535"
 HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
 HKR,NDI\params\AuthentAlg,type,,"enum"
 HKR,NDI\params\AuthentAlg,flag,1,"30","00","00","00"
 HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
 HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
 HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
 HKR,NDI\params\AuthentAlg,optional,0,"1"

 HKR,defaults,AdhocDemoMode,0,0
 HKR,Ndi\params\AdhocDemoMode,default,0,"0"
 HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
 HKR,NDI\params\AdhocDemoMode,type,,"enum"
 HKR,NDI\params\AdhocDemoMode,flag,1,"30","00","00","00"
 HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
 HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
 HKR,NDI\params\AdhocDemoMode,optional,0,"1"

 HKR,defaults,LoadFirmware,0,1
;HKR,NDI\params\LoadFirmware,,0,1 ; Moved to device specific entry
 HKR,Ndi\params\LoadFirmware,default,0,"1"
 HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
 HKR,NDI\params\LoadFirmware,type,,"enum"
 HKR,NDI\params\LoadFirmware,flag,1,"30","00","00","00"
 HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
 HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
 HKR,NDI\params\LoadFirmware,optional,0,"1"

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
; PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers


[PRISM_DRIVER.copy]
 EXPRESS.sys

;[PRISM_DRIVER.copy.ME]
; EXPRESS.sys
 
[PRISM_DRIVER.copy.NT]
 EXPRESS.sys
 
[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 EXPRESS.sys           = 1

;[SourceDisksFiles.ME]   ; WinMe
; EXPRESS.sys           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 EXPRESS.sys           = 1
