;*******************************************************************************
;*                                                                            **
;*                     I N T E L   P R O P R I E T A R Y                      **
;*                                                                            **
;*   COPYRIGHT (c) 2000-2003 BY INTEL CORPORATION. ALL RIGHTS RESERVED.  NO   **
;*   PART  OF  THIS  PROGRAM OR PUBLICATION MAY BE REPRODUCED, TRANSMITTED,   **
;*   TRANSCRIBED, STORED IN A RETRIEVAL  SYSTEM,  OR  TRANSLATED  INTO  ANY   **
;*   LANGUAGE OR COMPUTER LANGUAGE IN ANY FORM OR BY ANY MEANS, ELECTRONIC,   **
;*   MECHANICAL, MAGNETIC, OPTICAL, CHEMICAL, MANUAL, OR OTHERWISE, WITHOUT   **
;*   THE PRIOR WRITTEN PERMISSION OF :                                        **
;*                                                                            **
;*                             INTEL CORPORATION                              **
;*                                                                            **
;*                          2200 MISSION COLLEGE BLVD                         **
;*                                                                            **
;*                     SANTA CLARA, CALIFORNIA 95052-8119                     **
;*                                                                            **
;*******************************************************************************
;
;*******************************************************************************
; e100b325.INF
; $Revision: 11 $
;
; Intel 8255x-based PCI Ethernet Adapters
; PnP install script for Windows XP
;
;   Version 7.0.28

[Version]
Signature       = "$Windows NT$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %V_INTEL%
CatalogFile     = e100b325.cat
DriverVer       = 09/17/2003,7.0.28

[Manufacturer]
%V_INTEL%   = Intel, NTx86

[ControlFlags]
ExcludeFromSelect =  \
                        PCI\VEN_8086&DEV_1229&SUBSYS_00018086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00028086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00038086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00048086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00058086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00068086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_000B8086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_000C8086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00118086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00138086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00308086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00418086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10098086&REV_05,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10138086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10168086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10308086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10418086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10518086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10528086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_04,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_05,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21008086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21038086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21048086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21058086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21068086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22018086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22048086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22058086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22068086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24028086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24098086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_240F8086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24108086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24118086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24128086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24138086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_005C1014&REV_04,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_005C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_105C1014&REV_08,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_105C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_01F11014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_01F21014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_01BC1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_02071014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_023F1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_305C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_405C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_505C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_605C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_705C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_805C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10C0103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10C3103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10CA103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10CB103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10E3103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10E4103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_1200103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30010E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30020E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30030E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30040E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30050E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30060E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30070E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_009B1028&REV_08,\
                        PCI\VEN_8086&DEV_2449,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30108086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30118086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30128086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30138086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30148086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30158086,\
                        PCI\VEN_8086&DEV_1031,\
                        PCI\VEN_8086&DEV_1032,\
                        PCI\VEN_8086&DEV_1033,\
                        PCI\VEN_8086&DEV_1034,\
                        PCI\VEN_8086&DEV_1035,\
                        PCI\VEN_8086&DEV_1036,\
                        PCI\VEN_8086&DEV_1038,\
                        PCI\VEN_8086&DEV_1039,\
                        PCI\VEN_8086&DEV_103A,\
                        PCI\VEN_8086&DEV_103B,\
                        PCI\VEN_8086&DEV_103C,\
                        PCI\VEN_8086&DEV_103D,\
                        PCI\VEN_8086&DEV_103E,\
                        PCI\VEN_8086&DEV_1050,\
                        PCI\VEN_8086&DEV_1051,\
                        PCI\VEN_8086&DEV_1052,\
                        PCI\VEN_8086&DEV_1053,\
                        PCI\VEN_8086&DEV_1054,\
                        PCI\VEN_8086&DEV_1055,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_00120E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30118086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_01CE1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_01DC1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_01EB1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_01EC1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02021014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02051014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02171014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02651014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02671014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_026A1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_00120E11,\
                        PCI\VEN_8086&DEV_103D&SUBSYS_05221014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00708086,\
                        PCI\VEN_8086&DEV_1229&REV_01,\
                        PCI\VEN_8086&DEV_1229&REV_02,\
                        PCI\VEN_8086&DEV_1229&REV_04,\
                        PCI\VEN_8086&DEV_1229&REV_05,\
                        PCI\VEN_8086&DEV_1229&REV_08,\
                        PCI\VEN_8086&DEV_1229&REV_09,\
                        PCI\VEN_8086&DEV_1229&REV_0C,\
                        PCI\VEN_8086&DEV_1229&REV_0D,\
                        PCI\VEN_8086&DEV_1229&REV_0E,\
                        PCI\VEN_8086&DEV_1229&REV_0F,\
                        PCI\VEN_8086&DEV_1229&REV_10,\
                        PCI\VEN_8086&DEV_1059,\
                        PCI\VEN_8086&DEV_2459,\
                        PCI\VEN_8086&DEV_245D


[Intel.NTx86]
; DisplayName                Section        DeviceID
; -----------                -------        --------
; ich
%PCIE100EMBLON.DeviceDesc%      = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449
%PCIE100EMBEDDED.DeviceDesc%    = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30108086
%PCIE100EMBEDDED.DeviceDesc%    = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30108086&REV_01
%PCIE100EMBEDDED.DeviceDesc%    = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30108086&REV_03
%PCIE100PLUSEMBEDDED.DeviceDesc%= XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30118086
%PCIE100PLUSEMBEDDED.DeviceDesc%= XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30118086&REV_01
%PCIE100PLUSEMBEDDED.DeviceDesc%= XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30118086&REV_03
%PCIE1EMBEDDED.DeviceDesc%      = XP_D110G.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30128086
%PCIE1EMBEDDED.DeviceDesc%      = XP_D110G.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30128086&REV_01
%PCIE1EMBEDDED.DeviceDesc%      = XP_D110G.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30128086&REV_03

%PCIE100EMBLOM.DeviceDesc%      = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30138086
%PCIE100EMBLOM.DeviceDesc%      = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30138086&REV_01
%PCIE100EMBLOM.DeviceDesc%      = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30138086&REV_03
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30148086
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30148086&REV_01
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_30148086&REV_03

%PCIE100EMBLON.DeviceDesc%      = XP_D110KMP.ndi, PCI\VEN_8086&DEV_2449&SUBSYS_30188086
%PCIE100EMBLON.DeviceDesc%      = XP_D110KMP.ndi, PCI\VEN_8086&DEV_2449&SUBSYS_30188086&REV_01
%PCIE100EMBLON.DeviceDesc%      = XP_D110KMP.ndi, PCI\VEN_8086&DEV_2449&SUBSYS_30188086&REV_03

;ICH3 - kinerreth (9)LOM/(A)CNR/(B)+LOM/(C)+CNR/(D)LOM mobile/(E)+ Mobile
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1031&SUBSYS_9550107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1031&SUBSYS_5350107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1031&SUBSYS_1450107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1031&SUBSYS_0400107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1031&SUBSYS_0401107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1031&SUBSYS_0600107B
%PCIE100EMBLOM.DeviceDesc%      = XP_D110KMP.ndi, PCI\VEN_8086&DEV_1031
%PCIE100EMBLOM.DeviceDesc%      = XP_D110KMP.ndi, PCI\VEN_8086&DEV_1032
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110KMP.ndi, PCI\VEN_8086&DEV_1033
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110KMP.ndi, PCI\VEN_8086&DEV_1034
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110KMP.ndi, PCI\VEN_8086&DEV_1038

;ICH4 - kinerreth (9)LOM/(A)CNR/(B)+LOM/(C)+CNR/(D)LOM mobile/(E)+ Mobile
; need to see if there are different parameters required in registry between them
%PCIE100EMBLOM.DeviceDesc%      = XP_D110K.ndi,   PCI\VEN_8086&DEV_1039
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_1049107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_4000107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_2000107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_2700107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_5288107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_2009107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_2010107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_2018107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_2019107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_1039&SUBSYS_5350107B
%PCIE100EMBLOM.DeviceDesc%      = XP_D110K.ndi,   PCI\VEN_8086&DEV_103A
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110K.ndi,   PCI\VEN_8086&DEV_103B
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110K.ndi,   PCI\VEN_8086&DEV_103C
%PCIE100EMBLOM.DeviceDesc%      = XP_D110KMP.ndi, PCI\VEN_8086&DEV_103D
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_103D&SUBSYS_0402107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_103D&SUBSYS_0450107B
%PCIE100EMBLOM.DeviceDesc%	= XP_D110K.ndi,   PCI\VEN_8086&DEV_103D&SUBSYS_0601107B
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110KMP.ndi, PCI\VEN_8086&DEV_103E

;ICH5 - kinerreth (9)LOM/(A)CNR/(B)+LOM/(C)+CNR/(D)LOM mobile/(E)+ Mobile
%PCIE100EMBLOM.DeviceDesc%      = XP_D110K.ndi,   PCI\VEN_8086&DEV_1050
%PCIE100EMBLOM.DeviceDesc%      = XP_D110K.ndi,   PCI\VEN_8086&DEV_1051
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110K.ndi,   PCI\VEN_8086&DEV_1052
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110K.ndi,   PCI\VEN_8086&DEV_1053
%PCIE100EMBLOM.DeviceDesc%      = XP_D110KMP.ndi, PCI\VEN_8086&DEV_1054  ;mobile
%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110KMP.ndi, PCI\VEN_8086&DEV_1055  ;mobile

%PCIE100PLUSEMBLOM.DeviceDesc%  = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_00120E11
%PCIE100EMBLOM.DeviceDesc%      = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_00910E11

%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_01CE1014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_01DC1014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_01EB1014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_01EC1014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_02021014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_02051014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_02171014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_02341014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_023D1014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_02441014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_02451014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_02651014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_02671014
%IBMFEK.DeviceDesc%             = XP_D110K.ndi,   PCI\VEN_8086&DEV_2449&SUBSYS_026A1014
%IBMFES.DeviceDesc%             = XP_D110KMP.ndi, PCI\VEN_8086&DEV_1031&SUBSYS_022D1014
%PCIE100EMBLOM.DeviceDesc%      = XP_D110KMP.ndi, PCI\VEN_8086&DEV_1031&SUBSYS_02091014
%PCIE100EMBLOM.DeviceDesc%      = XP_D110KMP.ndi, PCI\VEN_8086&DEV_103D&SUBSYS_05221014

;=========== 1229 =====================================================

%PCIE10PPCI.DeviceDesc% = XP_E10P.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_00038086

%PCIE100BTX.DeviceDesc%         = XP_E100B.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00018086
%PCIE100BT4.DeviceDesc%         = XP_E100B.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00028086
%PCIE100RWU.DeviceDesc%         = XP_E100B.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00048086
%I557IFE.DeviceDesc%            = XP_E100B.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00058086
%I557IFEWFM.DeviceDesc%         = XP_E100B.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00068086

%I558IFE.DeviceDesc%            = XP_D101.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00078086
%I558IFEWFM.DeviceDesc%         = XP_D101.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00088086
%PCIE100PLUS.DeviceDesc%        = XP_D101r5.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00098086
%PCIE100MAN.DeviceDesc%         = XP_D101r5.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_000A8086

%PCIE100PLUS.DeviceDesc%        = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_000B8086
%PCIE100MAN.DeviceDesc%         = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_000C8086
%PCIE100AOL.DeviceDesc%         = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_000D8086
%PCIE100MANAOL.DeviceDesc%      = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_000E8086
%PCIE100S0.DeviceDesc%          = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_000F8086

%PCIE100S.DeviceDesc%           = XP_D101S.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00108086
%PCIE100S.DeviceDesc%           = XP_D101S.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00118086
%PCIE100SADV.DeviceDesc%        = XP_D101S.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00128086
%PCIE100SADV.DeviceDesc%        = XP_D101S.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00138086

%PCIE100MANAOLGC.DeviceDesc%    = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00308086
%PCIE100S0.DeviceDesc%          = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00318086
%PCIE100Sx.DeviceDesc%          = XP_D102SC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00408086
%PCIE100Sx.DeviceDesc%          = XP_D102SC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00418086
%PCIE100S0.DeviceDesc%          = XP_D102SCN.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_00428086
%PCIE100Sx.DeviceDesc%          = XP_D102mC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00508086
%PCIE100Sx.DeviceDesc%          = XP_D102mC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00518086
%PCIE100BSPLUSD.DeviceDesc%     = XP_D102mC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00608086
%PCIE100LAVON.DeviceDesc%       = XP_Lavon.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00708086
%PCIE100LAVON.DeviceDesc%       = XP_Lavon.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00718086

%PCIE100SERVER.DeviceDesc%      = XP_D101.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10098086&REV_04
%PCIE100SERVER.DeviceDesc%      = XP_D101r5.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10098086&REV_05
%PCIE100SERVERW.DeviceDesc%     = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_100C8086
%PCIE100SSVR.DeviceDesc%        = XP_D101SS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10128086
%PCIE100SSVR.DeviceDesc%        = XP_D101SS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10138086
%PCIE100DUALx.DeviceDesc%       = XP_D102m0.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10148086
%PCIE100DUALSx.DeviceDesc%      = XP_D102mS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10158086
%PCIE100DUALSx.DeviceDesc%      = XP_D102mS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10168086
%PCIE100DUAL.DeviceDesc%        = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10178086
%PCIE100MANAOLGS.DeviceDesc%    = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10308086
%PCIE100SxSVR.DeviceDesc%       = XP_D102SSC.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_10408086
%PCIE100SxSVR.DeviceDesc%       = XP_D102SSC.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_10418086
%PCIE100S0SVR.DeviceDesc%       = XP_D102SSCN.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_10428086
%PCIE100SxSVR.DeviceDesc%       = XP_D102mS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10508086
%PCIE100S0SVR.DeviceDesc%       = XP_D102SSCN.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_10518086
%PCIE100S0SVR.DeviceDesc%       = XP_D102SSCN.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_10528086
%PCIE100DUAL.DeviceDesc%        = XP_D101.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_04
%PCIE100DUAL.DeviceDesc%        = XP_D101r5D.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_05
%PCIE100BSPLUSS.DeviceDesc%     = XP_D102mS.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10608086

%I559IFE.DeviceDesc%            = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30008086
%I559IFEAOL.DeviceDesc%         = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30018086
%I559IFEAOL.DeviceDesc%         = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30018086&REV_09
%I559IFEAOLII.DeviceDesc%       = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30028086
%PCIE100SxL.DeviceDesc%         = XP_D102SC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_30068086
%PCIE100SxL.DeviceDesc%         = XP_D102SC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_30078086
%PCIE100S0L.DeviceDesc%         = XP_D102SCN.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_30088086
%PCIE100SxL.DeviceDesc%         = XP_D102mC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_30108086
%PCIE100SxL.DeviceDesc%         = XP_D102mC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_30118086


;Samsung

;Compaq
%I559CLONPCI.DeviceDesc%        = XP_D101S.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_B2090E11
%I559IFEAOLCPQ.DeviceDesc%      = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30010E11
%I559IFEAOLCPQ.DeviceDesc%      = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30020E11
%I559IFEAOLCPQ.DeviceDesc%      = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30030E11
%I559IFEAOLCPQ.DeviceDesc%      = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30040E11
%I559IFEAOLCPQ.DeviceDesc%      = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30050E11
%I559IFEAOLCPQ.DeviceDesc%      = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30060E11
%I559IFEAOLCPQ.DeviceDesc%      = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30070E11

;HP
%HPTX.DeviceDesc%               = XP_E100B.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10C0103C
%HPTX.DeviceDesc%               = XP_D101r5.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10C3103C
%HPTX.DeviceDesc%               = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10CA103C
%HPTX.DeviceDesc%               = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10CB103C
%HPTX.DeviceDesc%               = XP_D102SC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10E3103C
%HPTX.DeviceDesc%               = XP_D102SC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10E4103C
%HPTX.DeviceDesc%               = XP_E100B.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_1200103C
%HPTX.DeviceDesc%               = XP_D102m0.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_1273103C

;IBM
%IBMFE9.DeviceDesc%             = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_01BC1014&REV_09
%IBMFE9.DeviceDesc%             = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_01BC1014&REV_08
%IBMFE9.DeviceDesc%             = XP_D101M.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_01BC1014
%IBMFED.DeviceDesc%             = XP_D102SC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_02071014
%IBMFED.DeviceDesc%             = XP_D102SC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_023F1014

;Dell Viper
%PCIE100B.DeviceDesc%           = XP_D101MG.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_009B1028&REV_08
%PCIE100B.DeviceDesc%           = XP_D101MG.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_01061028&REV_08

%PCIE100B.DeviceDesc%           = XP_E100B.ndi,    PCI\VEN_8086&DEV_1229&REV_01
%PCIE100B.DeviceDesc%           = XP_E100B.ndi,    PCI\VEN_8086&DEV_1229&REV_02
%PCIE100B.DeviceDesc%           = XP_D101.ndi,     PCI\VEN_8086&DEV_1229&REV_04
%PCIE100B.DeviceDesc%           = XP_D101r5.ndi,   PCI\VEN_8086&DEV_1229&REV_05
%PCIE100B.DeviceDesc%           = XP_D101MG.ndi,   PCI\VEN_8086&DEV_1229&REV_08
%PCIE100B.DeviceDesc%           = XP_D101SG.ndi,   PCI\VEN_8086&DEV_1229&REV_09
%PCIE100B.DeviceDesc%           = XP_D102SCNG.ndi, PCI\VEN_8086&DEV_1229&REV_0C
%PCIE100B.DeviceDesc%           = XP_D102mG.ndi,   PCI\VEN_8086&DEV_1229&REV_0D
%PCIE100B.DeviceDesc%           = XP_D102mG.ndi,   PCI\VEN_8086&DEV_1229&REV_0E
%PCIE100LAVONLOM.DeviceDesc%    = XP_Lavon.ndi,    PCI\VEN_8086&DEV_1229&REV_0F
%PCIE100LAVONLOM.DeviceDesc%    = XP_Lavon.ndi,    PCI\VEN_8086&DEV_1229&REV_10
%PCIE100LAVONMB.DeviceDesc%     = XP_Lavonmb.ndi,  PCI\VEN_8086&DEV_1059&REV_0F
%PCIE100LAVONMB.DeviceDesc%     = XP_Lavonmb.ndi,  PCI\VEN_8086&DEV_1059&REV_10

; CICH support for embedded dual kinnereth
%PCIE100CICHEMBEDDED.DeviceDesc% = XP_D110K.ndi, PCI\VEN_8086&DEV_2459
%PCIE100CICHEMBEDDED.DeviceDesc% = XP_D110K.ndi, PCI\VEN_8086&DEV_245D

; The following NEC devices defined by PCI\VEN_8086&DEV_1031
;       PCI\VEN_8086&DEV_1031&SUBSYS_81691033
;       PCI\VEN_8086&DEV_1031&SUBSYS_81831033
;       PCI\VEN_8086&DEV_1031&SUBSYS_818b1033
;       PCI\VEN_8086&DEV_1031&SUBSYS_818c1033

;++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
;                        Installation sections
;++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

;--- 82550 Rev D Server
;
[XP_D102mS.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, Security.reg, SecSerDef.reg, LogLinkState.reg, CPUSaverServer.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102mS.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102mS.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev D Client
;
[XP_D102mC.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102mC.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102mC.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev D Client Mobile
;
[XP_D102mCm.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, ALR.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, EnableLLPD.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102mCm.ndi.NT.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102mCm.ndi.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev D Server NoDes
;
[XP_D102m0.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, LogLinkState.reg, CPUSaverServer.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102m0.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102m0.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev F Lavon
;
[XP_Lavon.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, LogLinkState.reg, CPUSaverServer.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_Lavon.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_Lavon.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev F Lavon Mobile
;
[XP_Lavonmb.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, ALR.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, EnableLLPD.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_Lavonmb.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_Lavonmb.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev D Generic
;
[XP_D102mG.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, ALR.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, EnableLLPD.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, Security.reg, LargeSendOffload.reg, LLPDD_OFF.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102mG.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102mG.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82557 Rev 1, 2
;
[XP_E100B.ndi.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82557DelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, e100b.ndi.NT.reg, XP_PowerSave.reg, LargeSendOffload.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_E100B.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_E100B.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82558 Rev 4
;
[XP_D101.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82557DelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, e100b.ndi.NT.reg, XP_PowerSave.reg, LargeSendOffload.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D101.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D101.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82558 Rev 5
;
[XP_D101r5.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, e100b.ndi.NT.reg, XP_PowerSave.reg, LargeSendOffload.reg, LogLinkState.reg, CPUSaverServer.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D101r5.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D101r5.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82558 Rev 5 (Dual)
;
[XP_D101r5D.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg, 82558r5dDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, e100b.ndi.NT.reg, LogLinkState.reg, CPUSaverServer.reg, LargeSendOffload.reg, WakeOnDisable.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D101r5D.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D101r5D.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82559 Rev 8
;
[XP_D101M.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, LogLinkState.reg
AddReg          = e100b.ndi.NT.reg, LargeSendOffload.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D101M.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D101M.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82559 Rev 8 Generic
;
[XP_D101MG.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, ALR.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, EnableLLPD.reg
AddReg          = LLPDD_OFF.reg, e100b.ndi.NT.reg, LargeSendOffload.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D101MG.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D101MG.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82559 Rev 9 Security
;
[XP_D101S.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = Security.reg, LargeSendOffload.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D101S.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D101S.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82559 Rev 9 Security Generic
;
[XP_D101SG.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, ALR.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, EnableLLPD.reg, LLPDD_OFF.reg, e100b.ndi.NT.reg
AddReg          = LargeSendOffload.reg, Security.reg, SecOff.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D101SG.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D101SG.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- D101S Rev 9 Server
;
[XP_D101SS.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = Security.reg, SecSerDef.reg, LargeSendOffload.reg, LogLinkState.reg, CPUSaverServer.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D101SS.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D101SS.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev C Server
;
[XP_D102SC.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, Security.reg, LogLinkState.reg, CPUSaverServer.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102SC.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102SC.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev C
;
[XP_D102SCN.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102SCN.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102SCN.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev C Generic
;
[XP_D102SCNG.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, ALR.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, EnableLLPD.reg, LLPDD_OFF.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, Security.reg, LargeSendOffload.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102SCNG.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102SCNG.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev C Security Server
;
[XP_D102SSC.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, Security.reg, SecSerDef.reg, LogLinkState.reg, CPUSaverServer.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102SSC.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102SSC.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev C Server
;
[XP_D102SSCN.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, LogLinkState.reg, CPUSaverServer.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102SSCN.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102SSCN.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- 82550 Rev C MiniPCI Security
;
[XP_D102MPS.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = TaskOffload.DelReg, ALR.DelReg, 82557DelReg.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, 82558.reg, 82558B.reg, EnablePME.reg, XP_PowerSave.reg, EnableLLPD.reg, e100b.ndi.NT.reg
AddReg          = CSumOffload.reg, LargeSendOffload.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D102MPS.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D102MPS.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- Intel(R) PRO/10+ PCI Adapter
;
[XP_E10P.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82557DelReg.DelReg
AddReg          = Speed10.reg, 82557.reg, e100b.ndi.NT.reg, XP_PowerSave.reg, LargeSendOffload.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_E10P.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_E10P.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- D110 Ethernet
;
[XP_D110K.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = Kinnerth.DelReg, TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg,ICH2.reg,Kinnereth.reg, EnablePME.reg, e100b.ndi.NT.reg, XP_PowerSave.reg, LogLinkState.reg
AddReg          = LargeSendOffload.reg, 82558B.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D110K.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D110K.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

;--- D110 Ethernet Mobile
;
[XP_D110KMP.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
DelReg          = Kinnerth.DelReg, TaskOffload.DelReg, ALR.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg,ICH2.reg,Kinnereth.reg, EnablePME.reg, EnableLLPD.reg, XP_PowerSave.reg, LogLinkState.reg
AddReg          = e100b.ndi.NT.reg, LargeSendOffload.reg, 82558B.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D110KMP.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D110KMP.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[XP_D110G.ndi.NTx86]
Characteristics = 0x84
BusType         = 5
AddReg          = Phone.reg,ICH2.reg,Gilad.reg, e100b.ndi.NT.reg, LogLinkState.reg
CopyFiles       = E100B_325.ndis5.CopyFiles, UninstallW2k.CopyFiles

[XP_D110G.ndi.NTx86.Services]
AddService = E100B, 2, e100b325.Service, common325.EventLog

[XP_D110G.ndi.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles


;+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
;                   Registry settings
;+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

;--- Common 82557 NDI parameters
;
[82557.reg]
HKR,Ndi\Params\NumRfd,                ParamDesc,  0, %RxBuffers%
HKR,Ndi\Params\NumRfd,                Type,       0, "int"
HKR,Ndi\Params\NumRfd,                Default,    0, "48"
HKR,Ndi\Params\NumRfd,                Min,        0, "8"
HKR,Ndi\Params\NumRfd,                Max,        0, "1024"
HKR,Ndi\Params\NumRfd,                Step,       0, "1"
HKR,Ndi\Params\NumRfd,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumRfd,   MiniHelp,   0, %RxBuffersMiniHelp%

HKR,Ndi\Params\NumTcb,                ParamDesc,  0, %TxBuffers%
HKR,Ndi\Params\NumTcb,                Type,       0, "int"
HKR,Ndi\Params\NumTcb,                Default,    0, "16"
HKR,Ndi\Params\NumTcb,                Min,        0, "8"
HKR,Ndi\Params\NumTcb,                Max,        0, "64"
HKR,Ndi\Params\NumTcb,                Step,       0, "1"
HKR,Ndi\Params\NumTcb,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumTcb,   MiniHelp,   0, %TxBuffersMiniHelp%

HKR,Ndi\Params\NumCoalesce,           ParamDesc,  0, %CoalesceBuffers%
HKR,Ndi\Params\NumCoalesce,           Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,           Default,    0, "8"
HKR,Ndi\Params\NumCoalesce,           Min,        0, "1"
HKR,Ndi\Params\NumCoalesce,           Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,           Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,           Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumCoalesce, MiniHelp, 0, %CoalesceBuffersMiniHelp%

HKR,Ndi\Params\Adaptive_IFS,          ParamDesc,  0, %AdaptiveIFS%
HKR,Ndi\Params\Adaptive_IFS,          Type,       0, "int"
HKR,Ndi\Params\Adaptive_IFS,          Default,    0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Min,        0, "0"
HKR,Ndi\Params\Adaptive_IFS,          Max,        0, "255"
HKR,Ndi\Params\Adaptive_IFS,          Step,       0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Adaptive_IFS, MiniHelp, 0, %AdaptiveIFSMiniHelp%

HKR,Ndi\Params\Threshold,             ParamDesc,  0, %AdaptiveTxThreshold%
HKR,Ndi\Params\Threshold,             Type,       0, "int"
HKR,Ndi\Params\Threshold,             Default,    0, "200"
HKR,Ndi\Params\Threshold,             Min,        0, "0"
HKR,Ndi\Params\Threshold,             Max,        0, "200"
HKR,Ndi\Params\Threshold,             Step,       0, "1"
HKR,Ndi\Params\Threshold,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Threshold, MiniHelp,  0, %AdaptiveTxThresholdMiniHelp%

HKR,Ndi\Params\HPQPriorityLevel,      ParamDesc,  0, %HPQPriorityLevelDef%
HKR,Ndi\Params\HPQPriorityLevel,      Type,       0, "int"
HKR,Ndi\Params\HPQPriorityLevel,      Default,    0, "4"
HKR,Ndi\Params\HPQPriorityLevel,      Min,        0, "0"
HKR,Ndi\Params\HPQPriorityLevel,      Max,        0, "7"
HKR,Ndi\Params\HPQPriorityLevel,      Step,       0, "1"
HKR,Ndi\Params\HPQPriorityLevel,      Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\HPQPriorityLevel, MiniHelp,  0, %HPQPriorityLevelDefMiniHelp%

HKR,Ndi\Params\UcodeSW,               ParamDesc,  0, %AdaptiveTechnology%
HKR,Ndi\Params\UcodeSW,               Type,       0, "enum"
HKR,Ndi\Params\UcodeSW,               Default,    0, "1"
HKR,Ndi\Params\UcodeSW\Enum,          "1",        0, %On%
HKR,Ndi\Params\UcodeSW\Enum,          "0",        0, %Off%
HKR,PROSetNdi\NdiExt\Params\UcodeSW,  MiniHelp,   0, %AdaptiveTechnologyMiniHelp%

HKR,Ndi\Params\Coalesce,              ParamDesc,  0, %PciBusEfficiency%
HKR,Ndi\Params\Coalesce,              Type,       0, "enum"
HKR,Ndi\Params\Coalesce,              Default,    0, "0"
HKR,Ndi\Params\Coalesce\Enum,         "1",        0, %Enabled%
HKR,Ndi\Params\Coalesce\Enum,         "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\Coalesce, MiniHelp,   0, %PciBusEfficiencyMiniHelp%

HKR,Ndi\Params\AlwaysConnectGoal,     ParamDesc,  0, %BasicConnectivity%
HKR,Ndi\Params\AlwaysConnectGoal,     Type,       0, "enum"
HKR,Ndi\Params\AlwaysConnectGoal,     Default,    0, "1"
HKR,Ndi\Params\AlwaysConnectGoal\Enum,"1",        0, %Enabled%
HKR,Ndi\Params\AlwaysConnectGoal\Enum,"0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\AlwaysConnectGoal, MiniHelp,   0,  %BasicConnectivityMiniHelp%

HKR,Ndi\Params\NetworkAddress,  ParamDesc,  0, %LocalyAdminAddress%
HKR,Ndi\Params\NetworkAddress,  Type,       0, "edit"
HKR,Ndi\Params\NetworkAddress,  Default,    0, ""
HKR,NDI\params\NetworkAddress,  LimitText,  0, "12"
HKR,NDI\params\NetworkAddress,  UpperCase,  0, "1"
HKR,NDI\params\NetworkAddress,  optional,   0, "1"
HKR,PROSetNdi\NdiExt\Params\NetworkAddress,  MiniHelp,   0, %LocalyAdminAddressMiniHelp%

HKR,Ndi\Params\ConfigIFS,             ParamDesc,  0, %RetransmitInterFrameSpace%
HKR,Ndi\Params\ConfigIFS,             Type,       0, "int"
HKR,Ndi\Params\ConfigIFS,             Default,    0, "6"
HKR,Ndi\Params\ConfigIFS,             Min,        0, "0"
HKR,Ndi\Params\ConfigIFS,             Max,        0, "15"
HKR,Ndi\Params\ConfigIFS,             Step,       0, "1"
HKR,Ndi\Params\ConfigIFS,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\ConfigIFS,   MiniHelp,   0, %RetransmitInterFrameSpaceMiniHelp%

HKR,,PcNic,                     0, "1"
HKR,,MWIEnable,                 2, "0"
HKR,,AdaptiveStalledInterrupts, 2, "1"
HKR,,AdaptiveCarrierLoss,       2, "1"
HKR,,AdaptiveTransmitMethod,    2, "1"
HKR,,Threshold,                 0, "200"

HKR,,DeviceVxDsPrefix,          0, "e100b"


;--- Log Link State Event
;
[LogLinkState.reg]
HKR,Ndi\Params\LogLinkStateEvent,         ParamDesc,  0, %LogLinkState%
HKR,Ndi\Params\LogLinkStateEvent,         Type,       0, "enum"
HKR,Ndi\Params\LogLinkStateEvent,         Default,    0, "0"
HKR,Ndi\Params\LogLinkStateEvent\Enum,    "1",        0, %Enabled%
HKR,Ndi\Params\LogLinkStateEvent\Enum,    "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\LogLinkStateEvent, MiniHelp, 0, %LogLinkStateMiniHelp%


;--- 82558 specifics
;
[82558.reg]
; 802.1p/802.1q Packet Tagging  - This parameter repeated in ICH2.REG
HKR,Ndi\Params\TaggingMode,         ParamDesc,  0, %QoSPacketTag%
HKR,Ndi\Params\TaggingMode,         Type,       0, "enum"
HKR,Ndi\Params\TaggingMode,         Default,    0, "0"
HKR,Ndi\Params\TaggingMode\Enum,    "1",        0, %Enabled%
HKR,Ndi\Params\TaggingMode\Enum,    "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\TaggingMode, MiniHelp, 0, %QosPacketTagMiniHelp%

; Flow Control Settings
HKR,Ndi\Params\FlowControl,         ParamDesc,  0, %FlowControlSettings%
HKR,Ndi\Params\FlowControl,         Type,       0, "enum"
HKR,Ndi\Params\FlowControl,         Default,    0, "3"
HKR,Ndi\Params\FlowControl\Enum,    "3",        0, %GenerateAndRespond%
HKR,Ndi\Params\FlowControl\Enum,    "2",        0, %Respond%
HKR,Ndi\Params\FlowControl\Enum,    "1",        0, %Generate%
HKR,Ndi\Params\FlowControl\Enum,    "0",        0, %Off%
HKR,PROSetNdi\NdiExt\Params\FlowControl, MiniHelp,   0, %FlowControlSettingsMiniHelp%
HKR,,				   FlowControl, 0, "3"

; Adaptive Performance Tuning
HKR,PROSetNdi\Params\CPUSaver,        ParamDesc,  0, %AdaptivePerfTuning%
HKR,PROSetNdi\Params\CPUSaver,        Type,       0, "slider"
HKR,PROSetNdi\Params\CPUSaver,        Default,    0, "0"
HKR,,CPUSaver,                                    0, "0"
HKR,PROSetNdi\Params\CPUSaver,        LeftLabel,  0, %AdapterBandwidth%
HKR,PROSetNdi\Params\CPUSaver,        RightLabel, 0, %CpuUtil%
HKR,PROSetNdi\Params\CPUSaver,        MiniHelp,   0, %AdaptivePerfTuningMiniHelp%
HKR,PROSetNdi\Params\CPUSaver\Values, "0",        0, "0"
HKR,PROSetNdi\Params\CPUSaver\Values, "1",        0, "1"
HKR,PROSetNdi\Params\CPUSaver\Values, "2",        0, "512"
HKR,PROSetNdi\Params\CPUSaver\Values, "3",        0, "768"
HKR,PROSetNdi\Params\CPUSaver\Values, "4",        0, "1024"
HKR,PROSetNdi\Params\CPUSaver\Values, "5",        0, "1280"
HKR,PROSetNdi\Params\CPUSaver\Values, "6",        0, "1536"
HKR,PROSetNdi\Params\CPUSaver\Values, "7",        0, "1792"
HKR,PROSetNdi\Params\CPUSaver\Values, "8",        0, "2048"
HKR,PROSetNdi\Params\CPUSaver\Values, "9",        0, "2304"
HKR,PROSetNdi\Params\CPUSaver\Values, "10",       0, "2560"
HKR,PROSetNdi\Params\CPUSaver\Values, "11",       0, "2816"
HKR,PROSetNdi\Params\CPUSaver\Values, "12",       0, "3072"
HKR,PROSetNdi\Params\CPUSaver\Values, "13",       0, "3328"
HKR,PROSetNdi\Params\CPUSaver\Values, "14",       0, "3584"
HKR,PROSetNdi\Params\CPUSaver\Values, "15",       0, "3840"
HKR,PROSetNdi\Params\CPUSaver\Values, "16",       0, "4096"


;--- 82558 B Rev 5 - no force wake on link
;
[82558B.reg]
; WakeOn
HKR, Ndi\Params\WakeOn,       	  ParamDesc,          0, %WakeOnSettings%
HKR, Ndi\Params\WakeOn,       	  default,            0, "246"
HKR, Ndi\Params\WakeOn\Enum,  	  "0",                0, %Disabled%
HKR, Ndi\Params\WakeOn\Enum,  	  "6",                0, %WakeOnMagicPacket%
HKR, Ndi\Params\WakeOn\Enum,  	  "116",              0, %WakeOnDirected%
HKR, Ndi\Params\WakeOn\Enum,  	  "118",              0, %WakeOnMagicAndDirectedPackets%
HKR, Ndi\Params\WakeOn\Enum,      "246",              0, %OSControlled%
HKR, Ndi\Params\WakeOn,       	  type,               0, "enum"
HKR, Ndi\Params\WakeOn,       	  ExposeLevel,        0, "2"
HKR, Ndi\Params\WakeOn,       	  MiniHelp,           0,  %WakeOnSettingsMiniHelp%
HKR,,				  WakeOn, 	      0, "246"

;Wake on Link parameter
HKR, Ndi\Params\WakeOnLink,       ParamDesc,          0, %WakeOnLinkSettings%
HKR, Ndi\Params\WakeOnLink\Enum,  "0",                0, %Disabled%
HKR, Ndi\Params\WakeOnLink\Enum,  "1",                0, %OSControlled% 
HKR, Ndi\Params\WakeOnLink\Enum,  "2",                0, %Forced%
HKR, Ndi\Params\WakeOnLink,       type,               0, "enum"
;HKR, Ndi\Params\WakeOnLink,       ExposeLevel,        0, "2"
HKR, PROSetNdi\NdiExt\Params\WakeOnLink,       MiniHelp,           0, %WakeOnLinkHelp% 

;--- Wake on disable - sets WakeOn registry key to 0
;
[WakeOnDisable.reg]
HKR,,				  WakeOn, 	      0, "0"

;--- 82559 Enable PME
;
[EnablePME.reg]
HKR,Ndi\Params\EnablePME,             ParamDesc,  0, %EnablePME%
HKR,Ndi\Params\EnablePME,             Type,       0, "enum"
HKR,Ndi\Params\EnablePME,             Default,    0, "2"
HKR,Ndi\Params\EnablePME\Enum,        "1",        0, %Enabled%
HKR,Ndi\Params\EnablePME\Enum,        "0",        0, %Disabled%
HKR,Ndi\Params\EnablePME\Enum,        "2",        0, %NoAction%
HKR,Ndi\Params\EnablePME\Enum,        "255",      0, %HardwareDefault%
HKR,PROSetNdi\NdiExt\Params\EnablePME, MiniHelp,  0, %EnablePMEMiniHelp%

;---
;
[XP_PowerSave.reg]
HKR,,AutoPowerSaveModeEnabled, 0, "0"
HKR,,Force10MbOnD3, 0, "1"
HKR,,SavePowerNowEnabled,    0, "1"

[ICH2.reg]
; 802.1p/802.1q Packet Tagging  - This parameter repeated in 82558.REG
HKR,Ndi\Params\TaggingMode,         ParamDesc,  0, %QoSPacketTag%
HKR,Ndi\Params\TaggingMode,         Type,       0, "enum"
HKR,Ndi\Params\TaggingMode,         Default,    0, "0"
HKR,Ndi\Params\TaggingMode\Enum,    "1",        0, %Enabled%
HKR,Ndi\Params\TaggingMode\Enum,    "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\TaggingMode, MiniHelp, 0, %QoSPacketTagMiniHelp%

; Flow Control Settings
HKR,Ndi\Params\FlowControl,         ParamDesc,  0, %FlowControlSettings%
HKR,Ndi\Params\FlowControl,         Type,       0, "enum"
HKR,Ndi\Params\FlowControl,         Default,    0, "3"
HKR,Ndi\Params\FlowControl\Enum,    "3",        0, %GenerateAndRespond%
HKR,Ndi\Params\FlowControl\Enum,    "2",        0, %Respond%
HKR,Ndi\Params\FlowControl\Enum,    "1",        0, %Generate%
HKR,Ndi\Params\FlowControl\Enum,    "0",        0, %Off%
HKR,PROSetNdi\NdiExt\Params\FlowControl, MiniHelp,   0, %FlowControlSettingsMiniHelp%

HKR,Ndi\Params\NumRfd,                ParamDesc,  0, %RxBuffers%
HKR,Ndi\Params\NumRfd,                Type,       0, "int"
HKR,Ndi\Params\NumRfd,                Default,    0, "48"
HKR,Ndi\Params\NumRfd,                Min,        0, "8"
HKR,Ndi\Params\NumRfd,                Max,        0, "1024"
HKR,Ndi\Params\NumRfd,                Step,       0, "1"
HKR,Ndi\Params\NumRfd,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumRfd,   MiniHelp,   0, %RxBuffersMiniHelp%

HKR,Ndi\Params\NumTcb,                ParamDesc,  0, %TxBuffers%
HKR,Ndi\Params\NumTcb,                Type,       0, "int"
HKR,Ndi\Params\NumTcb,                Default,    0, "16"
HKR,Ndi\Params\NumTcb,                Min,        0, "8"
HKR,Ndi\Params\NumTcb,                Max,        0, "64"
HKR,Ndi\Params\NumTcb,                Step,       0, "1"
HKR,Ndi\Params\NumTcb,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumTcb,   MiniHelp,   0, %TxBuffersMiniHelp%

HKR,Ndi\Params\NumCoalesce,           ParamDesc,  0, %CoalesceBuffers%
HKR,Ndi\Params\NumCoalesce,           Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,           Default,    0, "8"
HKR,Ndi\Params\NumCoalesce,           Min,        0, "1"
HKR,Ndi\Params\NumCoalesce,           Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,           Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,           Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumCoalesce, MiniHelp, 0, %CoalesceBuffersMiniHelp%

HKR,Ndi\Params\Adaptive_IFS,          ParamDesc,  0, %AdaptiveIFS%
HKR,Ndi\Params\Adaptive_IFS,          Type,       0, "int"
HKR,Ndi\Params\Adaptive_IFS,          Default,    0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Min,        0, "0"
HKR,Ndi\Params\Adaptive_IFS,          Max,        0, "255"
HKR,Ndi\Params\Adaptive_IFS,          Step,       0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Adaptive_IFS, MiniHelp, 0, %AdaptiveIFSMiniHelp%

HKR,Ndi\Params\Threshold,             ParamDesc,  0, %AdaptiveTxThreshold%
HKR,Ndi\Params\Threshold,             Type,       0, "int"
HKR,Ndi\Params\Threshold,             Default,    0, "200"
HKR,Ndi\Params\Threshold,             Min,        0, "0"
HKR,Ndi\Params\Threshold,             Max,        0, "200"
HKR,Ndi\Params\Threshold,             Step,       0, "1"
HKR,Ndi\Params\Threshold,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Threshold, MiniHelp,  0, %AdaptiveTxThresholdMiniHelp%

HKR,Ndi\Params\UcodeSW,               ParamDesc,  0, %AdaptiveTechnology%
HKR,Ndi\Params\UcodeSW,               Type,       0, "enum"
HKR,Ndi\Params\UcodeSW,               Default,    0, "1"
HKR,Ndi\Params\UcodeSW\Enum,          "1",        0, %On%
HKR,Ndi\Params\UcodeSW\Enum,          "0",        0, %Off%
HKR,PROSetNdi\NdiExt\Params\UcodeSW,  MiniHelp,   0, %AdaptiveTechnologyMiniHelp%

HKR,Ndi\Params\Coalesce,              ParamDesc,  0, %PciBusEfficiency%
HKR,Ndi\Params\Coalesce,              Type,       0, "enum"
HKR,Ndi\Params\Coalesce,              Default,    0, "0"
HKR,Ndi\Params\Coalesce\Enum,         "1",        0, %Enabled%
HKR,Ndi\Params\Coalesce\Enum,         "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\Coalesce, MiniHelp,   0, %PciBusEfficiencyMiniHelp%

; Adaptive Performance Tuning
HKR,PROSetNdi\Params\CPUSaver,        ParamDesc,  0, %AdaptivePerfTuning%
HKR,PROSetNdi\Params\CPUSaver,        Type,       0, "slider"
HKR,PROSetNdi\Params\CPUSaver,        Default,    0, "0"
HKR,,CPUSaver,                                    0, "0"
HKR,PROSetNdi\Params\CPUSaver,        LeftLabel,  0, %AdapterBandwidth%
HKR,PROSetNdi\Params\CPUSaver,        RightLabel, 0, %CpuUtil%
HKR,PROSetNdi\Params\CPUSaver,        MiniHelp,   0, %AdaptivePerfTuningMiniHelp%
HKR,PROSetNdi\Params\CPUSaver\Values, "0",        0, "0"
HKR,PROSetNdi\Params\CPUSaver\Values, "1",        0, "1"
HKR,PROSetNdi\Params\CPUSaver\Values, "2",        0, "512"
HKR,PROSetNdi\Params\CPUSaver\Values, "3",        0, "768"
HKR,PROSetNdi\Params\CPUSaver\Values, "4",        0, "1024"
HKR,PROSetNdi\Params\CPUSaver\Values, "5",        0, "1280"
HKR,PROSetNdi\Params\CPUSaver\Values, "6",        0, "1536"
HKR,PROSetNdi\Params\CPUSaver\Values, "7",        0, "1792"
HKR,PROSetNdi\Params\CPUSaver\Values, "8",        0, "2048"
HKR,PROSetNdi\Params\CPUSaver\Values, "9",        0, "2304"
HKR,PROSetNdi\Params\CPUSaver\Values, "10",       0, "2560"
HKR,PROSetNdi\Params\CPUSaver\Values, "11",       0, "2816"
HKR,PROSetNdi\Params\CPUSaver\Values, "12",       0, "3072"
HKR,PROSetNdi\Params\CPUSaver\Values, "13",       0, "3328"
HKR,PROSetNdi\Params\CPUSaver\Values, "14",       0, "3584"
HKR,PROSetNdi\Params\CPUSaver\Values, "15",       0, "3840"
HKR,PROSetNdi\Params\CPUSaver\Values, "16",       0, "4096"

HKR,Ndi\Params\NetworkAddress,  ParamDesc,  0, %LocalyAdminAddress%
HKR,Ndi\Params\NetworkAddress,  Type,       0, "edit"
HKR,Ndi\Params\NetworkAddress,  Default,    0, ""
HKR,NDI\params\NetworkAddress,  LimitText,  0, "12"
HKR,NDI\params\NetworkAddress,  UpperCase,  0, "1"
HKR,NDI\params\NetworkAddress,  optional,   0, "1"
HKR,PROSetNdi\NdiExt\Params\NetworkAddress,  MiniHelp,   0, %LocalyAdminAddressMiniHelp%

HKR,Ndi\Params\ConfigIFS,             ParamDesc,  0, %RetransmitInterFrameSpace%
HKR,Ndi\Params\ConfigIFS,             Type,       0, "int"
HKR,Ndi\Params\ConfigIFS,             Default,    0, "10"
HKR,Ndi\Params\ConfigIFS,             Min,        0, "0"
HKR,Ndi\Params\ConfigIFS,             Max,        0, "15"
HKR,Ndi\Params\ConfigIFS,             Step,       0, "1"
HKR,Ndi\Params\ConfigIFS,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\ConfigIFS,   MiniHelp,   0, %RetransmitInterFrameSpaceMiniHelp%

HKR,,TaggingMode,               0, "0"          ; Tagging mode
HKR,,PcNic,                     0, "1"
HKR,,MWIEnable,                 0, "0"
HKR,,DeviceVxDsPrefix,          0, "e100b"
HKR,,HPQDisable,                0, "1"
HKR,,AdaptiveStalledInterrupts, 2, "1"
HKR,,AdaptiveCarrierLoss,       2, "1"
HKR,,AdaptiveTransmitMethod,    2, "1"
HKR,,Threshold,                 0, "200"

;--- Kinnereth
[Kinnereth.reg]
HKR,,BroadcastEnable,           0, "1"
HKR,,EnableDynamicReducedPower, 0, "1"

[Kinnerth.DelReg]
HKR,Ndi\Params\AcpiWol
HKR,,AcpiWol

;--- Gilad parameters starts
[Gilad.reg]
HKR,,EnablePME,         0, "2"
HKR,,BroadcastEnable,   0, "0"

;--- Enable Power Down
;
[EnableLLPD.reg]
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      ParamDesc,  0, %SmartPowerDown%
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Type,       0, "enum"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Default,    0, "1"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss\Enum, "1",        0, %Enabled%
HKR,Ndi\Params\EnablePowerDownOnLinkLoss\Enum, "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\EnablePowerDownOnLinkLoss, MiniHelp, 0, %SmartPowerDownMiniHelp%

;HKR,Ndi\Params\LinkBasedLogin,              ParamDesc,  0, %AdaptiveLinkResponse%
;HKR,Ndi\Params\LinkBasedLogin,              Type,       0, "enum"
;HKR,Ndi\Params\LinkBasedLogin,              Default,    0, "0"
;HKR,Ndi\Params\LinkBasedLogin\Enum,         "1",        0, %On%
;HKR,Ndi\Params\LinkBasedLogin\Enum,         "0",        0, %Off%
;HKR,PROSetNdi\NdiExt\Params\LinkBasedLogin, MiniHelp,   0, %AdaptiveLinkResponseMiniHelp%

[LLPDD_OFF.reg]
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Default,    0, "0"

;--- Security
;
[Security.reg]
HKR,Ndi\Params\IPSecEnabled,     ParamDesc,  0, %IPSecEnabled%
HKR,Ndi\Params\IPSecEnabled,     Type,       0, "enum"
HKR,Ndi\Params\IPSecEnabled,     Default,    0, "1"
HKR,Ndi\Params\IPSecEnabled\Enum,"0",        0, %Disabled%
HKR,Ndi\Params\IPSecEnabled\Enum,"1",        0, %Enabled%
HKR,PROSetNdi\NdiExt\Params\IPSecEnabled, MiniHelp, 0, %IPSecEnabledMiniHelp%

HKR,Ndi\Params\MaxNumSecAssoc,  ParamDesc,  0, %SecurityAssociations%
HKR,Ndi\Params\MaxNumSecAssoc,  Type,       0, "int"
HKR,Ndi\Params\MaxNumSecAssoc,  Default,    0, "64"     ; Client
HKR,Ndi\Params\MaxNumSecAssoc,  Min,        0, "1"
HKR,Ndi\Params\MaxNumSecAssoc,  Max,        0, "5000"
HKR,Ndi\Params\MaxNumSecAssoc,  Step,       0, "1"
HKR,Ndi\Params\MaxNumSecAssoc,  Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\MaxNumSecAssoc, MiniHelp, 0, %SecurityAssociationsMiniHelp%

HKR,,IPSecTunnelMode, 2, "1"
HKR,,MaxNumSecAssoc,  2, "64"

[SecSerDef.reg]
HKR,Ndi\Params\MaxNumSecAssoc,  Default,    0, "1000"   ; Server
HKR,,MaxNumSecAssoc,  2, "1000"

[SecOff.reg]
HKR,Ndi\Params\IPSecEnabled,     Default,    0, "0"

[SecDisable.reg]
HKR,,IPSecEnabled,    0, "0"

;--- Checksum Offload
;
[CSumOffload.reg]
HKR,Ndi\Params\ChecksumEnabled,     ParamDesc,  0, %ChecksumEnabled%
HKR,Ndi\Params\ChecksumEnabled,     Type,       0, "enum"
HKR,Ndi\Params\ChecksumEnabled,     Default,    0, "1"
HKR,Ndi\Params\ChecksumEnabled\Enum,"0",        0, %Disabled%
HKR,Ndi\Params\ChecksumEnabled\Enum,"1",        0, %Enabled%
HKR,PROSetNdi\NdiExt\Params\ChecksumEnabled,  MiniHelp, 0, %ChecksumEnabledMiniHelp%

;--- Large Send Offload
;
[LargeSendOffload.reg]
HKR,Ndi\Params\LargeSendEnabled,     ParamDesc,  0, %LargeSendEnabled%
HKR,Ndi\Params\LargeSendEnabled,     Type,       0, "enum"
HKR,Ndi\Params\LargeSendEnabled,     Default,    0, "1"
HKR,Ndi\Params\LargeSendEnabled\Enum,"0",        0, %Disabled%
HKR,Ndi\Params\LargeSendEnabled\Enum,"1",        0, %Enabled%
HKR,PROSetNdi\NdiExt\Params\LargeSendEnabled,  MiniHelp, 0, %LargeSendEnabledMiniHelp%


;--- CPUSaver Server
[CPUSaverServer.reg]
HKR,PROSetNdi\Params\CPUSaver,	Default,    0, "1536"
HKR,,CPUSaver,                              0, "1536"

;--- CPUSaver override for Cardbus
;
[CPUSaverOverride.reg]
HKR,PROSetNdi\Params\CPUSaver,  Default,    0, "1"
HKR,,CPUSaver,                              0, "1"

;--- Speed Duplex Mode common base 10Mb
;
[Speed10.reg]
HKR, Ndi\params\SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR, Ndi\params\SpeedDuplex,       default,    0, "1"
HKR, Ndi\params\SpeedDuplex,       type,       0, "enum"
HKR, Ndi\params\SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, MiniHelp,    0, %SpeedDuplex10MiniHelp%
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, ExposeLevel, 0, "3"

;--- Speed Duplex Mode common base 10/100Mb
;
[Speed100.reg]
HKR, Ndi\params\SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR, Ndi\params\SpeedDuplex,       default,    0, "0"
HKR, Ndi\params\SpeedDuplex,       type,       0, "enum"
HKR, Ndi\params\SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR, Ndi\params\SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, MiniHelp,    0, %SpeedDuplexMiniHelp%
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, ExposeLevel, 0, "3"

;--- Gilad Phoneline
;
[Phone.reg]
HKR, Ndi\params\PhyPhonePower,       ParamDesc,  0, %PhyPhonePower%
HKR, Ndi\params\PhyPhonePower,       default,    0, "0"
HKR, Ndi\params\PhyPhonePower,       type,       0, "enum"
HKR, Ndi\params\PhyPhonePower\enum,  "0",        0, %Low%
HKR, Ndi\params\PhyPhonePower\enum,  "1",        0, %High%

HKR, Ndi\params\PhyPhoneSpeed,       ParamDesc,  0, %PhyPhoneSpeed%
HKR, Ndi\params\PhyPhoneSpeed,       default,    0, "1"
HKR, Ndi\params\PhyPhoneSpeed,       type,       0, "enum"
HKR, Ndi\params\PhyPhoneSpeed\enum,  "0",        0, %Low%
HKR, Ndi\params\PhyPhoneSpeed\enum,  "1",        0, %High%

HKR, Ndi\params\PhyGiladIfs,       ParamDesc,  0, %PhyGiladIfs%
HKR, Ndi\params\PhyGiladIfs,       default,    0, "96"
HKR, Ndi\params\PhyGiladIfs,       type,       0, "enum"
HKR, Ndi\params\PhyGiladIfs\enum,  "96",       0, " 96 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "112",      0, "112 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "128",      0, "128 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "144",      0, "144 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "160",      0, "160 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "176",      0, "176 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "192",      0, "192 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "208",      0, "208 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "224",      0, "224 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "240",      0, "240 bit-times"

;--- Clkrun
[Clkrun.reg]
HKR,,CLKRUN,                                      0, "1"

; Del Reg section
;------------------------------------
[SpeedDpx.DelReg]
HKR,Ndi\Params\Speed
HKR,Ndi\Params\ForceDpx
HKR,Ndi\Params\PacketTagging
HKR,,Speed
HKR,,ForceDpx
HKR,,PacketTagging

[TaskOffload.DelReg]
HKR,Ndi\Params\TaskOffload
HKR,,TaskOffload

[ALR.DelReg]
HKR,Ndi\Params\LinkBasedLogin
HKR,,LinkBasedLogin

[82557DelReg.DelReg]
HKR,Ndi\Params\FlowControlReceive
HKR,,FlowControlReceive

[82558BDelReg.DelReg]
HKR, PROSetNdi\Params\WakeOn
HKR, Ndi\Params\WakeOn
HKR, Ndi\Params\WakeOnLink

[82558r5dDelReg.DelReg]
HKR,,AutoPowerSaveModeEnabled
HKR,,Force10MbOnD3

;--- NT NDI object registration
;
[e100b.ndi.NT.reg]
HKR,Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR,Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR,Ndi,            Service,    0, "E100B"

HKR,,LogErrorMessages, 0, "1"

HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1031, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1032, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1033, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1034, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1035, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1036, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1038, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1039, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103A, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103B, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103C, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103D, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103E, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1050, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1051, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1052, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1053, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1054, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1055, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1059, 0, "82551"

;--- Uninstallation
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,DisplayName, 0, %UninstallString%
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,UninstallString, 0, "Prounstl.exe"
HKLM,Software\Intel\Prounstl\Dins, e100b325.din, 0, "8255x.Uninstall"

;  Do MWI in coinstaller
HKR,,CoInstallFlag, 0x00010001, "0x80000004"

;--- NT Service
;
[e100b325.Service]
DisplayName     = %e100bnt.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\e100b325.sys
LoadOrderGroup  = NDIS
AddReg          = TextModeFlags.reg

;--- NT Common base
;
[common325.EventLog]
AddReg = common325.AddEventLog.reg

[common325.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, %MessageStringSource%
HKR, , TypesSupported,   0x00010001, 7

[TextModeFlags.reg]
HKR, , TextModeFlags,    0x00010001, 0x0001


;--- Copy files
;
[DestinationDirs]
DefaultDestDir            = 11
E100B_325.ndis5.CopyFiles  = 12

[SourceDisksNames]
1 = %DISKNAME%,,,

[SourceDisksFiles]
e100b325.din = 1,,
e100b325.sys = 1,,
Prounstl.exe = 1,,
IntelNic.dll = 1,,
e100bmsg.dll = 1,,

[E100B_325.ndis5.CopyFiles]
e100b325.sys,,,2

[UninstallW2k.CopyFiles]
Prounstl.exe,,,2
e100b325.din,,,2

;--- Coinstaller
[CoInstaller_CopyFiles]
IntelNic.dll,,,2
e100bmsg.dll,,,2

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000,"IntelNic.dll,NicCoInstallerEntry"

;--- Localizable Strings
;
[Strings]
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString = "Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      = "%SystemRoot%\System32\netevent.dll;%SystemRoot%\system32\drivers\e100b325.sys"

; NT service name
e100bnt.Service.DispName = "Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       = "On"
Off                      = "Off"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
AutoDetect               = "Auto Detect"
10Mb-Half-Duplex         = "10Mbps/Half Duplex"
10Mb-Full-Duplex         = "10Mbps/Full Duplex"
100Mb-Half-Duplex        = "100Mbps/Half Duplex"
100Mb-Full-Duplex        = "100Mbps/Full Duplex"
High                     = "High"
Low                      = "Low"
None                     = "None"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       = "Generate and Respond"
Respond                  = "Respond"
Generate                 = "Generate"
NoAction                 = "No Action"
HardwareDefault          = "Hardware Default"
OSControlled             = "OS Controlled"
Forced                   = "Forced"

; advanced tab strings
RxBuffers                             = "Receive Descriptors"
RxBuffersMiniHelp                     = "Number of buffers used by the driver when copying data to the protocol memory."
TxBuffers                             = "Transmit Descriptors"
TxBuffersMiniHelp                     = "Sets the number of control blocks available for adapter use."
CoalesceBuffers                       = "Coalesce Buffers"
CoalesceBuffersMiniHelp               = "Number of buffers available for transmits acceleration."
AdaptiveIFS                           = "Adaptive Inter-Frame Spacing"
AdaptiveIFSMiniHelp                   = "Compensates for excessive Ethernet packet collisions by controlling back-to-back timing."
AdaptiveTxThreshold                   =  "Adaptive Transmit Threshold"
AdaptiveTxThresholdMiniHelp           = "Sets number of bytes before adapter empties its FIFO buffer. Actual value is 8 times setting."
HPQPriorityLevelDef                   = "Priority Level Definition"
HPQPriorityLevelDefMiniHelp           = "Sets the controlled cutoff level for using HPQ."
AdaptiveTechnology                    = "Adaptive Technology"
AdaptiveTechnologyMiniHelp            = "Enables/Disables the Adaptive Technology performance feature."
PciBusEfficiency                      = "PCI Bus Efficiency"
PciBusEfficiencyMiniHelp              = "Coalesces transmit packets into single buffer before sending them to network. "
BasicConnectivity                     = "Low Resource Connectivity"
BasicConnectivityMiniHelp             = "Try to load the driver in low resources environment."
LocalyAdminAddress                    = "Locally Administered Address"
LocalyAdminAddressMiniHelp            = "By default, an address is not present and the value field is left blank. To set a LAA in Intel(R) PROSet, enter one in the value field. Note: To set a LAA in Device Manager, select the Value option and enter an address in the field provided."
RetransmitInterFrameSpace             = "Retransmit Inter-Frame Spacing"
RetransmitInterFrameSpaceMiniHelp     = "Compensates for excessive Ethernet packet collisions by controlling retransmit timing."
LogLinkState                          = "Log Link State Event"
LogLinkStateMiniHelp                  = "Enables/Disables the link state message to logger. "
QoSPacketTag                          = "QoS Packet Tagging"
QosPacketTagMiniHelp                  = "Send and receive IEEE Tagged frames (802.3ac/802.1p/802.1Q)."
FlowControlSettings                   = "Flow Control Settings"
FlowControlSettingsMiniHelp           = "Pauses packet transmission on receipt of full flow control frame and Send full flow control frame to notify the other side to stop transmission."
SpeedDuplex                           = "Link Speed & Duplex"
SpeedDuplex10MiniHelp                 = "Sets link speed to 10 Mbps and duplex to half or full. Must coincide with switch port or no link will occur."
SpeedDuplexMiniHelp                   = "Sets link speed to 10/100 Mbps and duplex to half or full. Must coincide with switch port or no link will occur."
PhyPhoneSpeed                         = "Phoneline Transmit Speed"
PhyPhonePower                         = "Phoneline Power Level"
PhyGiladIfs                           = "Inter Frame Spacing"
IPSecEnabled                          = "Offload IP Security"
IPSecEnabledMiniHelp                  = "Saves CPU cycles when using IPSec."
ChecksumEnabled                       = "Offload TCP/IP Checksum"
ChecksumEnabledMiniHelp               = "Allows adapter to verify TCP/IP checksum on received packet, and compute checksum on transmitted packets. This improves TCP/IP performance."
LargeSendEnabled                      = "Offload TCP Segmentation"
LargeSendEnabledMiniHelp              = "Allows the adapter to offload the task of segmenting TCP messages and improves CPU utilization."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  = "Security Associations"
SecurityAssociationsMiniHelp          = "Simultaneous Security Associations that can be offloaded to the adapters co-processor."
AdaptivePerfTuning                    = "Adaptive Performance Tuning"
AdapterBandwidth                      = "Adapter Bandwidth"
CpuUtil                               = "CPU Utilization"
AdaptivePerfTuningMiniHelp            = "Sets optimal point of CPU/Adapter performance for this system.  See help."
WakeOnSettings                        = "Wake on Settings"
WakeOnLink                            = "Wake on Link Change"
WakeOnMagicPacket                     = "Wake on Magic Packet"
WakeOnMagicAndDirectedPackets 	      = "Wake on Magic & Directed"
WakeOnLAA                             = "Wake on LAA"
WakeOnArp                             = "Wake on ARP"
WakeOnDirected                        = "Wake on directed packet"
WakeOnNBT                             = "Wake on NBT Query"
WakeOnSettingsMiniHelp                = "Determines which packets can be enabled to Wake up the system (Direct Packets, Magic Packet etc.)."
ForceWakeOnLink                       = "Force Wake On Link"
ForceWakeOnLinkMiniHelp               = "When enabled, forces system to wake on link change"
EnablePME                             = "Enable PME"
EnablePMEMiniHelp                     = "Allows wake-up from APM power management when enabled. Disable shuts down LAN controller under ACPI"
SmartPowerDown                        = "Smart Power Down"
SmartPowerDownMiniHelp                = "Removes adapter power when LAN cable disconnected."
AdaptiveLinkResponse                  = "Adaptive Link Response"
AdaptiveLinkResponseMiniHelp          = "Enables Adaptive Link Response to check PHYLink status."
WakeOnLinkSettings                    = "Wake On Link Settings"
WakeOnLinkHelp                        = "Allows wake-up from APM power management when link is reconnected."


; Device descriptions
PCIE100B.DeviceDesc              = "Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            = "Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            = "Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            = "Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            = "Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               = "Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            = "82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               = "Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            = "Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           = "Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         = "Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            = "Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            = "Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         = "Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        = "Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           = "Intel(R) PRO/100+ Dual Port Server Adapter"


PCIE100AOL.DeviceDesc            = "Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         = "Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       = "Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       = "Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               = "Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            = "Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          = "Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              = "Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           = "Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           = "Intel(R) PRO/100 S Server Adapter"


PCIE100S0.DeviceDesc             = "Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             = "Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          = "Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          = "Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            = "Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            = "Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          = "Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        = "Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       = "Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           = "Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         = "Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       = "Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   = "Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         = "82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         = "Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     = "Intel(R) PRO/100 VM Network Connection"


PCIE100EMBLON.DeviceDesc         = "Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         = "Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          = "Intel(R) PRO/100 Dual Port Server Adapter"


PCIE100BSPLUSD.DeviceDesc        = "Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        = "Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  = "NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                = "Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                = "Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                = "Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                = "iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         = "Intel 8255x-based Fast Ethernet"


DL_EMBLOM.DeviceDesc             = "Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   = "Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0416] ; Brazilian Portuguese
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="Ativado"
Off                      ="Desativado"
Enabled                  ="Ativado"
Disabled                 ="Desativado"
AutoDetect               ="Detecção automática"
10Mb-Half-Duplex         ="10Mbps/Half duplex"
10Mb-Full-Duplex         ="10Mbps/Full duplex"
100Mb-Half-Duplex        ="100Mbps/Half duplex"
100Mb-Full-Duplex        ="100Mbps/Full duplex"
High                     ="Alto"
Low                      ="Baixo"
None                     ="Nenhum"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Gerar e responder"
Respond                  ="Responder"
Generate                 ="Gerar"
NoAction                 ="Nenhuma ação"
HardwareDefault          ="Hardware padrão"
OSControlled             ="Controlado por SO"
Forced                   ="Forçado"

; advanced tab strings
RxBuffers                             ="Descritores de recepção"
RxBuffersMiniHelp                     ="Número de buffers usados pelo driver ao copiar dados na memória do protocolo."
TxBuffers                             ="Descritores de transmissão"
TxBuffersMiniHelp                     ="Define o número de blocos de controle disponíveis para o adaptador usar."
CoalesceBuffers                       ="Buffers de coalescência"
CoalesceBuffersMiniHelp               ="Número de buffers disponíveis para a aceleração da transmissão."
AdaptiveIFS                           ="Espaçamento inter-frames adaptativo"
AdaptiveIFSMiniHelp                   ="Compensa as colisões excessivas de pacotes Ethernet controlando a temporização back-to-back."
AdaptiveTxThreshold                   ="Limiar adaptativo de transmissão"
AdaptiveTxThresholdMiniHelp           ="Define o número de bytes antes do adaptador esvaziar seu buffer de FIFO. O valor real é uma configuração de 8 vezes."
HPQPriorityLevelDef                   ="Definição do nível de prioridade"
HPQPriorityLevelDefMiniHelp           ="Define o limite de nível controlado para usar HPQ."
AdaptiveTechnology                    ="Tecnologia adaptativa"
AdaptiveTechnologyMiniHelp            ="Habilita/desabilita o recurso de desempenho da Tecnologia adaptativa."
PciBusEfficiency                      ="Eficiência do barramento PCI"
PciBusEfficiencyMiniHelp              ="Agrupa os pacotes de transmissão em um buffer único enviando-os para a rede. "
BasicConnectivity                     ="Conectividade para ambiente com poucos recursos"
BasicConnectivityMiniHelp             ="Experimente carregar o driver em ambiente de poucos recursos"
LocalyAdminAddress                    ="Endereço administrado localmente"
LocalyAdminAddressMiniHelp            ="Por padrão, o endereço não está presente e o campo de valor está em branco. Para definir o LAA no Intel(R) PROSet, digite-o no campo de valor. Nota: para definir o LAA no Device Manager, selecione a opção Valor e digite o endereço no campo correspondente."
RetransmitInterFrameSpace             ="Espaçamento inter-frames de retransmissão"
RetransmitInterFrameSpaceMiniHelp     ="Compensa as colisões excessivas de pacotes Ethernet controlando a temporização back-to-back."
LogLinkState                          ="Evento de estado de link de registro"
LogLinkStateMiniHelp                  ="Habilita/desabilita a mensagem de estado de link para o registrador"
QoSPacketTag                          ="Rotulação de pacotes de QoS"
QosPacketTagMiniHelp                  ="Envia e recebe frames rotuladas IEEE (802.3ac / 802.1p / 802.1Q)."
FlowControlSettings                   ="Configurações do controle de fluxo"
FlowControlSettingsMiniHelp           ="Pausa a transmissão de pacote na recepção de frame de controle de fluxo completo e envia frame de controle de fluxo completo para notificar o outro lado a fim de parar a transmissão."
SpeedDuplex                           ="Velocidade de link e duplex"
SpeedDuplex10MiniHelp                 ="Define a velocidade do link para 10 Mbps e duplex para half ou full. Deve coincidir com a porta do switch ou não ocorrerá nenhum link."
SpeedDuplexMiniHelp                   ="Define a velocidade do link para 10/100 Mbps e duplex para half ou full. Deve coincidir com a porta do switch ou não ocorrerá nenhum link."
PhyPhoneSpeed                         ="Velocidade de transmissão da linha telefônica"
PhyPhonePower                         ="Nível de potência da linha telefônica"
PhyGiladIfs                           ="Espaçamento inter-frames"
IPSecEnabled                          ="Offload Segurança de IP"
IPSecEnabledMiniHelp                  ="Salva os ciclos da CPU ao usar IPSec."
ChecksumEnabled                       ="Offload Checksum de TCP/IP"
ChecksumEnabledMiniHelp               ="Permite ao adaptador verificar a checksum de TCP/IP dos pacotes recebidos e computa a checksum nos pacotes transmitidos. Isso melhora o desempenho de TCP/IP."
LargeSendEnabled                      ="Offload Segmentação de TCP"
LargeSendEnabledMiniHelp              ="Permite ao adaptador fazer offload da tarefa de segmentar mensagens de TCP e melhora a utilização da CPU."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Associações de segurança"
SecurityAssociationsMiniHelp          ="Associações simultâneas de segurança que podem ser descarregados no coprocessador do adaptador."
AdaptivePerfTuning                    ="Ajuste adaptativo de desempenho"
AdapterBandwidth                      ="Largura de banda do adaptador"
CpuUtil                               ="Utilização da CPU"
AdaptivePerfTuningMiniHelp            ="Define o ponto otimizado de desempenho da CPU/adaptador para este sistema. Consulte a ajuda."
WakeOnSettings                        ="Configurações de ativação"
WakeOnLink                            ="Ativar com mudança de link"
WakeOnMagicPacket                     ="Ativar com Magic Packet"
WakeOnLAA                             ="Ativar com LAA"
WakeOnArp                             ="Ativar com ARP"
WakeOnDirected                        ="Ativar com pacote dirigido"
WakeOnMagicAndDirectedPackets 	      ="Ativar com pacotes Magic e Dirigidos"
WakeOnNBT                             ="Ativar com consulta NBT"
WakeOnSettingsMiniHelp                ="Determina quais pacotes podem ser habilitados para ativar o sistema (Magic packet, Pacotes dirigidos, etc.)."
ForceWakeOnLink                       ="Forçar ativação com mudança de link"
ForceWakeOnLinkMiniHelp               ="Se for habilitado, ele força a ativação do sistema com a mudança do link"
EnablePME                             ="Habilitar PME"
EnablePMEMiniHelp                     ="Permite a ativação do gerenciamento de energia APM quando habilitado. A desabilitação desliga o controlador de LAN no ACPI"
SmartPowerDown                        ="Desativação inteligente"
SmartPowerDownMiniHelp                ="Remove a energia do adaptador quando o cabo de LAN é desconectado."
AdaptiveLinkResponse                  ="Resposta do link adaptativa"
AdaptiveLinkResponseMiniHelp          ="Habilita a Resposta de link adaptativa para verificar o status de PHYLink."
WakeOnLinkSettings                    ="Configurações de Wake On Link (ativação por link)"
WakeOnLinkHelp                        ="Permite a ativação pelo gerenciamento de energia APM quando o link é reconectado."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0c0a] ; Castilian Spanish
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="Activado"
Off                      ="Desactivado"
Enabled                  ="Activado"
Disabled                 ="Desactivado"
AutoDetect               ="Detección automática"
10Mb-Half-Duplex         ="10Mbps/Dúplex medio"
10Mb-Full-Duplex         ="10Mbps/Dúplex completo"
100Mb-Half-Duplex        ="100Mbps/Dúplex medio"
100Mb-Full-Duplex        ="100Mbps/Dúplex completo"
High                     ="Alto"
Low                      ="Bajo"
None                     ="Ninguno"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Generar y responder"
Respond                  ="Responder"
Generate                 ="Generar"
NoAction                 ="Ninguna acción"
HardwareDefault          ="Predeterminada del hardware"
OSControlled             ="Controlado por el SO"
Forced                   ="Forzado"

; advanced tab strings
RxBuffers                             ="Descriptores de recepción"
RxBuffersMiniHelp                     ="Número de búferes utilizados por el controlador cuando se copian datos a la memoria del protocolo."
TxBuffers                             ="Descriptores de transmisión"
TxBuffersMiniHelp                     ="Establece el número de bloques de control disponibles para que los utilice el adaptador."
CoalesceBuffers                       ="Búferes de unión"
CoalesceBuffersMiniHelp               ="Número de búferes disponibles para la aceleración de la transmisión."
AdaptiveIFS                           ="Separación entre tramas ajustable"
AdaptiveIFSMiniHelp                   ="Compensa las colisiones excesivas de paquetes Ethernet mediante el control de intervalos consecutivos."
AdaptiveTxThreshold                   ="Umbral de transmisión ajustable"
AdaptiveTxThresholdMiniHelp           ="Establece el número de bytes antes de que el adaptador vacíe su búfer FIFO. El valor real es 8 veces el valor de configuración."
HPQPriorityLevelDef                   ="Definición de niveles de prioridad"
HPQPriorityLevelDefMiniHelp           ="Establece el nivel controlado de detención para el uso de HPQ."
AdaptiveTechnology                    ="Tecnología ajustable"
AdaptiveTechnologyMiniHelp            ="Activa o desactiva la función de rendimiento de la Tecnología ajustable."
PciBusEfficiency                      ="Eficiencia del bus PCI"
PciBusEfficiencyMiniHelp              ="Une los paquetes de transmisión en un solo búfer antes de enviarlos a la red."
BasicConnectivity                     ="Conectividad de recursos reducidos"
BasicConnectivityMiniHelp             ="Intenta cargar el controlador en entorno con pocos recursos."
LocalyAdminAddress                    ="Dirección administrada localmente"
LocalyAdminAddressMiniHelp            ="De manera predeterminada, la dirección no está presente y el campo de valor se encuentra en blanco. Para establecer un LAA en Intel(R) PROSet, introduzca uno en el campo de valor. Nota: Para establecer un LAA en el Administrador de dispositivos, seleccione la opción de valor e introduzca una dirección en el campo indicado."
RetransmitInterFrameSpace             ="Separación entre tramas de retransmisiones"
RetransmitInterFrameSpaceMiniHelp     ="Compensa las colisiones excesivas de paquetes Ethernet mediante el control de intervalos de retransmisión."
LogLinkState                          ="Registrar suceso de estado de enlace"
LogLinkStateMiniHelp                  ="Activa o desactiva el mensaje de estado de enlace para el que registra."
QoSPacketTag                          ="Etiquetado de paquete QoS"
QosPacketTagMiniHelp                  ="Tramas de envío y recepción con etiqueta IEEE (802.3ac / 802.1p / 802.1Q)."
FlowControlSettings                   ="Configuración del control de flujo"
FlowControlSettingsMiniHelp           ="Detiene la transmisión de paquetes al recibir una trama de control de flujo completo y envía una trama de control de flujo completo para notificar al asociado que detenga la transmisión."
SpeedDuplex                           ="Velocidad y dúplex del enlace"
SpeedDuplex10MiniHelp                 ="Establece la velocidad del enlace en 10 Mbps y el dúplex en medio o completo. Debe coincidir con el puerto conmutador para que se realice el enlace."
SpeedDuplexMiniHelp                   ="Establece la velocidad del enlace en 10/100 Mbps y el dúplex en medio o completo. Debe coincidir con el puerto conmutador para que se realice el enlace."
PhyPhoneSpeed                         ="Velocidad de transmisión de la línea telefónica"
PhyPhonePower                         ="Nivel de potencia de la línea telefónica"
PhyGiladIfs                           ="Separación entre tramas"
IPSecEnabled                          ="Descarga de Seguridad IP"
IPSecEnabledMiniHelp                  ="Guarda los ciclos CPU cuando utiliza IPSec."
ChecksumEnabled                       ="Descarga suma de verific. TCP/IP"
ChecksumEnabledMiniHelp               ="Permite que el adaptador verifique la suma de verificación TCP/IP de los paquetes recibidos y calcula la suma de verificación de los paquetes transmitidos. Mejora el rendimiento de TCP/IP."
LargeSendEnabled                      ="Descarga de Segmentación TCP "
LargeSendEnabledMiniHelp              ="Permite que el adaptador descargue la tarea de segmentación de mensajes TCP y mejora el uso de la CPU."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Asociaciones de seguridad"
SecurityAssociationsMiniHelp          ="Asociaciones de seguridad simultáneas que pueden descargarse a el coprocesador del adaptador."
AdaptivePerfTuning                    ="Optimización de rendimiento ajustable"
AdapterBandwidth                      ="Ancho de banda del adaptador"
CpuUtil                               ="Uso de la CPU"
AdaptivePerfTuningMiniHelp            ="Establece el punto óptimo del rendimiento de la CPU y el adaptador para este sistema. Consulte la Ayuda."
WakeOnSettings                        ="Configuración Wake on (activación)"
WakeOnLink                            ="Activar en cambio de enlace"
WakeOnMagicPacket                     ="Activar en Magic Packet"
WakeOnLAA                             ="Activar en LAA"
WakeOnArp                             ="Activar en ARP"
WakeOnDirected                        ="Activar en Paquete dirigido"
WakeOnMagicAndDirectedPackets 	      ="Activar en Magic y Dirigidos"
WakeOnNBT                             ="Activar en consulta NBT"
WakeOnSettingsMiniHelp                ="Determina cuáles paquetes pueden ser habilitados para la activación del sistema (Direct Packets, Magic Packet, etc.)."
ForceWakeOnLink                       ="Forzar Activación en enlace"
ForceWakeOnLinkMiniHelp               ="Cuando se activa, fuerza al sistema a activarse al efectuarse un cambio de enlace."
EnablePME                             ="Activar PME"
EnablePMEMiniHelp                     ="Cuando se activa, permite la activación desde la administración de energía APM. Cuando se desactiva, apaga el controlador de red local bajo ACPI"
SmartPowerDown                        ="Apagado inteligente"
SmartPowerDownMiniHelp                ="Quita la energía del adaptador cuando se desconecta el cable de red local."
AdaptiveLinkResponse                  ="Respuesta de enlace ajustable"
AdaptiveLinkResponseMiniHelp          ="Activa la respuesta de enlace ajustable para verificar el estado de PHYLink."
WakeOnLinkSettings                    ="Configuración Wake On Link"
WakeOnLinkHelp                        ="Cuando se reconecta el enlace,  permite la activación desde la administración de energía APM."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0804] ; ChineseSimplified
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\system32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="开"
Off                      ="关"
Enabled                  ="已启用"
Disabled                 ="已禁用"
AutoDetect               ="自动检测"
10Mb-Half-Duplex         ="10Mbps/半双工"
10Mb-Full-Duplex         ="10Mbps/全双工"
100Mb-Half-Duplex        ="100Mbps/半双工"
100Mb-Full-Duplex        ="100Mbps/全双工"
High                     ="高"
Low                      ="低"
None                     ="无"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="生成和响应"
Respond                  ="响应"
Generate                 ="生成"
NoAction                 ="无操作"
HardwareDefault          ="硬件默认"
OSControlled             ="控制操作系统"
Forced                   ="强制"

; advanced tab strings
RxBuffers                             ="接收描述符"
RxBuffersMiniHelp                     ="将数据复制至协议内存中时驱动程序使用的缓冲区数。"
TxBuffers                             ="传输描述符"
TxBuffersMiniHelp                     ="设置供适配器使用的控制块数。"
CoalesceBuffers                       ="接合缓冲区"
CoalesceBuffersMiniHelp               ="可用于传输加速的缓冲区数。"
AdaptiveIFS                           ="适应性帧间距调整"
AdaptiveIFSMiniHelp                   ="通过控制背靠背定时来补偿过多的以太网数据包碰撞。"
AdaptiveTxThreshold                   ="适应性传输阈值"
AdaptiveTxThresholdMiniHelp           ="设置适配器清空其 FIFO 缓冲区之前的字节数。实际值为设置值的 8 倍。"
HPQPriorityLevelDef                   ="优先性级别定义"
HPQPriorityLevelDefMiniHelp           ="设置使用高优先队列(HPQ)的受控截止级。"
AdaptiveTechnology                    ="适应性技术"
AdaptiveTechnologyMiniHelp            ="启用/禁用适应性技术性能功能"
PciBusEfficiency                      ="PCI 总线效率"
PciBusEfficiencyMiniHelp              ="在将进入单一缓冲区的接合传输数据包发送至网络之前的数据包数。"
BasicConnectivity                     ="低资源时的连接性"
BasicConnectivityMiniHelp             ="尝试在低资源环境下加载驱动程序"
LocalyAdminAddress                    ="本地管理的地址"
LocalyAdminAddressMiniHelp            ="默认情况下，地址不存在，而且值字段为空。若要在英特尔(R) PROSet 中设定 LAA，将其输入值字段。注意：若要在 "设备管理器" 中设定 LAA，选择 "值" 选项，并在提供的字段中输入一个地址。"
RetransmitInterFrameSpace             ="重新传输帧间距调整"
RetransmitInterFrameSpaceMiniHelp     ="通过控制重新传输定时来补偿过多的以太网数据包碰撞。"
LogLinkState                          ="记录链接状态事件"
LogLinkStateMiniHelp                  ="启用/禁用将链接状态消息记入日志。"
QoSPacketTag                          ="QoS 数据包标签"
QosPacketTagMiniHelp                  ="发送和接收 IEEE 标签帧（802.3ac / 802.1p / 802.1Q）。"
FlowControlSettings                   ="流程控制设置"
FlowControlSettingsMiniHelp           ="在接收到流程控制帧满时暂停数据包传输，并发送流程控制帧以满信息以通知对方停止传输。"
SpeedDuplex                           ="链接速度和双工"
SpeedDuplex10MiniHelp                 ="设置链接速度为 10 Mbps 及双工模式为半工或全工。必须与交换器端口设置相符，否则无链接。"
SpeedDuplexMiniHelp                   ="设置链接速度为 10/100 Mbps 及双工模式为半工或全工。必须与交换器端口设置相符，否则无链接。"
PhyPhoneSpeed                         ="电话线传输速度"
PhyPhonePower                         ="电话线电源级别"
PhyGiladIfs                           ="帧间距调整"
IPSecEnabled                          ="分载 IP 安全性"
IPSecEnabledMiniHelp                  ="使用 IPSec 时保存 CPU 周期。"
ChecksumEnabled                       ="分载传输 TCP/IP 校验和"
ChecksumEnabledMiniHelp               ="允许适配器验证接收到的数据包的 TCP/IP 校验和，并计算传输的数据包的校验和。这可提高 TCP/IP 性能。"
LargeSendEnabled                      ="分载 TCP 分段"
LargeSendEnabledMiniHelp              ="允许适配器分载对 TCP消息分段的工作量，并提高 CPU 利用率。"
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="安全性联合"
SecurityAssociationsMiniHelp          ="同步安全性联合可分载至适配器的协处理器。"
AdaptivePerfTuning                    ="适应性性能调整"
AdapterBandwidth                      ="适配器带宽"
CpuUtil                               ="CPU利用率"
AdaptivePerfTuningMiniHelp            ="为本系统设置 CPU/适配器性能最佳点。参阅“帮助”。"
WakeOnSettings                        ="唤醒设置"
WakeOnLink                            ="唤醒链接更改"
WakeOnMagicPacket                     ="唤醒魔包"
WakeOnLAA                             ="唤醒本地管理地址(LAA)"
WakeOnArp                             ="唤醒地址解析协议(ARP)"
WakeOnDirected                        ="唤醒定向数据包"
WakeOnMagicAndDirectedPackets 	      ="唤醒魔包或定向数据包"
WakeOnNBT                             ="唤醒 NBT 查询"
WakeOnSettingsMiniHelp                ="决定可启用哪些数据包来唤醒系统（直接数据包、魔包等）。"
ForceWakeOnLink                       ="强制唤醒链接"
ForceWakeOnLinkMiniHelp               ="启用时，强制系统在链接更改时唤醒"
EnablePME                             ="启用 PME"
EnablePMEMiniHelp                     ="启用时允许从 APM 电源管理唤醒。禁用时关闭 ACPI 下的 LAN 控制器"
SmartPowerDown                        ="机智关闭电源"
SmartPowerDownMiniHelp                ="在 LAN 电缆断开时除去适配器电源。"
AdaptiveLinkResponse                  ="适应性链接响应"
AdaptiveLinkResponseMiniHelp          ="起用适应性链接响应以检查 PHYLink（物理层链接）状态。"
WakeOnLinkSettings                    ="唤醒链接设置"
WakeOnLinkHelp                        ="允许在链接有连接时从 APM 电源管理唤醒。"


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0404] ; Chinese Traditional
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="開啟"
Off                      ="關閉"
Enabled                  ="啟用"
Disabled                 ="停用"
AutoDetect               ="自動偵測"
10Mb-Half-Duplex         ="10Mbps∕半雙工"
10Mb-Full-Duplex         ="10Mbps∕全雙工"
100Mb-Half-Duplex        ="100Mbps∕半雙工"
100Mb-Full-Duplex        ="100Mbps∕全雙工"
High                     ="高"
Low                      ="低"
None                     ="無"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="產生與回應"
Respond                  ="回應"
Generate                 ="產生"
NoAction                 ="無動作"
HardwareDefault          ="硬體預設值"
OSControlled             ="受控的作業系統"
Forced                   ="強迫"

; advanced tab strings
RxBuffers                             ="接收描述器"
RxBuffersMiniHelp                     ="複製資料到通訊協定記憶體時，驅動程式使用的緩衝區數目。"
TxBuffers                             ="傳輸描述器"
TxBuffersMiniHelp                     ="設定介面卡可使用的控制區塊數。"
CoalesceBuffers                       ="結合緩衝區"
CoalesceBuffersMiniHelp               ="可用於傳輸加速的緩衝區數。"
AdaptiveIFS                           ="介面式框架內間隔"
AdaptiveIFSMiniHelp                   ="控制連續計時來補償過度的 Ethernet 封包衝突。"
AdaptiveTxThreshold                   ="介面式傳送閾值"
AdaptiveTxThresholdMiniHelp           ="介面卡清空其 FIFO 緩衝區之前設定的位元組數。實際值是 8 乘以設定值。"
HPQPriorityLevelDef                   ="優先層級定義"
HPQPriorityLevelDefMiniHelp           ="設定使用 HPQ 的控制停止層級。"
AdaptiveTechnology                    ="介面科技"
AdaptiveTechnologyMiniHelp            ="啟用∕停用介面科技效用功能。"
PciBusEfficiency                      ="PCI 匯流排效率"
PciBusEfficiencyMiniHelp              ="封包傳送到網路之前將傳輸封包結合到單一緩衝區。"
BasicConnectivity                     ="低資源連線"
BasicConnectivityMiniHelp             ="在低資源環境嘗試載入驅動程式。"
LocalyAdminAddress                    ="本地管理位址"
LocalyAdminAddressMiniHelp            ="依照預設，位址不會存在，值欄位會留成空白。在 Intel(R) PROSet 中設定 LAA，請在值欄位輸入一個。注意：要在「裝置管理員」中設定 LAA，請選取「值」選項，並在提供的欄位中輸入一個位址。"
RetransmitInterFrameSpace             ="重新傳輸框架內間隔"
RetransmitInterFrameSpaceMiniHelp     ="控制重新傳輸計時來補償過度的 Ethernet 封包衝突。"
LogLinkState                          ="登錄連結狀態事件"
LogLinkStateMiniHelp                  ="啟用∕停用登錄器的連結狀態訊息。"
QoSPacketTag                          ="QoS 封包標籤"
QosPacketTagMiniHelp                  ="傳送和接收 IEEE 標示的框架（802.3ac / 802.1p / 802.1Q）。"
FlowControlSettings                   ="流程控制設定值"
FlowControlSettingsMiniHelp           ="接收到全速流程控制框架時“暫停”封包傳輸，並“傳送”全速流程框架以通知另外一方停止傳輸。"
SpeedDuplex                           ="連結速度與雙工"
SpeedDuplex10MiniHelp                 ="將連結速度設為 10 Mbps，並將雙工處理設為半雙工或全雙工。一定要與開關連接埠相符，否則就無法連結。"
SpeedDuplexMiniHelp                   ="將連結速度設為 10/100 Mbps，並將雙工處理設為半雙工或全雙工。一定要與開關連接埠相符，否則就無法連結。"
PhyPhoneSpeed                         ="電話線傳輸速度"
PhyPhonePower                         ="電話線電源程度"
PhyGiladIfs                           ="框架內間隔"
IPSecEnabled                          ="卸載 IP 保全性"
IPSecEnabledMiniHelp                  ="使用 IPSec 時，儲存 CPU 週期。"
ChecksumEnabled                       ="卸載 TCP/IP 總值"
ChecksumEnabledMiniHelp               ="允許介面卡驗證接收封包上的 TCP/IP 總值，並計算傳輸封包上的總值。如此可以改善 TCP/IP 的效能。"
LargeSendEnabled                      ="卸載 TCP 區段"
LargeSendEnabledMiniHelp              ="允許介面卡卸載區段處理 TCP 訊息的工作並改善 CPU 的使用。"
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="保全性關聯"
SecurityAssociationsMiniHelp          ="可以卸載到介面卡輔助處理器的同步保全性關聯。"
AdaptivePerfTuning                    ="介面效能調整"
AdapterBandwidth                      ="介面卡頻寬"
CpuUtil                               ="CPU 的使用"
AdaptivePerfTuningMiniHelp            ="為此系統設定 CPU∕介面卡效能的最佳點。請參閱「說明」。"
WakeOnSettings                        ="喚醒設定"
WakeOnLink                            ="喚醒連結變更"
WakeOnMagicPacket                     ="喚醒神奇封包"
WakeOnLAA                             ="喚醒 LAA"
WakeOnArp                             ="喚醒 ARP "
WakeOnDirected                        ="喚醒直接封包"
WakeOnMagicAndDirectedPackets 	      ="喚醒神奇封包和直接封包"
WakeOnNBT                             ="喚醒 NBT 查詢"
WakeOnSettingsMiniHelp                ="決定可以啟用哪個封包來喚醒該系統（直接封包、神奇封包、等等）。"
ForceWakeOnLink                       ="強迫“喚醒連結” "
ForceWakeOnLinkMiniHelp               ="啟用時，強迫系統在連結變更時喚醒"
EnablePME                             ="啟用 PME"
EnablePMEMiniHelp                     ="啟用時，允許從 APM 電源管理喚醒。在 ACPI 下停止關閉 LAN 控制器"
SmartPowerDown                        ="自動電源關閉"
SmartPowerDownMiniHelp                ="斷開 LAN 纜線時，移除介面卡的電源。"
AdaptiveLinkResponse                  ="介面連結回應"
AdaptiveLinkResponseMiniHelp          ="啟用介面連結回應來檢查實體階層的連結狀態。"
WakeOnLinkSettings                    ="喚醒連結設定"
WakeOnLinkHelp                        ="重新連結時，允許從 APM 電源管理喚醒。"


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0406] ; Danish
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="Til"
Off                      ="Fra"
Enabled                  ="Aktiveret"
Disabled                 ="Deaktiveret"
AutoDetect               ="Autogenkend"
10Mb-Half-Duplex         ="10Mbps/halv duplex"
10Mb-Full-Duplex         ="10Mbps/fuld duplex"
100Mb-Half-Duplex        ="100Mbps/halv duplex"
100Mb-Full-Duplex        ="100Mbps/fuld duplex"
High                     ="Høj"
Low                      ="Lav"
None                     ="Ingen"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Generer og svar"
Respond                  ="Svar"
Generate                 ="Generer"
NoAction                 ="Ingen handling"
HardwareDefault          ="Hardwarestandard"
OSControlled             ="OS-styret"
Forced                   ="Tvunget"

; advanced tab strings
RxBuffers                             ="Beskrivelser for modtagelse"
RxBuffersMiniHelp                     ="Antal buffere der anvendes af driveren under kopiering af data til protokolhukommelse."
TxBuffers                             ="Beskrivelser for overførsel"
TxBuffersMiniHelp                     ="Indstiller antallet af kontrolblokke, der er til rådighed for adapteren."
CoalesceBuffers                       ="Coalesce-bufferer"
CoalesceBuffersMiniHelp               ="Antal buffere til rådighed til transmissionsaccelleration."
AdaptiveIFS                           ="Adap. inter-rammeafstand"
AdaptiveIFSMiniHelp                   ="Kompenserer for uforholdsmæssigt mange Ethernet-pakkekollisioner ved at kontrollere back-to-back timingen."
AdaptiveTxThreshold                   ="Adap. trans. stærskelværdi"
AdaptiveTxThresholdMiniHelp           ="Indstiller antallet af bytes inden adapteren tømmer sin FIFO-buffer. Aktuel værdi er 8 gange indstilling."
HPQPriorityLevelDef                   ="Definition af prioritetsniveau"
HPQPriorityLevelDefMiniHelp           ="Indstiller det kontrollerede afskæringsniveau for brug af HPQ (højprioritetskø)."
AdaptiveTechnology                    ="Adaptiv teknologi"
AdaptiveTechnologyMiniHelp            ="Aktiverer/deaktiverer ydelsesfunktionen Adaptiv teknologi"
PciBusEfficiency                      ="PCI-buseffektivitet"
PciBusEfficiencyMiniHelp              ="Sammenlægger transmissionspakker i en enkelt buffer, inden de sendes til netværket."
BasicConnectivity                     ="Konnektivitet lave ressourcer"
BasicConnectivityMiniHelp             ="Prøv at indlæse driveren i det lave ressourcemiljø."
LocalyAdminAddress                    ="Lokalt administreret adresse"
LocalyAdminAddressMiniHelp            ="Som standard er en adresse ikke tilstede, og værdifeltet er tomt. Indstil en LAA i Intel(R) PROSet ved at indtaste en værdi i værdifeltet. Bemærk: For at indstille LAA i Enhedsstyring skal du vælge indstillingen Værdi, og indtaste en adresse i feltet."
RetransmitInterFrameSpace             ="Retrans. inter-rammeafstand"
RetransmitInterFrameSpaceMiniHelp     ="Kompenserer for uforholdsmæssigt mange Ethernet-pakkekollisioner ved at kontrollere retransmissionstimingen."
LogLinkState                          ="Log Link tilstandshændelse"
LogLinkStateMiniHelp                  ="Aktiverer/deaktiverer linktilstandsmeddelelsen til logger."
QoSPacketTag                          ="QoS-pakkemærkning"
QosPacketTagMiniHelp                  ="Send og modtag IEEE-mærkede rammer (802.3ac / 802.1p / 802.1Q)."
FlowControlSettings                   ="Flow Control-indstillinger"
FlowControlSettingsMiniHelp           ="Standser pakketransmission ved modtagelse af fuld flow-kontrol-ramme og Send fuld flow-kontrol-ramme, for at få den anden part til at standse transmissionen."
SpeedDuplex                           ="Linkhastighed og duplex"
SpeedDuplex10MiniHelp                 ="Indstiller linkhastigheden til 10 Mbps og duplex til halv eller fuld. Skal stemme overens med switch-port, ellers vil der ikke ske linkning."
SpeedDuplexMiniHelp                   ="Indstiller linkhastigheden til 10/100 Mbps og duplex til halv eller fuld. Skal stemme overens med switch-port, ellers vil der ikke ske linkning."
PhyPhoneSpeed                         ="Telefon trans.-hastighed"
PhyPhonePower                         ="Telefon spændingsniveau"
PhyGiladIfs                           ="Inter-rammeafstand"
IPSecEnabled                          ="Aflast IP-sikkerhed"
IPSecEnabledMiniHelp                  ="Gemmer CPU-cyklusser ved brug af IPSec."
ChecksumEnabled                       ="Aflast TCP/IP-checksum"
ChecksumEnabledMiniHelp               ="Tillader adapteren at kontrollere TCP/IP-checksummen for modtagne pakker og beregne checksummen for overførte pakker. Dette forbedrer TCP/IP-ydelsen."
LargeSendEnabled                      ="Fjern TCP-segmentering"
LargeSendEnabledMiniHelp              ="Tillader adapteren at aflaste segmentering af TCP-meddelelser og forbedrer CPU-udnyttelsen."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Sikkerhedstilknytninger"
SecurityAssociationsMiniHelp          ="Samtidige sikkerhedstilknytninger, der kan aflastes til adapterens co-processor."
AdaptivePerfTuning                    ="Adaptiv ydelsestuning"
AdapterBandwidth                      ="Adapter- båndbredde"
CpuUtil                               ="CPU-udnyttelse"
AdaptivePerfTuningMiniHelp            ="Indstiller det optimale punkt for CPU/adapterydelse for dette system. Se Hjælp."
WakeOnSettings                        ="Væk på-indstillinger"
WakeOnLink                            ="Væk på Link Change"
WakeOnMagicPacket                     ="Væk på Magic Packet"
WakeOnLAA                             ="Væk på LAA (lokalt administreret adresse)"
WakeOnArp                             ="Væk på ARP"
WakeOnDirected                        ="Væk på Directed Packet"
WakeOnMagicAndDirectedPackets 	      ="Væk på Magic & Directed"
WakeOnNBT                             ="Væk på NBT-forespørgsel"
WakeOnSettingsMiniHelp                ="Bestemmer hvordan systemet vækkes (Direct Packets, Magic Packets, mv.)."
ForceWakeOnLink                       ="Gennemtving Væk på link"
ForceWakeOnLinkMiniHelp               ="Ved aktivering tvinges systemet til Væk på link change"
EnablePME                             ="Aktiver PME"
EnablePMEMiniHelp                     ="Tillader ved aktivering opvågning fra APM-strømstyring. Deaktiverer nedlukning af LAN-controller under ACPI."
SmartPowerDown                        ="Smart strømnedlukning"
SmartPowerDownMiniHelp                ="Slukker for strøm til adapteren, hvis LAN-kablet afbrydes."
AdaptiveLinkResponse                  ="Adaptivt link-svar"
AdaptiveLinkResponseMiniHelp          ="Aktiverer adaptivt link-svar for kontrol af PH-link status."
WakeOnLinkSettings                    ="Væk på link-indstillinger"
WakeOnLinkHelp                        ="Tillader opvågning fra APM-strømstyring, når link gentilsluttes."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0413] ; Dutch
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\system32\drivers\e100bnt5.sys"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="Aan"
Off                      ="Uit"
Enabled                  ="Ingeschakeld"
Disabled                 ="Uitgeschakeld"
AutoDetect               ="Autodetectie"
10Mb-Half-Duplex         ="10 Mbps/half-duplex"
10Mb-Full-Duplex         ="10 Mbps/full-duplex"
100Mb-Half-Duplex        ="100 Mbps/half-duplex"
100Mb-Full-Duplex        ="100 Mbps/full-duplex"
High                     ="Hoog"
Low                      ="Laag"
None                     ="Geen"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Genereren en antwoorden"
Respond                  ="Antwoorden"
Generate                 ="Genereren"
NoAction                 ="Geen actie"
HardwareDefault          ="Hardwarestandaard"
OSControlled             ="Beheerd door besturingssysteem"
Forced                   ="Geforceerd"

; advanced tab strings
RxBuffers                             ="Ontvangst-descriptors"
RxBuffersMiniHelp                     ="Het aantal buffers dat het stuurprogramma gebruikt bij het kopiëren van gegevens naar het protocolgeheugen."
TxBuffers                             ="Verzend-descriptors"
TxBuffersMiniHelp                     ="Hiermee wordt het aantal controleblokken ingesteld dat beschikbaar is voor gebruik door de adapter."
CoalesceBuffers                       ="Coalesce-buffers"
CoalesceBuffersMiniHelp               ="Het aantal beschikbare buffers om het verzenden te versnellen."
AdaptiveIFS                           ="Adaptieve afstand tussen frames"
AdaptiveIFSMiniHelp                   ="Compenseert overmatige Ethernet-pakketconflicten via beheer van back to back-timing."
AdaptiveTxThreshold                   ="Adaptieve drempelwaarde verzending"
AdaptiveTxThresholdMiniHelp           ="Hiermee wordt het aantal bytes ingesteld dat kan worden bereikt voordat de FIFO-buffer van de adapter wordt leeggemaakt. De feitelijke waarde is 8 maal de instelling."
HPQPriorityLevelDef                   ="Definitie prioriteitsniveau"
HPQPriorityLevelDefMiniHelp           ="Hiermee wordt het gecontroleerde begrenzingsniveau ingesteld voor het gebruik van HPQ."
AdaptiveTechnology                    ="Adaptieve technologie"
AdaptiveTechnologyMiniHelp            ="Hiermee wordt de prestatiemetingsfunctie voor adaptieve technologie in- of uitgeschakeld."
PciBusEfficiency                      ="Efficiëntie PCI-bus"
PciBusEfficiencyMiniHelp              ="Hiermee worden verzendpakketten samengevoegd tot één buffer voordat deze naar het netwerk worden verzonden."
BasicConnectivity                     ="Verbindingen bij weinig resources"
BasicConnectivityMiniHelp             ="Probeer het stuurprogramma te laden in een omgeving met weinig resources."
LocalyAdminAddress                    ="Lokaal beheerd adres"
LocalyAdminAddressMiniHelp            ="Standaard is er geen adres aanwezig en wordt het veld leeg gelaten. Om een lokaal beheerd adres in te stellen in Intel(R) PROSet, geeft u een adres op in het veld. Opmerking: Om een lokaal beheerd adres in te stellen in Apparaatbeheer, selecteert u de optie Waarde en geeft u een adres op in het daarvoor bestemde veld."
RetransmitInterFrameSpace             ="Afstand tussen frames bij opnieuw verzenden"
RetransmitInterFrameSpaceMiniHelp     ="Compenseert overmatige Ethernet-pakketconflicten via het beheer van de timing bij opnieuw verzenden."
LogLinkState                          ="Gebeurtenis verbindingsstatus vastleggen"
LogLinkStateMiniHelp                  ="Vastleggen van berichten over verbindingsstatus in logboek in- of uitschakelen."
QoSPacketTag                          ="Codering QoS-pakketten"
QosPacketTagMiniHelp                  ="Frames met IEEE-markeringen (802.3ac / 802.1p / 802.1Q) verzenden en ontvangen."
FlowControlSettings                   ="Instellingen datatransportbesturing"
FlowControlSettingsMiniHelp           ="Onderbreekt pakketverzending bij ontvangst van volledig datatransportbesturingsframe en verzendt volledig datatransportbesturingsframe om de andere zijde te vragen de verzending te stoppen."
SpeedDuplex                           ="Verbindingssnelheid & duplex"
SpeedDuplex10MiniHelp                 ="Hiermee wordt de verbindingssnelheid ingesteld op 10 Mbps en de duplexmodus op half- of full-duplex. Moet overeenstemmen met de instellingen van de switchpoort, anders wordt geen verbinding tot stand gebracht."
SpeedDuplexMiniHelp                   ="Hiermee wordt de verbindingssnelheid ingesteld op 10/100 Mbps en de duplexmodus op half- of full-duplex. Moet overeenstemmen met de instellingen van de switchpoort, anders wordt geen verbinding tot stand gebracht."
PhyPhoneSpeed                         ="Zendsnelheid telefoonlijn"
PhyPhonePower                         ="Energieniveau telefoonlijn"
PhyGiladIfs                           ="Afstand tussen frames"
IPSecEnabled                          ="Offload IP-beveiliging"
IPSecEnabledMiniHelp                  ="Bespaart CPU-cycli wanneer IPSec wordt gebruikt."
ChecksumEnabled                       ="Offload TCP/IP-checksum"
ChecksumEnabledMiniHelp               ="Hiermee kan de adapter de TCP/IP-controlesom van een ontvangen pakket verifiëren en de controlesom van verzonden pakketten berekenen. Dit komt ten goede van de TCP/IP-prestaties."
LargeSendEnabled                      ="Offload TCP-segmentatie"
LargeSendEnabledMiniHelp              ="Hiermee kan de adapter het segmenteren van TCP-berichten offloaden en wordt het CPU-gebruik verbeterd."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Beveiligingskoppelingen"
SecurityAssociationsMiniHelp          ="Gelijktijdige beveiligingskoppelingen die kunnen worden overgenomen door de coprocessor van de adapter."
AdaptivePerfTuning                    ="Adaptieve prestatieafstemming"
AdapterBandwidth                      ="Bandbreedte adapter"
CpuUtil                               ="CPU-gebruik"
AdaptivePerfTuningMiniHelp            ="Hiermee wordt het optimale punt ingesteld voor CPU/adapter-prestaties voor dit systeem. Raadpleeg de Help."
WakeOnSettings                        ="Wake on-instellingen"
WakeOnLink                            ="Wake on bij verbindingswijziging"
WakeOnMagicPacket                     ="Wake on bij Magic Packet"
WakeOnLAA                             ="Wake on LAA"
WakeOnArp                             ="Wake on ARP"
WakeOnDirected                        ="Wake on bij gericht pakket"
WakeOnMagicAndDirectedPackets 	      ="Wake on bij Magic Packets en gerichte pakketten"
WakeOnNBT                             ="Wake on NBT Query"
WakeOnSettingsMiniHelp                ="Hiermee bepaalt u met welke pakketten het systeem wordt geactiveerd (Direct Packets, Magic Packets, enzovoort)."
ForceWakeOnLink                       ="Wake on-koppeling forceren"
ForceWakeOnLinkMiniHelp               ="Indien ingeschakeld, wordt de activering van het systeem geforceerd bij een verbindingswijziging"
EnablePME                             ="PME inschakelen"
EnablePMEMiniHelp                     ="Maakt activering bij APM-energiebeheer mogelijk indien ingeschakeld. Schakelt de LAN-controller uit onder ACPI, indien uitgeschakeld."
SmartPowerDown                        ="Slim uitschakelen"
SmartPowerDownMiniHelp                ="Hiermee wordt de adaptervoeding uitgeschakeld als de LAN-kabel wordt losgekoppeld."
AdaptiveLinkResponse                  ="Adaptief antwoord koppeling"
AdaptiveLinkResponseMiniHelp          ="Hiermee wordt Adaptief antwoord koppeling ingeschakeld ter controle van de PHYLink-status."
WakeOnLinkSettings                    ="Instellingen Wake On-verbinding"
WakeOnLinkHelp                        ="Maakt activering bij APM-energiebeheer mogelijk wanneer de verbinding opnieuw tot stand wordt gebracht."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.040b] ; Finnish
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="Päälle"
Off                      ="Pois päältä"
Enabled                  ="Käytössä"
Disabled                 ="Pois käytöstä"
AutoDetect               ="Automaattitunnistus"
10Mb-Half-Duplex         ="10 Mbps/yksisuuntainen"
10Mb-Full-Duplex         ="10 Mbps/kaksisuuntainen"
100Mb-Half-Duplex        ="100 Mbps/yksisuuntainen"
100Mb-Full-Duplex        ="100 Mbps/kaksisuuntainen"
High                     ="Korkea"
Low                      ="Matala"
None                     ="Ei mitään"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Luo ja vastaa"
Respond                  ="Vastaa"
Generate                 ="Luo"
NoAction                 ="Ei toimenpiteitä"
HardwareDefault          ="Laitteisto-oletus"
OSControlled             ="Käyttöjärjestelmän ohjaama"
Forced                   ="Pakotettu"

; advanced tab strings
RxBuffers                             ="Vastaanottokuvaajat"
RxBuffersMiniHelp                     ="Ohjaimen käyttämien puskurien määrä kopioitaessa tietoja yhteyskäytäntömuistiin."
TxBuffers                             ="Lähetyksen kuvaajat"
TxBuffersMiniHelp                     ="Määrittää sovittimen käytettävissä olevien ohjauslohkojen määrän."
CoalesceBuffers                       ="Yhdistetyt puskurit"
CoalesceBuffersMiniHelp               ="Lähetyksen nopeuttamiseen saatavilla olevien puskurien määrä."
AdaptiveIFS                           ="Mukautuvat kehystenväliset ajat"
AdaptiveIFSMiniHelp                   ="Korjaa Ethernet-pakettien liialliset yhteentörmäykset ohjaamalla peräkkäisajoitusta."
AdaptiveTxThreshold                   ="Mukautuva lähetyskynnys"
AdaptiveTxThresholdMiniHelp           ="Määrittää tavujen määrän, ennen kuin sovitin tyhjentää FIFO-puskurinsa. Todellinen arvo on 8-kertainen asetus."
HPQPriorityLevelDef                   ="Prioriteettitason määritys"
HPQPriorityLevelDefMiniHelp           ="Määrittää suuren prioriteetin jonon katkaisutason."
AdaptiveTechnology                    ="Mukautuva tekniikka"
AdaptiveTechnologyMiniHelp            ="Ottaa käyttöön suorituskykyä lisäävän Mukautuva tekniikka -ominaisuuden tai poistaa sen käytöstä."
PciBusEfficiency                      ="PCI-väylän suorituskyky"
PciBusEfficiencyMiniHelp              ="Yhdistää lähetyspaketit yksittäiseen puskuriin ennen niiden lähettämistä verkkoon."
BasicConnectivity                     ="Yhteydenmuodostus resurs. vähäisiä"
BasicConnectivityMiniHelp             ="Yritä ladata ohjain vähäisten resurssien ympäristössä."
LocalyAdminAddress                    ="Paikallisesti hallittu osoite"
LocalyAdminAddressMiniHelp            ="Oletusarvoisesti osoite ei ole käytössä ja arvokenttä jätetään tyhjäksi. Aseta LAA Intelin(R) PROSetissä kirjoittamalla yksi arvokenttään. Huomautus: Kun määrität LAA:n Laitehallinnassa, valitse Arvo-asetus ja kirjoita osoite annettuun kenttään."
RetransmitInterFrameSpace             ="Kehystenvälinen aika kun läht. uudelleen"
RetransmitInterFrameSpaceMiniHelp     ="Korjaa Ethernet-pakettien liialliset yhteentörmäykset ohjaamalla uudelleenlähetyksen ajoitusta."
LogLinkState                          ="Kirjaa linkin tilatapahtuma lokiin"
LogLinkStateMiniHelp                  ="Ottaa käyttöön linkin tilasanoman lokiin tai poistaa sen käytöstä."
QoSPacketTag                          ="QoS-paketin merkintä"
QosPacketTagMiniHelp                  ="IEEE Tagged -kehysten (802.3ac / 802.1p / 802.1Q) lähetys ja vastaanotto."
FlowControlSettings                   ="Vuonohjausasetukset"
FlowControlSettingsMiniHelp           ="Keskeyttää pakettien lähettämisen vastaanotettaessa täyden vuonohjauskehyksen ja lähettää täyden vuonohjauksen kehyksen toiselle osapuolelle lähetyksen lopettamisen ilmoittamiseksi."
SpeedDuplex                           ="Linkkinopeus ja kaksisuuntainen"
SpeedDuplex10MiniHelp                 ="Määrittää linkin nopeudeksi 10 Mbps ja suuntaisuuden yksi- tai kaksisuuntaiseksi. Pitää yhdentyä kytkinportin kanssa tai linkkiä ei muodostu."
SpeedDuplexMiniHelp                   ="Määrittää linkin nopeudeksi 10/100 Mbps ja suuntaisuuden yksi- tai kaksisuuntaiseksi. Pitää yhdentyä kytkinportin kanssa tai linkkiä ei muodostu."
PhyPhoneSpeed                         ="Puhelinlinjan siirtonopeus"
PhyPhonePower                         ="Puhelinlinjan tehotaso"
PhyGiladIfs                           ="Kehystenvälinen aika"
IPSecEnabled                          ="Pura IP-suojaus"
IPSecEnabledMiniHelp                  ="Tallentaa suoritinkierrot käytettäessä IPSec-suojausta."
ChecksumEnabled                       ="Pura TCP/IP-tarkistussumma"
ChecksumEnabledMiniHelp               ="Sallii sovittimen tarkistaa vastaanotetun paketin TCP/IP-tarkistussumman ja laskea lähetettyjen pakettien tarkistussumman. Tämä parantaa TCP/IP-lähetyksen suorituskykyä."
LargeSendEnabled                      ="TCP-lohkomisen purkaminen"
LargeSendEnabledMiniHelp              ="Sallii sovittimen purkaa TCP-sanomien lohkomistehtävän ja parantaa suorittimen käyttöä."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Suojaussidokset"
SecurityAssociationsMiniHelp          ="Samanaikaiset suojaussidokset, jotka voidaan purkaa sovittimen apusuorittimeen."
AdaptivePerfTuning                    ="Mukautuva suorituskyvyn hienosäätö"
AdapterBandwidth                      ="Sovittimen kaistanleveys"
CpuUtil                               ="Suorittimen käyttö"
AdaptivePerfTuningMiniHelp            ="Määrittää suorittimen/sovittimen suorituskyvyn ihanteellisen pisteen tässä järjestelmässä. Lisätietoja ohjeessa."
WakeOnSettings                        ="Herätysasetukset"
WakeOnLink                            ="Herätys linkinmuutoksella"
WakeOnMagicPacket                     ="Herätys taikapaketilla"
WakeOnLAA                             ="Herätys LAA:lla"
WakeOnArp                             ="Herätys ARP:llä"
WakeOnDirected                        ="Herätys ohjatulla paketilla"
WakeOnMagicAndDirectedPackets 	      ="Herätys taikapaketilla ja ohjatulla"
WakeOnNBT                             ="Herätys NBT-kyselyllä"
WakeOnSettingsMiniHelp                ="Määrittää, millä paketeilla järjestelmä voidaan herättää (suorat paketit, taikapaketti jne.)."
ForceWakeOnLink                       ="Pakota herätys linkillä"
ForceWakeOnLinkMiniHelp               ="Kun käytössä, pakottaa järjestelmän heräämään linkinmuutoksen yhteydessä."
EnablePME                             ="Ota PME käyttöön"
EnablePMEMiniHelp                     ="Kun käytössä, sallii herätyksen APM-virranhallinnasta. Kun poissa käytöstä, sammuttaa ACPI:n alaisen verkko-ohjaimen."
SmartPowerDown                        ="Älykäs sammuttaminen"
SmartPowerDownMiniHelp                ="Katkaisee sovittimen virran, kun verkkokaapeli irrotetaan."
AdaptiveLinkResponse                  ="Mukautuva linkin palaute"
AdaptiveLinkResponseMiniHelp          ="Ottaa käyttöön mukautuvan linkin palautteen PHYLink-tilan tarkistamista varten."
WakeOnLinkSettings                    ="Herätys linkinmuutoksella -asetukset"
WakeOnLinkHelp                        ="Sallii herätyksen APM-virranhallinnasta, kun linkki muodostetaan uudelleen."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.040c] ; French
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="Activé(e)"
Off                      ="Désactivé(e)"
Enabled                  ="Activé(e)"
Disabled                 ="Désactivé(e)"
AutoDetect               ="Détection automatique"
10Mb-Half-Duplex         ="10 Mbits/s half duplex"
10Mb-Full-Duplex         ="10 Mbits/s full duplex"
100Mb-Half-Duplex        ="100 Mbits/s half duplex"
100Mb-Full-Duplex        ="100 Mbits/s full duplex"
High                     ="Haut"
Low                      ="Faible"
None                     ="Aucun"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Générer et répondre"
Respond                  ="Répondre"
Generate                 ="Générer"
NoAction                 ="Aucune action"
HardwareDefault          ="Matériel par défaut"
OSControlled             ="Contrôlé par le système"
Forced                   ="Forcé"

; advanced tab strings
RxBuffers                             ="Descripteurs de réception"
RxBuffersMiniHelp                     ="Le nombre de tampons utilisés par le pilote lors de la copie des données dans la mémoire de protocole."
TxBuffers                             ="Descripteurs de transmission"
TxBuffersMiniHelp                     ="Définit le nombre de blocs de contrôle disponibles pour la carte réseau."
CoalesceBuffers                       ="Tampons de regroupement"
CoalesceBuffersMiniHelp               ="Nombre de tampons disponibles pour l'accélération des transmissions."
AdaptiveIFS                           ="Espacement intertrame dynamique"
AdaptiveIFSMiniHelp                   ="Compense les collisions excessives des paquets Ethernet en contrôlant les synchronisations successives."
AdaptiveTxThreshold                   ="Seuil dynamique de transmission"
AdaptiveTxThresholdMiniHelp           ="Définit le nombre d'octets avant la remise à zéro du tampon FIFO de la carte réseau. La valeur réelle est de 8 fois la valeur définie."
HPQPriorityLevelDef                   ="Définition du niveau de priorité"
HPQPriorityLevelDefMiniHelp           ="Définit le point de coupure contrôlé pour l'utilisation de la fonction HPQ."
AdaptiveTechnology                    ="Technologie Adaptive"
AdaptiveTechnologyMiniHelp            ="Active/désactive la fonctionnalité Technologie Adaptive."
PciBusEfficiency                      ="Rendement du bus PCI"
PciBusEfficiencyMiniHelp              ="Regroupe les paquets de transmission en un seul tampon avant de les envoyer sur le réseau."
BasicConnectivity                     ="Connectivité (ressources insuff.)"
BasicConnectivityMiniHelp             ="Essayez de charger le pilote dans un environnement où les ressources sont insuffisantes."
LocalyAdminAddress                    ="Adresse administrée localement"
LocalyAdminAddressMiniHelp            ="Par défaut, aucune adresse n'est définie et le champ valeur est laissé vide. Pour définir une adresse administrée localement dans Intel(R) PROSet, saisissez une adresse dans le champ valeur. Remarque : pour définir une adresse administrée localement dans le Gestionnaire de périphériques, sélectionnez l'option Valeur et entrez une adresse dans le champ proposé."
RetransmitInterFrameSpace             ="Espacement intertrame des retransmissions"
RetransmitInterFrameSpaceMiniHelp     ="Compense les collisions excessives des paquets Ethernet en contrôlant la cadence des retransmissions."
LogLinkState                          ="Consigner l'événement de la liaison"
LogLinkStateMiniHelp                  ="Active/désactive le message d'état de la liaison du consignateur."
QoSPacketTag                          ="Repérage des paquets QS"
QosPacketTagMiniHelp                  ="Envoyer et recevoir les trames étiquetées IEEE (802.3ac / 802.1p / 802.1Q)."
FlowControlSettings                   ="Paramètres de contrôle de flux"
FlowControlSettingsMiniHelp           ="Interrompt la transmission des paquets en cas de réception d'une trame de contrôle de flux complète et envoie une trame de contrôle de flux au partenaire de communication afin de stopper la transmission."
SpeedDuplex                           ="Vitesse de liaison et duplex"
SpeedDuplex10MiniHelp                 ="Définit la vitesse de liaison sur 10 Mbits/s et le duplex sur half ou full. Si les paramètres ne coïncident pas avec le port de commutation, aucune liaison ne se produira. "
SpeedDuplexMiniHelp                   ="Définit la vitesse de liaison sur 10/100 Mbits/s et le duplex sur half ou full. Si les paramètres ne coïncident pas avec le port de commutation, aucune liaison ne se produira. "
PhyPhoneSpeed                         ="Vitesse de trans. téléphonique"
PhyPhonePower                         ="Puissance de ligne téléphonique"
PhyGiladIfs                           ="Espacement intertrame"
IPSecEnabled                          ="Délestage sécurité IP"
IPSecEnabledMiniHelp                  ="Enregistre les cycles du processeur lorsque IPSec est utilisé."
ChecksumEnabled                       ="Délester somme de contrôle TCP/IP"
ChecksumEnabledMiniHelp               ="Permet à la carte réseau de contrôler la somme de contrôle TCP/IP des paquets entrants, et de calculer la somme de contrôle des paquets sortants. Ceci permet d'améliorer les performances TCP/IP."
LargeSendEnabled                      ="Délestage segmentation TCP"
LargeSendEnabledMiniHelp              ="Permet à la carte réseau de délester la tâche de la segmentation des messages TCP et d'optimiser le taux d'utilisation du processeur."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Associations de sécurité"
SecurityAssociationsMiniHelp          ="Associations de sécurité simultanées pouvant être délestées sur le coprocesseur des cartes réseau."
AdaptivePerfTuning                    ="Optimisation dynamique des performances"
AdapterBandwidth                      ="Largeur de bande de la carte"
CpuUtil                               ="Taux d’utilisation du processeur"
AdaptivePerfTuningMiniHelp            ="Définit le niveau optimal des performances UC/carte réseau du système. Voir l'Aide."
WakeOnSettings                        ="Paramètres Wake On"
WakeOnLink                            ="Fonction Wake on Link Change"
WakeOnMagicPacket                     ="Wake on Magic Packet"
WakeOnLAA                             ="Fonction Wake on LAA"
WakeOnArp                             ="Fonction Wake on ARP"
WakeOnDirected                        ="Wake on Directed Packet"
WakeOnMagicAndDirectedPackets 	      ="Wake on Magic & Directed Packet"
WakeOnNBT                             ="Fonction Wake on NBT Query"
WakeOnSettingsMiniHelp                ="Détermine les paquets pouvant être activés afin de réveiller le système (Direct Packets, Magic Packet, etc.)."
ForceWakeOnLink                       ="Forcer la fonction Wake on Link"
ForceWakeOnLinkMiniHelp               ="Lorsqu'elle est activée, cette fonction force le réveil du système en fonction des modifications de liaison."
EnablePME                             ="Activer PME"
EnablePMEMiniHelp                     ="Lorsqu'elle est activée, cette fonction permet un réveil depuis la fonctionnalité Gestion avancée de l'alimentation (APM). Si elle est désactivée, le contrôleur LAN est mis hors tension par l'interface ACPI."
SmartPowerDown                        ="Extinction automatique"
SmartPowerDownMiniHelp                ="Supprime l'alimentation de la carte réseau lorsque le câble LAN est déconnecté."
AdaptiveLinkResponse                  ="Réponse dynamique de liaison"
AdaptiveLinkResponseMiniHelp          ="Permet d'activer la fonction Réponse dynamique de liaison pour la vérification de l'état de PHYLink."
WakeOnLinkSettings                    ="Paramètres Wake On Link"
WakeOnLinkHelp                        ="Permet un réveil depuis la fonctionnalité Gestion avancée de l'alimentation (APM) lorsque la liaison est rétablie."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0407] ; German
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="Ein"
Off                      ="Aus"
Enabled                  ="Aktiviert"
Disabled                 ="Deaktiviert"
AutoDetect               ="Automatische Erkennung"
10Mb-Half-Duplex         ="10 Mbit/s/Halbduplex"
10Mb-Full-Duplex         ="10 Mbit/s/Vollduplex"
100Mb-Half-Duplex        ="100 Mbit/s/Halbduplex"
100Mb-Full-Duplex        ="100 Mbit/s/Vollduplex"
High                     ="Hoch"
Low                      ="Schwach"
None                     ="Keine"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Generieren und Reagieren"
Respond                  ="Reagieren"
Generate                 ="Generieren"
NoAction                 ="Keine Aktion"
HardwareDefault          ="Hardware-Standard"
OSControlled             ="Betriebssystem-gesteuert"
Forced                   ="Erzwungen"

; advanced tab strings
RxBuffers                             ="Empfangsdescriptors"
RxBuffersMiniHelp                     ="Anzahl der Puffer, die der Treiber beim Kopieren von Daten in den Protokollspeicher verwendet."
TxBuffers                             ="Übertragungsdescriptors"
TxBuffersMiniHelp                     ="Bestimmt die Anzahl der Steuerungsblöcke, die den Adaptern zur Verfügung stehen."
CoalesceBuffers                       ="Coalesce Buffers"
CoalesceBuffersMiniHelp               ="Anzahl der zur Übertragungsbeschleunigung verfügbaren Puffer."
AdaptiveIFS                           ="Adaptives Inter-Frame Spacing"
AdaptiveIFSMiniHelp                   ="Kompensiert übermäßige Ethernet-Paketkollisionen durch Steuerung der aufeinanderfolgenden Pakete."
AdaptiveTxThreshold                   ="Adaptive Transmit-Threshold"
AdaptiveTxThresholdMiniHelp           ="Bestimmt die Anzahl der Byte, bevor der Adapter seine FIFO-Puffer leert. Der aktuelle Wert beträgt 8 Mal die Einstellung."
HPQPriorityLevelDef                   ="Definition der Prioritätsebene"
HPQPriorityLevelDefMiniHelp           ="Bestimmt die überwachte Abschaltebene für HPQ."
AdaptiveTechnology                    ="Adaptive Technology"
AdaptiveTechnologyMiniHelp            ="Aktiviert/deaktiviert die Funktionalität von Adaptive Technology."
PciBusEfficiency                      ="PCI Bus-Effizienz"
PciBusEfficiencyMiniHelp              ="Fügt Übertragungspakete in einem einzigen Puffer zusammen, bevor sie über das Netzwerk übertragen werden. "
BasicConnectivity                     ="Verbindung mit beschr. Ressourcen"
BasicConnectivityMiniHelp             ="Laden Sie den Treiber in einer Umgebung ohne Ressourcen."
LocalyAdminAddress                    ="Lokal verwaltete Adresse"
LocalyAdminAddressMiniHelp            ="Standardmäßig wird keine Adresse angezeigt und das Wertefeld bleibt leer. Um ein LAA in Intel(R) PROSet zu definieren, geben Sie in das Wertefeld 1 ein. Hinweis: Um ein LAA im Geräte-Manager zu definieren, wählen Sie die Option "Wert" und geben eine Adresse in das dafür vorgesehene Feld ein."
RetransmitInterFrameSpace             ="Inter-Frame Spacing bei Neuübertragung"
RetransmitInterFrameSpaceMiniHelp     ="Kompensiert übermäßige Ethernet-Paketkollisionen durch Überwachung der zeitlichen Regulierung neu zu übertragender Pakete."
LogLinkState                          ="Verbindungsereignis protokollieren"
LogLinkStateMiniHelp                  ="Aktiviert/deaktiviert die Verbindungszustandsmeldung zum Protokoll."
QoSPacketTag                          ="QoS Packet-Tagging"
QosPacketTagMiniHelp                  ="Mit IEEE gekennzeichnete Frames (802.3ac / 802.1p / 802.1Q) senden und erhalten."
FlowControlSettings                   ="Flusssteuerungseinstellungen"
FlowControlSettingsMiniHelp           ="Unterbricht die Paketübertragung beim Erhalt eines vollen Flusssteuerungsframes und sendet vollen Flusssteuerungsframe, um die andere Seite aufzufordern, die Übertragung zu stoppen."
SpeedDuplex                           ="Geschwindigkeit und Duplexmodus"
SpeedDuplex10MiniHelp                 ="Setzt die Verbindungsgeschwindigkeit auf 10 Mbit/s und den Duplexmodus auf Halb- oder Vollduplex. Die Einstellungen müssen mit dem Switchanschluss übereinstimmen, da andernfalls keine Verbindung zustande kommt."
SpeedDuplexMiniHelp                   ="Setzt die Verbindungsgeschwindigkeit auf 10/100 Mbit/s und den Duplexmodus auf Halb- oder Vollduplex. Die Einstellungen müssen mit dem Switchanschluss übereinstimmen, da andernfalls keine Verbindung zustande kommt."
PhyPhoneSpeed                         ="Geschwindigkeit der Telefonleitung"
PhyPhonePower                         ="Stromstärke der Telefonleitung"
PhyGiladIfs                           ="Inter-Frame Spacing"
IPSecEnabled                          ="IP Security entladen"
IPSecEnabledMiniHelp                  ="Speichert bei der Verwendung von IPSec die CPU-Zyklen."
ChecksumEnabled                       ="TCP/IP-Prüfsumme entladen"
ChecksumEnabledMiniHelp               ="Ermöglicht dem Adapter, die TCP/IP-Prüfsumme empfangener Pakete zu überprüfen und die Prüfsumme übertragener Pakete zu berechnen. Dadurch wird die TCP-Empfangsleistung gesteigert."
LargeSendEnabled                      ="TCP-Segmentierung entladen"
LargeSendEnabledMiniHelp              ="Ermöglicht dem Adapter, die Segmentierung von TCP-Meldungen abzugeben und die Prozessorauslastung zu verbessern."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Sicherheitszuordnungen"
SecurityAssociationsMiniHelp          ="Gleichzeitige Sicherheitszuordnungen, die auf den Co-Prozessoren des Adapters abgeladen werden können."
AdaptivePerfTuning                    ="Adaptives Leistungs-Tuning"
AdapterBandwidth                      ="Adapterbandbreite"
CpuUtil                               ="CPU-Auslastung"
AdaptivePerfTuningMiniHelp            ="Bestimmt den optimalen Punkt der Prozessor-/Adapterleistung dieses Systems. Siehe Hilfe."
WakeOnSettings                        ="Aktivierungseinstellungen"
WakeOnLink                            ="Aktivierung bei Verbindungsänderung"
WakeOnMagicPacket                     ="Akt. über Magic Packet"
WakeOnLAA                             ="Aktivierung über LAA"
WakeOnArp                             ="Aktivierung über ARP"
WakeOnDirected                        ="Akt. über adressiertes Paket"
WakeOnMagicAndDirectedPackets 	      ="Magic & adressierte Pakete"
WakeOnNBT                             ="Remoteaktivierung über NBT-Abfrage"
WakeOnSettingsMiniHelp                ="Bestimmt, welche Pakete zur Fernaktivierung des Systems befähigt werden (Direktpakete, Magic Packet usw.)."
ForceWakeOnLink                       ="Akt. bei Verbindungsänderung erzwingen"
ForceWakeOnLinkMiniHelp               ="Wenn aktiviert, wird die Aktivierung des Systems bei Verbindungsänderung erzwungen."
EnablePME                             ="PME aktivieren"
EnablePMEMiniHelp                     ="Wenn die Option aktiviert ist, ist die Aktivierung im APM-Energiesparmodus möglich. Ist sie deaktiviert, wird der LAN-Controller im ACPI-Energiesparmodus abgeschaltet."
SmartPowerDown                        ="Smart Power Down"
SmartPowerDownMiniHelp                ="Schaltet bei der Trennung des LAN-Kabels den Adapterstrom ab."
AdaptiveLinkResponse                  ="Adaptive Verbindungsreaktion"
AdaptiveLinkResponseMiniHelp          ="Aktiviert die adaptive Verbindungsreaktion, um den PHYLink-Status zu überprüfen."
WakeOnLinkSettings                    ="Einst. für Aktivierung bei Verbindung"
WakeOnLinkHelp                        ="Ermöglicht die Aktivierung im APM-Energiesparmodus, wenn die Verbindung wiederhergestellt wird."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0410] ; Italian
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="Attivo"
Off                      ="Disattivo"
Enabled                  ="Attivato"
Disabled                 ="Disattivato"
AutoDetect               ="Rilevamento automatico"
10Mb-Half-Duplex         ="10Mbps/half duplex"
10Mb-Full-Duplex         ="10Mbps/full duplex"
100Mb-Half-Duplex        ="100Mbps/half duplex"
100Mb-Full-Duplex        ="100Mbps/full duplex"
High                     ="Alto"
Low                      ="Basso"
None                     ="Nessuno"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Genera e rispondi"
Respond                  ="Rispondi"
Generate                 ="Genera"
NoAction                 ="Nessuna azione"
HardwareDefault          ="Impostazioni predefinite hardware"
OSControlled             ="Controllato dal sis. operativo"
Forced                   ="Imposto"

; advanced tab strings
RxBuffers                             ="Descrittori di ricezione"
RxBuffersMiniHelp                     ="Numero di buffer usati dal driver durante la copia dei dati nella memoria del protocollo."
TxBuffers                             ="Descrittori di trasmissione"
TxBuffersMiniHelp                     ="Imposta il numero di blocchi di gestione a disposizione della scheda di rete."
CoalesceBuffers                       ="Buffer coalesce"
CoalesceBuffersMiniHelp               ="Numero di buffer disponibili per l'accelerazione delle trasmissioni."
AdaptiveIFS                           ="Spaziatura adattiva tra frame"
AdaptiveIFSMiniHelp                   ="Consente di compensare le collisioni eccessive di pacchetti Ethernet tramite il controllo della sincronizzazione back to back. "
AdaptiveTxThreshold                   ="Soglia adattiva di trasmissione"
AdaptiveTxThresholdMiniHelp           ="Imposta il numero di byte raggiunto il quale la scheda di rete svuota il proprio buffer FIFO. Il valore effettivo è 8 volte l'impostazione."
HPQPriorityLevelDef                   ="Definizione del livello di priorità"
HPQPriorityLevelDefMiniHelp           ="Imposta il livello limite per il controllo dell'utilizzo della coda a priorità alta."
AdaptiveTechnology                    ="Tecnologia Adaptive"
AdaptiveTechnologyMiniHelp            ="Attiva/disattiva la funzione delle prestazioni della tecnologia Adaptive."
PciBusEfficiency                      ="Efficienza bus PCI"
PciBusEfficiencyMiniHelp              ="Assegna i pacchetti di trasmissione a un buffer singolo prima di inviarli alla rete."
BasicConnectivity                     ="Connettività in presenza di risorse scarse"
BasicConnectivityMiniHelp             ="Tentativo di caricare il driver in un ambiente con scarse risorse."
LocalyAdminAddress                    ="Indirizzo amministrato localmente"
LocalyAdminAddressMiniHelp            ="Per impostazione predefinita, non viene inserito un indirizzo e il campo valore viene lasciato vuoto. Per impostare un indirizzo LAA in Intel(R) PROSet, immettere un indirizzo nel campo valore. Per impostare un indirizzo LAA in Gestione periferiche, selezionare l'opzione Valore ed immettere un indirizzo nel campo visualizzato."
RetransmitInterFrameSpace             ="Spaziatura tra frame di ritrasmissioni"
RetransmitInterFrameSpaceMiniHelp     ="Consente di compensare le collisioni eccessive di pacchetti Ethernet tramite il controllo della sincronizzazione di ritrasmissione. "
LogLinkState                          ="Registra evento stato del collegamento"
LogLinkStateMiniHelp                  ="Attiva/disattiva il messaggio di stato del collegamento inviato al programma di registro."
QoSPacketTag                          ="Codifica pacchetti QoS"
QosPacketTagMiniHelp                  ="Invio e ricezione di frame con codifica IEEE (802.3ac / 802.1p / 802.1Q)."
FlowControlSettings                   ="Impostazioni di controllo del flusso"
FlowControlSettingsMiniHelp           ="Sospende la trasmissione dei pacchetti al ricevimento di un frame di controllo indicante di flusso completo e invia un frame di controllo di flusso completo per avvisare l'altra parte di interrompere la trasmissione."
SpeedDuplex                           ="Velocità di collegamento e duplex"
SpeedDuplex10MiniHelp                 ="Imposta la velocità del collegamento a 10 Mbps e il duplex a half o full. Affinché il collegamento avvenga, è necessario che queste impostazioni coincidano con la porta di commutazione."
SpeedDuplexMiniHelp                   ="Imposta la velocità del collegamento a 10/100 Mbps e il duplex a half o full. Affinché il collegamento avvenga, è necessario che coincida con la porta di commutazione."
PhyPhoneSpeed                         ="Velocità di trasmissione della linea telefonica"
PhyPhonePower                         ="Livello di alimentazione della linea telefonica"
PhyGiladIfs                           ="Spaziatura tra frame"
IPSecEnabled                          ="Offload della protezione IP"
IPSecEnabledMiniHelp                  ="Salva i cicli della CPU quando viene utilizzato IPSec."
ChecksumEnabled                       ="Offload del checksum IP/TCP"
ChecksumEnabledMiniHelp               ="Consente alla scheda di verificare il checksum TCP/IP dei pacchetti ricevuti e di calcolare il checksum dei pacchetti trasmessi, migliorando le prestazioni di trasmissione TCP/IP."
LargeSendEnabled                      ="Offload della segmentazione TCP"
LargeSendEnabledMiniHelp              ="Consente alla scheda di effettuare l'offload dell'operazione di segmentazione dei messaggi TCP e migliora l'utilizzo della CPU."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Associazioni protezione"
SecurityAssociationsMiniHelp          ="Associazioni di protezione simultanee che possono essere scaricate sul coprocessore delle schede di rete."
AdaptivePerfTuning                    ="Ottimizzazione adattiva delle prestazioni"
AdapterBandwidth                      ="Larghezza di banda della scheda di rete"
CpuUtil                               ="Utilizzo della CPU"
AdaptivePerfTuningMiniHelp            ="Imposta il punto ottimale delle prestazioni CPU/scheda di rete per il sistema. Consultare la Guida."
WakeOnSettings                        ="Impostazioni di attivazione"
WakeOnLink                            ="Attiva su modifica del collegamento"
WakeOnMagicPacket                     ="Attiva con Magic Packet"
WakeOnLAA                             ="Attiva con LAA"
WakeOnArp                             ="Attiva con ARP"
WakeOnDirected                        ="Attiva con Directed Packet"
WakeOnMagicAndDirectedPackets 	      ="Attiva con Magic e Directed"
WakeOnNBT                             ="Attiva su query NTB"
WakeOnSettingsMiniHelp                ="Determina quali pacchetti sono abilitati ad attivare il sistema (Direct Packet, Magic Packet ecc.)."
ForceWakeOnLink                       ="Imponi attivazione alla modifica del collegamento"
ForceWakeOnLinkMiniHelp               ="Quando attivato, impone al sistema di attivarsi quando cambia il collegamento."
EnablePME                             ="Abilita PME"
EnablePMEMiniHelp                     ="Quando attivato, consente l'attivazione da parte di un evento di risparmio energia avanzato (APM). Quando disattivato, il controller LAN di ACPI viene disattivato."
SmartPowerDown                        ="Spegnimento intelligente"
SmartPowerDownMiniHelp                ="Rimuove l'alimentazione della scheda di rete quando il cavo LAN è scollegato."
AdaptiveLinkResponse                  ="Risposta adattiva dei collegamenti"
AdaptiveLinkResponseMiniHelp          ="Attiva la risposta adattiva dei collegamenti per il controllo dello stato di PHYLink."
WakeOnLinkSettings                    ="Impostazioni di attivazione alla modifica del collegamento"
WakeOnLinkHelp                        ="Consente l'attivazione da uno stato di risparmio energia avanzato (APM) quando il collegamento viene ristabilito."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0411] ; Japanese
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="オン"
Off                      ="オフ"
Enabled                  ="オン"
Disabled                 ="オフ"
AutoDetect               ="自動検出"
10Mb-Half-Duplex         ="10Mbps/半二重通信"
10Mb-Full-Duplex         ="10Mbps/全二重通信"
100Mb-Half-Duplex        ="100Mbps/半二重通信"
100Mb-Full-Duplex        ="100Mbps/全二重通信"
High                     ="高"
Low                      ="低"
None                     ="なし"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="作成と応答"
Respond                  ="応答"
Generate                 ="作成"
NoAction                 ="アクションなし"
HardwareDefault          ="ハードウェア デフォルト"
OSControlled             ="OS が制御"
Forced                   ="強制"

; advanced tab strings
RxBuffers                             ="受信記述子"
RxBuffersMiniHelp                     ="データをプロトコル メモリにコピー中にドライバが使うバッファ数。"
TxBuffers                             ="送信記述子"
TxBuffersMiniHelp                     ="アダプタの使用に使えるコントロール ブロック数を設定します。"
CoalesceBuffers                       ="集合バッファ"
CoalesceBuffersMiniHelp               ="送信の高速化に使用できるバッファ数。"
AdaptiveIFS                           ="アダプティブ インターフレーム スぺ－シング"
AdaptiveIFSMiniHelp                   ="過剰なイーサネット パケットのコリジョンを連続タイミングにより補償します。"
AdaptiveTxThreshold                   ="アダプティブ送信しきい値"
AdaptiveTxThresholdMiniHelp           ="アダプタが FIFO バッファを空にする前のバイト数を設定します。実値は設定値の 8 倍です。"
HPQPriorityLevelDef                   ="優先レベルの定義"
HPQPriorityLevelDefMiniHelp           ="HPQ 使用のための制御された切り捨てレベルを設定します。"
AdaptiveTechnology                    ="アダプティブ テクノロジ"
AdaptiveTechnologyMiniHelp            ="アダプティブ テクノロジ パフォーマンス機能のオン/オフを切り替えます。"
PciBusEfficiency                      ="PCI バス効率"
PciBusEfficiencyMiniHelp              ="送信パケットをネットワークに送信する前に 1 つのバッファに集積します。"
BasicConnectivity                     ="リソース不足時の接続"
BasicConnectivityMiniHelp             ="低リソース環境でのドライバのロードを試行します。"
LocalyAdminAddress                    ="ローカル管理されるアドレス"
LocalyAdminAddressMiniHelp            ="デフォルトではアドレスは表示されず値のフィールドは空白になります。Intel(R) PROSet で LAA を設定するには、値のフィールドに入力してください。注意：デバイス マネージャで LAA を設定するには、値のオプションを選択し、フィールドにアドレスを入力してください。"
RetransmitInterFrameSpace             ="インターフレーム スぺ－シングの再送信"
RetransmitInterFrameSpaceMiniHelp     ="過剰なイーサネット パケットのコリジョンを再送信のタイミングにより補償します。"
LogLinkState                          ="リンク ステート イベントのログ"
LogLinkStateMiniHelp                  ="ログへのリンク ステート メッセージをオン/オフに切り替えます。"
QoSPacketTag                          ="QoS パケット タグ"
QosPacketTagMiniHelp                  ="IEEE タグ付きフレームの送受信 (802.3ac / 802.1p / 802.1Q)。"
FlowControlSettings                   ="フロー制御設定"
FlowControlSettingsMiniHelp           ="完全なフロー制御フレームの受信時にパケット送信を一時停止し、反対側で送信停止を通知するように完全なフロー制御フレームを送信します。"
SpeedDuplex                           ="リンク速度とデュプレックス"
SpeedDuplex10MiniHelp                 ="リンク速度を10 Mbps に、デュプレックスを半二重または全二重に設定します。設定がスイッチ ポートと一致しないと、リンクされません。"
SpeedDuplexMiniHelp                   ="リンク速度を10/100 Mbps に、デュプレックスを半二重または全二重に設定します。設定がスイッチ ポートと一致しないと、リンクされません。"
PhyPhoneSpeed                         ="電話回線送信速度"
PhyPhonePower                         ="電話回線電力レベル"
PhyGiladIfs                           ="インターフレーム スぺ－シング"
IPSecEnabled                          ="ＩＰ セキュリティのオフロード"
IPSecEnabledMiniHelp                  ="IPSec を使う場合の CPU サイクルを節約します。"
ChecksumEnabled                       ="TCP/IP  チェックサムのオフロード"
ChecksumEnabledMiniHelp               ="アダプタによる受信パケットの TCP/IP チェックサムの確認を可能とし、送信されたパケットのチェックサムを計算します。これにより TCP/IP パフォーマンスが向上します。"
LargeSendEnabled                      ="TCP セグメンテーションのオフロード"
LargeSendEnabledMiniHelp              ="アダプタによる TCP メッセージの分断タスクのオフロードを可能とし、CPU 使用率を改善します。"
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="セキュリティ関連"
SecurityAssociationsMiniHelp          ="アダプタのコプロセッサにオフロードすることのできる並列のセキュリティ関連。"
AdaptivePerfTuning                    ="アダプティブ パフォーマンス チューニング"
AdapterBandwidth                      ="アダプタの帯域幅"
CpuUtil                               ="CPU 使用率"
AdaptivePerfTuningMiniHelp            ="このシステムで最適な CPU/アダプタ パフォーマンスを設定します。ヘルプをご参照ください。"
WakeOnSettings                        ="Wake on 設定"
WakeOnLink                            ="Wake on Link Change"
WakeOnMagicPacket                     ="Wake on Magic Packet"
WakeOnLAA                             ="Wake on LAA"
WakeOnArp                             ="Wake on ARP"
WakeOnDirected                        ="Wake on Directed Packet"
WakeOnMagicAndDirectedPackets 	      ="Magic および Directed"
WakeOnNBT                             ="Wake on NBT Query"
WakeOnSettingsMiniHelp                ="システムをウェークアップするパケット (Direct Packets、Magic Packet 等) を決定します。"
ForceWakeOnLink                       ="Wake on Link の強制"
ForceWakeOnLinkMiniHelp               ="オンの場合、リンク変更時にウェークアップするように強制します。"
EnablePME                             ="PME をオンにする"
EnablePMEMiniHelp                     ="オンの場合は APM 電源管理からのウェークアップを可能とします。オフの場合は ACPI で LAN コントローラをシャットダウンします。"
SmartPowerDown                        ="スマート パワー ダウン"
SmartPowerDownMiniHelp                ="LAN ケーブルの切断時にアダプタの電源を切ります。"
AdaptiveLinkResponse                  ="アダプティブ リンク レスポンス"
AdaptiveLinkResponseMiniHelp          ="PHYLink ステータスを確認するために、アダプティブ リンク レスポンスをオンにします。"
WakeOnLinkSettings                    ="Wake On Link 設定"
WakeOnLinkHelp                        ="リンクが再接続されると APM 電源管理からのウェークアップを可能とします。"


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0412] ; Korean
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="온"
Off                      ="오프"
Enabled                  ="활성화됨"
Disabled                 ="활성 해제됨"
AutoDetect               ="자동 검색"
10Mb-Half-Duplex         ="10Mbps/반이중"
10Mb-Full-Duplex         ="10Mbps/전이중"
100Mb-Half-Duplex        ="100Mbps/반이중"
100Mb-Full-Duplex        ="100Mbps/전이중"
High                     ="높음"
Low                      ="낮음"
None                     ="없음"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="생성 및 응답"
Respond                  ="응답"
Generate                 ="생성"
NoAction                 ="동작 없음"
HardwareDefault          ="하드웨어 기본값"
OSControlled             ="OS 제어 방식"
Forced                   ="강제"

; advanced tab strings
RxBuffers                             ="수신 설명자"
RxBuffersMiniHelp                     ="프로토콜 메모리에 데이터를 복사할 때 드라이버에서 사용하는 버퍼의 수입니다."
TxBuffers                             ="전송 설명자"
TxBuffersMiniHelp                     ="어댑터에 사용할 수 있는 제어 블록의 수를 설정합니다."
CoalesceBuffers                       ="가속 시 가용 버퍼 수"
CoalesceBuffersMiniHelp               ="전송 가속화에 사용할 수 있는 버퍼의 수입니다."
AdaptiveIFS                           ="적응 프레임간 간격"
AdaptiveIFSMiniHelp                   ="백-투-백 타이밍을 제어하여 과도한 이더넷 패킷 충돌을 보상합니다."
AdaptiveTxThreshold                   ="적응 전송 임계값"
AdaptiveTxThresholdMiniHelp           ="어댑터가 해당 FIFO 버퍼를 비우기 전의 바이트 수를 설정합니다. 실제 값은 8회로 설정되어 있습니다."
HPQPriorityLevelDef                   ="우선순위 레벨 정의"
HPQPriorityLevelDefMiniHelp           ="HPQ 사용에 적합하도록 제어된 경계 레벨을 설정합니다."
AdaptiveTechnology                    ="적용 기술"
AdaptiveTechnologyMiniHelp            ="적용 기술 성능 기능을 활성화/활성 해제합니다."
PciBusEfficiency                      ="PCI 버스 효율성"
PciBusEfficiencyMiniHelp              ="네트워크로 보내기 전에 전송 패킷을 하나의 버퍼로 통합합니다."
BasicConnectivity                     ="리소스가 부족한 경우 연결"
BasicConnectivityMiniHelp             ="리소스가 부족한 환경에서 드라이버 로드를 시도합니다."
LocalyAdminAddress                    ="로컬 관리 주소"
LocalyAdminAddressMiniHelp            ="기본적으로, 주소가 존재하지 않으며 값 필드는 비어 있습니다. Intel(R) PROSet에서 LAA를 설정하려면 값 필드에 LAA를 입력하십시오. 참고: 장치 관리자에서 LAA를 설정하려면 값 옵션을 선택하고 필드에 주소를 입력하십시오."
RetransmitInterFrameSpace             ="재전송 프레임간 간격"
RetransmitInterFrameSpaceMiniHelp     ="재전송 타이밍을 제어하여 과도한 이더넷 패킷 충돌을 보상합니다."
LogLinkState                          ="링크 상태 이벤트 기록"
LogLinkStateMiniHelp                  ="링크 상태 메시지 기록 기능 활성화/활성 해제"
QoSPacketTag                          ="QoS 패킷 태그 지정"
QosPacketTagMiniHelp                  ="IEEE 태그 있는 프레임(802.3ac / 802.1p / 802.1Q)을 전송 및 수신합니다."
FlowControlSettings                   ="흐름 제어 설정"
FlowControlSettingsMiniHelp           ="전체 흐름 제어 프레임 수신 시 패킷 전송을 중단하고 전체 흐름 제어 프레임을 보내 다른 쪽에서 전송을 중지하도록 알립니다."
SpeedDuplex                           ="링크 속도 및 이중성"
SpeedDuplex10MiniHelp                 ="링크 속도를 10Mbps로 설정하고 이중성을 반이중 또는 전이중으로 설정합니다. 이 설정은 반드시 스위치 포트와 일치해야 합니다. 그렇지 않으면 어떠한 링크도 발생하지 않습니다."
SpeedDuplexMiniHelp                   ="링크 속도를 10/100Mbps로 설정하고 이중성을 반이중 또는 전이중으로 설정합니다. 이 설정은 반드시 스위치 포트와 일치해야 합니다. 그렇지 않으면 어떠한 링크도 발생하지 않습니다."
PhyPhoneSpeed                         ="전화선 전송 속도"
PhyPhonePower                         ="전화선 전원 레벨"
PhyGiladIfs                           ="프레임간 간격"
IPSecEnabled                          ="오프로드 IP 보안"
IPSecEnabledMiniHelp                  ="IPSec 사용 시 CPU 사이클을 저장합니다."
ChecksumEnabled                       ="오프로드 TCP/IP 체크섬"
ChecksumEnabledMiniHelp               ="어댑터가 수신된 패킷의 TCP/IP 체크섬을 확인하고 전송된 패킷의 체크섬을 계산할 수 있습니다. 따라서 TCP/IP 성능이 향상됩니다."
LargeSendEnabled                      ="TCP 세그먼트화 오프로드"
LargeSendEnabledMiniHelp              ="어댑터가 TCP 메시지 세그먼트화 작업을 오프로드할 수 있으며 이로 인해 CPU 이용률이 향상됩니다."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="보안 연결"
SecurityAssociationsMiniHelp          ="어댑터 코프로세서로 오프로드할 수 있는 동시 보안 연결 수입니다."
AdaptivePerfTuning                    ="적응 성능 조정"
AdapterBandwidth                      ="어댑터 대역폭"
CpuUtil                               ="CPU 이용률"
AdaptivePerfTuningMiniHelp            ="이 시스템에서 최적의 CPU/어댑터 성능을 내는 지점을 설정합니다. 도움말을 참조하십시오."
WakeOnSettings                        ="깨우기 설정"
WakeOnLink                            ="링크 변경 시 깨우기"
WakeOnMagicPacket                     ="매직 패킷 발생 시 깨우기"
WakeOnLAA                             ="LAA 발견 시 깨우기"
WakeOnArp                             ="ARP 시 깨우기"
WakeOnDirected                        ="유도 패킷 발생 시 깨우기"
WakeOnMagicAndDirectedPackets 	      ="매직 및 직접 패킷 발생 시 깨우기"
WakeOnNBT                             ="NBT 쿼리 시 깨우기"
WakeOnSettingsMiniHelp                ="시스템을 깨우기 위해 패킷을 활성화하는 방법(예: 직접 패킷, 매직 패킷)을 결정합니다."
ForceWakeOnLink                       ="링크 시 강제로 깨우기"
ForceWakeOnLinkMiniHelp               ="활성화된 경우 링크 변경 시 강제로 깨어나도록 합니다."
EnablePME                             ="PME 활성화"
EnablePMEMiniHelp                     ="활성화된 경우 APM 전원 관리를 종료할 수 있습니다. 활성 해제하면 ACPI에서 LAN 컨트롤러가 종료됩니다."
SmartPowerDown                        ="스마트 전원 차단"
SmartPowerDownMiniHelp                ="LAN 케이블이 분리되어 있으면 어댑터 전원을 제거합니다."
AdaptiveLinkResponse                  ="적응 링크 응답"
AdaptiveLinkResponseMiniHelp          ="적응 링크 응답이 PHYLink 상태를 검사할 수 있도록 합니다."
WakeOnLinkSettings                    ="링크 시 깨우기 설정"
WakeOnLinkHelp                        ="다시 연결될 때 APM 전원 관리에서 깨울 수 있습니다."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.0414] ; Norwegian
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="På"
Off                      ="Av"
Enabled                  ="Aktivert"
Disabled                 ="Deaktivert"
AutoDetect               ="Registrer automatisk"
10Mb-Half-Duplex         ="10 Mbps / Halv dupleks"
10Mb-Full-Duplex         ="10 Mbps / Hel dupleks"
100Mb-Half-Duplex        ="100 Mbps / Halv dupleks"
100Mb-Full-Duplex        ="100 Mbps / Hel dupleks"
High                     ="Høy"
Low                      ="Lav"
None                     ="Ingen"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Generer og svar"
Respond                  ="Svar"
Generate                 ="Generer"
NoAction                 ="Ingen handling"
HardwareDefault          ="Standard maskinvareinnstilling"
OSControlled             ="Styrt av OS"
Forced                   ="Fremtvunget"

; advanced tab strings
RxBuffers                             ="Mottaksdeskriptorer"
RxBuffersMiniHelp                     ="Antallet buffere driveren bruker når data blir kopiert til protokollminnet."
TxBuffers                             ="Overføringsdeskriptorer"
TxBuffersMiniHelp                     ="Angir antall kontrollblokker som er tilgjengelig for adapterens bruk."
CoalesceBuffers                       ="Oppsamlingsbuffere"
CoalesceBuffersMiniHelp               ="Antall buffere som er tilgjengelige for å øke farten på overføringer."
AdaptiveIFS                           ="Adaptivt rammeintervall"
AdaptiveIFSMiniHelp                   ="Kompenserer for store mengder Ethernet-pakkekollisjoner ved å kontrollere tidsintervall mellom pakker."
AdaptiveTxThreshold                   ="Terskel for adaptivt rammeintervall"
AdaptiveTxThresholdMiniHelp           ="Angir antall byte før adapteren tømmer FIFO-bufferen. Faktisk verdi er 8 ganger innstillingen."
HPQPriorityLevelDef                   ="Angi prioritetsnivå"
HPQPriorityLevelDefMiniHelp           ="Angir styrt grensenivå for bruk av HPQ."
AdaptiveTechnology                    ="Adaptiv teknologi"
AdaptiveTechnologyMiniHelp            ="Aktiverer/deaktiverer ytelsesfunksjonen Adaptiv teknologi."
PciBusEfficiency                      ="Effektivitet for PCI-buss"
PciBusEfficiencyMiniHelp              ="Samler pakker som skal overføres i en enkelt buffer før de blir sendt til nettverket."
BasicConnectivity                     ="Lite ressurser-tilkobling"
BasicConnectivityMiniHelp             ="Prøv å laste driveren i miljø med lite ressurser."
LocalyAdminAddress                    ="Lokalt administrert adresse"
LocalyAdminAddressMiniHelp            ="Som standard er ingen adresse tilgjengelig, og verdifeltet står tomt. Hvis du vil angi en LAA i Intel(R) PROSet, skriv inn en i verdifeltet. Merk: Hvis du vil angi en LAA i Enhetsbehandling, angi verdialternativet og skriv inn en adresse i det angitte feltet."
RetransmitInterFrameSpace             ="Rammeintervall for gjentatt overføring"
RetransmitInterFrameSpaceMiniHelp     ="Kompenserer for store mengder Ethernet-pakkekollisjoner ved å kontrollere tidsintervall mellom gjentatte overføringer."
LogLinkState                          ="Logg forbindelsestilstand-hendelser"
LogLinkStateMiniHelp                  ="Aktiverer/deaktiverer meldinger om forbindelsestilstand til loggfunksjonen."
QoSPacketTag                          ="Markering av QoS-pakke"
QosPacketTagMiniHelp                  ="Send og motta IEEE-markerte rammer (802.3ac / 802.1p / 802.1Q)."
FlowControlSettings                   ="Innstillinger for flytkontroll"
FlowControlSettingsMiniHelp           ="Tar pause i pakkeoverføring ved mottak av full flytkontrollramme og send full flytkontrollramme for å be den andre siden om å stoppe overføringen."
SpeedDuplex                           ="Kommunikasjonshastighet og dupleks"
SpeedDuplex10MiniHelp                 ="Setter kommunikasjonshastigheten til 10 Mbps og dupleks til halv eller full. Må stemme med port på svitsj, ellers blir forbindelse ikke opprettet."
SpeedDuplexMiniHelp                   ="Setter kommunikasjonshastigheten til 10 Mbps og dupleks til halv eller full. Må stemme med port på svitsj, ellers blir forbindelse ikke opprettet."
PhyPhoneSpeed                         ="Overføringshastighet for telefonlinje"
PhyPhonePower                         ="Strømnivå for telefonlinje"
PhyGiladIfs                           ="Rammeintervall"
IPSecEnabled                          ="Avlast IP-sikkerhet"
IPSecEnabledMiniHelp                  ="Lagrer CPU-sykluser når IPSec brukes."
ChecksumEnabled                       ="Avlast TCP/IP-kontrollsum"
ChecksumEnabledMiniHelp               ="Gir kortet mulighet til å verifisere TCP/IP-kontrollsum for innkommende pakker samt beregne kontrollsum for overførte pakker. Dette gir bedre ytelse ved TCP/IP-overføringer."
LargeSendEnabled                      ="Avlast TCP-segmentering"
LargeSendEnabledMiniHelp              ="Gir adapteren mulighet til å avlaste oppgaven med å segmentere TCP-meldinger og gir bedre utnyttelse av prosessoren."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Sikkerhetstilordninger"
SecurityAssociationsMiniHelp          ="Samtidige sikkerhetstilordninger som kan avlastes til koprosessoren i adapteren."
AdaptivePerfTuning                    ="Adaptiv ytelsesjustering"
AdapterBandwidth                      ="Båndbredde for adapter"
CpuUtil                               ="Prosessorutnyttelse"
AdaptivePerfTuningMiniHelp            ="Angir optimalt punkt for prosessor/adapter-ytelse for systemet. Se Hjelp."
WakeOnSettings                        ="Innstillinger for oppvåkning"
WakeOnLink                            ="Våkne ved endring i forbindelse"
WakeOnMagicPacket                     ="Ved magisk pakke"
WakeOnLAA                             ="Våkne ved LAA"
WakeOnArp                             ="Våkne ved ARP"
WakeOnDirected                        ="Ved adressert pakke"
WakeOnMagicAndDirectedPackets 	      ="Ved magiske og adresserte"
WakeOnNBT                             ="Våkne ved NBT-forespørsel"
WakeOnSettingsMiniHelp                ="Bestemmer hvilke pakker som kan aktiveres for å vekke systemet (adresserte pakker, magiske pakker osv.)."
ForceWakeOnLink                       ="Tvungen våkne ved forbindelse"
ForceWakeOnLinkMiniHelp               ="Når dette er aktivt, blir systemet tvunget til å våkne ved endring i forbindelse"
EnablePME                             ="Aktiver PME"
EnablePMEMiniHelp                     ="Tillater oppvåkning fra APM-strømstyring når det er aktivert. Deaktiver slår av nettverkskontrolleren under ACPI"
SmartPowerDown                        ="Smart strømsparingsmodus"
SmartPowerDownMiniHelp                ="Slutter å sende strøm til adapteren når nettverkskabelen blir koblet fra."
AdaptiveLinkResponse                  ="Adaptiv forbindelsesrespons"
AdaptiveLinkResponseMiniHelp          ="Aktiverer adaptiv forbindelsesrespons for å sjekke fysisk forbindelsesstatus."
WakeOnLinkSettings                    ="Innstillinger for Reaktiver ved kobling"
WakeOnLinkHelp                        ="Tillater reaktivering fra APM-strømstyring når koblingen etableres på nytt."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
[Strings.041d] ; Swedish
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

UninstallString ="Intel(R) PRO Network Adapters and Drivers"

MessageStringSource      ="%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\e100bmsg.dll"

; NT service name
e100bnt.Service.DispName ="Intel(R) PRO Adapter Driver"

; Parameters
; values
On                       ="På"
Off                      ="Av"
Enabled                  ="Aktiverad"
Disabled                 ="Avaktiverad"
AutoDetect               ="Automatisk identifiering"
10Mb-Half-Duplex         ="10Mbps/Halv duplex"
10Mb-Full-Duplex         ="10Mbps/Full duplex"
100Mb-Half-Duplex        ="100Mbps/Halv duplex"
100Mb-Full-Duplex        ="100Mbps/Full duplex"
High                     ="Högt"
Low                      ="Lågt"
None                     ="Inget"
;Ipsecurity               = "IP Security"
;Checksum_str             = "Checksum"
;LargeSend_str            = "Large Send"
;All_str                  = "All"
GenerateAndRespond       ="Generera och svara"
Respond                  ="Svara"
Generate                 ="Generera"
NoAction                 ="Ingen åtgärd"
HardwareDefault          ="Maskinvarans standard"
OSControlled             ="OS-styrd"
Forced                   ="Tvingat"

; advanced tab strings
RxBuffers                             ="Mottagningsbeskrivare"
RxBuffersMiniHelp                     ="Antal buffertar som används av drivrutinen när data kopieras till protokollminnet."
TxBuffers                             ="Överföringsbeskrivare"
TxBuffersMiniHelp                     ="Ställer in antalet kontrollblock som kortet kan använda."
CoalesceBuffers                       ="Sammanslagningsbuffertar"
CoalesceBuffersMiniHelp               ="Antal buffertar som är tillgängliga för sändningsacceleration."
AdaptiveIFS                           ="Anpass. avstånd mellan ramar"
AdaptiveIFSMiniHelp                   ="Kompenserar för många Ethernet-paketkollisioner genom att styra kontinuerlig timing."
AdaptiveTxThreshold                   ="Anpass. tröskelvärde för överföring"
AdaptiveTxThresholdMiniHelp           ="Ställer in antalet byte innan kortet tömmer sin FIFO-buffert. Faktiskt värde är 8 gånger inställningen."
HPQPriorityLevelDef                   ="Definition av prioritetsnivå"
HPQPriorityLevelDefMiniHelp           ="Ställer in den styrda kapningsnivån för att använda HPQ."
AdaptiveTechnology                    ="Anpassningsbar teknologi"
AdaptiveTechnologyMiniHelp            ="Aktiverar/avaktiverar prestandafunktionen Anpassningsbar teknologi."
PciBusEfficiency                      ="PCI-busseffektivitet"
PciBusEfficiencyMiniHelp              ="Slår samman paket till en enda buffring innan de skickas till nätverket."
BasicConnectivity                     ="Anslutningsbarhet vid få resurser"
BasicConnectivityMiniHelp             ="Prova att ladda drivrutinen i lågresursmiljö."
LocalyAdminAddress                    ="Lokalt administrerad adress"
LocalyAdminAddressMiniHelp            ="Standard är att det inte finns någon adress och att värdefältet lämnas tomt. Om du vill ange en LAA i Intel(R) PROSet anger du den i värdefältet. Obs! Om du vill ange en LAA i Enhetshanteraren, markera alternativet Värde och ange en adress i det fältet du får."
RetransmitInterFrameSpace             ="Överför avstånd mellan ramar igen"
RetransmitInterFrameSpaceMiniHelp     ="Kompenserar för många Ethernet-paketkollistioner genom att styra återsändningstiming."
LogLinkState                          ="Loggningslänk statushändelse"
LogLinkStateMiniHelp                  ="Aktiverar/avaktiverar länkstatusmeddelandet till loggaren."
QoSPacketTag                          ="Markering av QoS-paket"
QosPacketTagMiniHelp                  ="Skicka och ta emot IEEE-markerade ramar (802.3ac / 802.1p / 802.1Q)."
FlowControlSettings                   ="Inställningar för flödeskontroll"
FlowControlSettingsMiniHelp           ="Gör paus i paketsändningen vid mottagning av full flödeskontrollram och skicka full flödeskontrollram för att meddela den andra sidan om att stoppa sändning."
SpeedDuplex                           ="Länkhastighet & duplexinställningar"
SpeedDuplex10MiniHelp                 ="Ställer in länkhastigheten på 10 Mbps och duplex på halv eller full. Måste sammanfalla med växelport för att länken ska uppstå."
SpeedDuplexMiniHelp                   ="Ställer in länkhastigheten på 10/100 Mbps och duplex på halv eller full. Måste sammanfalla med växelport för att länken ska uppstå."
PhyPhoneSpeed                         ="Telefonlinjens överföringshastighet"
PhyPhonePower                         ="Telefonlinjens strömnivå"
PhyGiladIfs                           ="Avstånd mellan ramar"
IPSecEnabled                          ="Avlasta IP-säkerhet"
IPSecEnabledMiniHelp                  ="Sparar CPU-cykler när du använder IPSec."
ChecksumEnabled                       ="Avlasta TCP/IP-kontrollsumma"
ChecksumEnabledMiniHelp               ="Gör det möjligt för kortet att verifiera TCP/IP-kontrollsumma på mottaget paket och beräkna kontrollsumma på överförda paket. Detta ger bättre TCP/IP-prestanda."
LargeSendEnabled                      ="Avlasta TCP-segmentering"
LargeSendEnabledMiniHelp              ="Gör det möjligt för kortet att avlasta uppgiften att segmentera TCP-meddelanden och förbättrar processorbelastningen."
;TaskOffload                           = "Offloading"
;TaskOffloadMiniHelp                   = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security."
;TaskOffloadXsumMiniHelp               = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum."
;TaskOffloadLSOMiniHelp                = "Saves CPU cycles if set to correspond to the adapter type. Range: None, IP Security, Checksum, Larges Send." 
SecurityAssociations                  ="Säkerhetsassociationer"
SecurityAssociationsMiniHelp          ="Samtidiga säkerhetsassociationer som kan avlastas till kortets extraprocessor."
AdaptivePerfTuning                    ="Anpassningsbar prestandajustering"
AdapterBandwidth                      ="Kortbandbredd"
CpuUtil                               ="Processorbelastning"
AdaptivePerfTuningMiniHelp            ="Ställer in optimal prestanda för processor/kort för detta system. Se hjälp."
WakeOnSettings                        ="Wake vid Inställningar"
WakeOnLink                            ="Wake vid länkändring"
WakeOnMagicPacket                     ="Wake vid Magic Packet"
WakeOnLAA                             ="Wake vid LAA"
WakeOnArp                             ="Wake vid ARP"
WakeOnDirected                        ="Wake vid dirigerat paket"
WakeOnMagicAndDirectedPackets 	      ="Wake vid Magic och dirigerat"
WakeOnNBT                             ="Wake vid NBT-fråga"
WakeOnSettingsMiniHelp                ="Avgör vilka paket som kan aktiveras för att väcka systemet (Direct Packet, Magic Packet osv.)."
ForceWakeOnLink                       ="Tvinga wake vid länk"
ForceWakeOnLinkMiniHelp               ="När det är aktiverat tvingar det systemet att vakna vid länkändring"
EnablePME                             ="Aktivera PME"
EnablePMEMiniHelp                     ="Gör det möjligt att starta från strömhantering med APM när det är aktiverat. Inaktivering stänger LAN-styrenheten under ACPI"
SmartPowerDown                        ="Smart avstängning"
SmartPowerDownMiniHelp                ="Tar bort strömmen från kortet när LAN-kabeln är frånkopplad."
AdaptiveLinkResponse                  ="Anpassningsbart länksvar"
AdaptiveLinkResponseMiniHelp          ="Gör det möjligt för anpassningsbart länksvar att kontrollera PHYLink-status."
WakeOnLinkSettings                    ="Wake vid Länk-inställningar"
WakeOnLinkHelp                        ="Möjliggör wake-up från APM-strömhantering när länken återansluts."


; Device descriptions
PCIE100B.DeviceDesc              ="Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc            ="Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc            ="Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc            ="Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc               ="Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc            ="82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc               ="Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc            ="Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc           ="Intel(R) PRO/100+ PCI Adapter"
PCIE100PLUS64.DeviceDesc         ="Intel(R) PRO/100+ PCI Adapter not supported"
PCIE100LOM.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
PCIE100MAN.DeviceDesc            ="Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc         ="Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc        ="Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc           ="Intel(R) PRO/100+ Dual Port Server Adapter"

PCIE100SCBRCOMBONODES.DeviceDesc ="Intel(R) PRO/100 R Mobile Combo Adapter"

PCIE100AOL.DeviceDesc            ="Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc         ="Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc       ="Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559IFE.DeviceDesc               ="Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc            ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc          ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"

PCIE100S.DeviceDesc              ="Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc           ="Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc           ="Intel(R) PRO/100 S Server Adapter"

MiniPCIComboDes.DeviceDesc       ="Intel(R) PRO/100 SP Mobile Combo Adapter"

PCIE100S0.DeviceDesc             ="Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc             ="Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc          ="Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc          ="Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc            ="Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc            ="Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc          ="Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONMB.DeviceDesc        ="Intel(R) PRO/100 M Mobile Connection"
PCIE100LAVONLOM.DeviceDesc       ="Intel(R) PRO/100 M Network Connection"

I559CLONPCI.DeviceDesc           ="Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFEAOLCPQ.DeviceDesc         ="Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

PCIE100EMBEDDED.DeviceDesc       ="Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc   ="Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc         ="82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc         ="Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc     ="Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc         ="Intel(R) PRO/100 Network Connection"

PCIE100DUALSx.DeviceDesc         ="Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100DUALx.DeviceDesc          ="Intel(R) PRO/100 Dual Port Server Adapter"

PCIE100BSPLUSD.DeviceDesc        ="Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc        ="Intel(R) PRO/100 S+ Server Adapter"

HPTX.DeviceDesc                  ="NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc                ="Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc                ="Intel(R) PRO/100 S Network Connection"
IBMFEK.DeviceDesc                ="Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc                ="iSeries 2892 10/100 Ethernet Port"


Toshiba82559B.DeviceDesc         ="Intel 8255x-based Fast Ethernet"

DL_EMBLOM.DeviceDesc             ="Intel(R) PRO/100 VE Adapter"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc   ="Intel(R) 82562 based Fast Ethernet Connection"
﻿
;**********************************************************************
;************** End          of      Installation     File ************
;**********************************************************************