; VA32W2.INF  -- This file contains descriptions of DuoATA the 
;              CardBus SCSI Host adapters supported in Windows2000
;

[Version]
signature="$Windows NT$"
;Class=SCSIAdapter
Class=hdc
;ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
ClassGuid={4D36E96A-E325-11CE-BFC1-08002BE10318}
Provider=%SONY%
;;LayoutFile=LAYOUT.INF
Catalogfile=va32xp.cat
DriverVer=07/02/2001,1.11.16

; Class Install
[ClassInstall32.NT]
AddReg=HDC_Class
;Addreg=SCSIReg

;;[SCSIReg]
;;HKR,,,,%SCSIClassName%
;;HKR,,Installer32,,"SysSetup.Dll,ScsiClassInstaller"
;;HKR,,Icon,,"-10"
;;HKR,,LegacyInfOption,,"SCSI"
;;HKR,,DeviceType,0x10001,4                       ; FILE_DEVICE_CONTROLLER
;;HKR,,DeviceCharacteristics,0x10001,0x100        ; Use same security checks on relative opens

[HDC_Class]
HKR,,,,%HDCClassName%
HKR,,Icon,,"-9"
HKR,,Installer32,,"SysSetup.Dll,HdcClassInstaller"
HKR,,TroubleShooter-0,,"tshoot.chm,hdw_drives.htm"
HKR,,DeviceType,0x10001,4                       ; FILE_DEVICE_CONTROLLER
HKR,,DeviceCharacteristics,0x10001,0x100        ; Use same security checks on relative opens

;-----------------------------------------------
;;[ClassInstall]
;;Addreg=HDCReg

;;[HDCReg]
;;HKR,,,,%HDCClassName%
;;HKR,,Icon,,-9

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS

; Table of Contents
[Manufacturer]
%SONY%=SONY

[SONY]
%WB_DuoATA.DeviceDesc%= DuoATA_Inst ,PCI\VEN_1145&DEV_F020

[DuoATA_Inst]
CopyFiles = @va32w2.sys

[DuoATA_Inst.Services]
AddService = va32w2, %SPSVCINST_ASSOCSERVICE%, DuoATA_Service_Inst, Miniport_EventLog_Inst
;;AddReg     = cardbus_interface_type

[DuoATA_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\va32w2.sys
LoadOrderGroup = SCSI Miniport
AddReg         = pnpsafe_pci_addreg


[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

;;[cardbus_interface_type]
;;HKR, "ScsiPort", "LegacyInterfaceType", 0x00010001, 0x00000005

;*************************************************************
;The EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7

[SourceDisksFiles]
va32w2.sys=1

[SourceDisksNames]
1="Sony CardBus ATA PC Card for Windows XP Driver Disk",,0

;-----------------------------------------------------------

[Strings]
SONY = "Sony"
;SCSIClassName="SCSI and RAID controllers"
HDCClassName="IDE ATA/ATAPI controllers"
WB_DuoATA.DeviceDesc = "Sony CardBus ATA PC Card for Windows XP"

;*******************************************
;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001


