; Copyright (c) 2001, Microsoft Corporation

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %LUCENT%
DriverVer   = 08/31/2001,7.16.0.189
CatalogFile = wlluc48.cat

[Manufacturer]
%LUCENT%    = LUCENT
%Sony%      = Sony Corporation

[ControlFlags]
ExcludeFromSelect = *

[LUCENT]
%wlluc48a.DeviceDesc%    = wlluc48.Install, PCMCIA\LUCENT_TECHNOLOGIES-WAVELAN/IEEE-364C
%wlluc48b.DeviceDesc%    = wlluc481.Install, PCMCIA\LUCENT_TECHNOLOGIES-WAVELAN/IEEE-911F

[Sony Corporation]
%wlson48_LT.DeviceDesc%  = wlluc48.Install, PCMCIA\SONY_CORPORATION-PCWA-C100-FFBF

;-------------------------------------------------------------------------------
; Lucent PC Card
;
[wlluc48.Install]
AddReg          = params.reg, wlluc48.reg, lucent.reg
Characteristics = 0x84
BusType         = 8
CopyFiles       = wlluc48.CopyFiles

[wlluc48.Install.Services]
AddService      = wlluc48, 2, wlluc48.Service, wlluc48.EventLog

;-------------------------------------------------------------------------------
; Lucent miniPCI Card
;
[wlluc481.Install]
AddReg          = params.reg, wlluc48.reg, lucent.reg, miniPCI.reg
Characteristics = 0x84
BusType         = 8
CopyFiles       = wlluc48.CopyFiles

[wlluc481.Install.Services]
AddService      = wlluc48, 2, wlluc48.Service, wlluc48.EventLog



[lucent.reg]
HKR,,VendorDescription,,"ORINOCO PC Card"

[miniPCI.reg]
HKR,,miniPCI,,"1"
;-------------------------------------------------------------------------------
;
[params.reg]

;
; OwnChannel
;
HKR,NDI\params\OwnChannel,          ParamDesc,  0, %CHANNEL%
HKR,NDI\params\OwnChannel,          Type,       0, enum
HKR,NDI\params\OwnChannel,          Default,    0, 0
HKR,NDI\params\OwnChannel\enum,     0,          0, %DEFAULT%
HKR,NDI\params\OwnChannel\enum,     1,          0, %CHANNEL1%
HKR,NDI\params\OwnChannel\enum,     2,          0, %CHANNEL2%
HKR,NDI\params\OwnChannel\enum,     3,          0, %CHANNEL3%
HKR,NDI\params\OwnChannel\enum,     4,          0, %CHANNEL4%
HKR,NDI\params\OwnChannel\enum,     5,          0, %CHANNEL5%
HKR,NDI\params\OwnChannel\enum,     6,          0, %CHANNEL6%
HKR,NDI\params\OwnChannel\enum,     7,          0, %CHANNEL7%
HKR,NDI\params\OwnChannel\enum,     8,          0, %CHANNEL8%
HKR,NDI\params\OwnChannel\enum,     9,          0, %CHANNEL9%
HKR,NDI\params\OwnChannel\enum,     10,         0, %CHANNEL10%
HKR,NDI\params\OwnChannel\enum,     11,         0, %CHANNEL11%
HKR,NDI\params\OwnChannel\enum,     12,         0, %CHANNEL12%
HKR,NDI\params\OwnChannel\enum,     13,         0, %CHANNEL13%
HKR,NDI\params\OwnChannel\enum,     14,         0, %CHANNEL14%

;
; Client Name
;
HKR,NDI\params\OwnName,             ParamDesc,  0, %STATIONNAME%
HKR,NDI\params\OwnName,             Type,       0, edit
HKR,NDI\params\OwnName,             LimitText,  0, 32
HKR,NDI\params\OwnName,             Default,    0, ""

;
; TxRateControl
;
HKR,NDI\params\TxRateControl,      	ParamDesc,  0, %TXRATE%
HKR,NDI\params\TxRateControl,       Type,       0, enum
HKR,NDI\params\TxRateControl,       Default,    0, 3
HKR,NDI\params\TxRateControl\enum,  3,          0, %AUTORATE%
HKR,NDI\params\TxRateControl\enum,  1,          0, %FIXEDLOW%
HKR,NDI\params\TxRateControl\enum,	2,          0, %FIXEDSTD%
HKR,NDI\params\TxRateControl\enum,	4,          0, %FIXEDMED%
HKR,NDI\params\TxRateControl\enum,	5,          0, %FIXEDHI%
HKR,NDI\params\TxRateControl\enum,	6,          0, %AUTORATESTD%
HKR,NDI\params\TxRateControl\enum,	7,          0, %AUTORATEMED%

;
; Power Management
;
HKR,NDI\params\PMEnabled,           ParamDesc,  0, %POWERMANAGEMENT%
HKR,NDI\params\PMEnabled,           Type,       0, enum
HKR,NDI\params\PMEnabled,           Default,    0, 0
HKR,NDI\params\PMEnabled\enum,      1,          0, %ON%
HKR,NDI\params\PMEnabled\enum,      0,          0, %OFF%

HKR,,Configured,,1
HKR,,DriverVariant,,"1"
HKR,,DriverMajor,,"7"
HKR,,DriverMinor,,"16"
HKR,,DesiredSSID,,"Agere Systems"
;-------------------------------------------------------------------------------
; Lucent specific
;
[wlluc48.reg]
HKR, Ndi\Interfaces,                UpperRange,    0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange,    0, "ethernet"
HKR, Ndi,                           Service,       0, "wlluc48"

[wlluc48.Copyfiles]
wlluc48.sys,,,2

[wlluc48.Service]
DisplayName     = %wlluc48.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\wlluc48.sys
LoadOrderGroup  = NDIS

[wlluc48.EventLog]
AddReg = wlluc48.AddEventLog.reg

[wlluc48.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\wlluc48.sys"
HKR, , TypesSupported,   0x00010001, 7

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir            = 12
wlluc48.CopyFiles         = 12


;-------------------------------------------------------------------------------
[SourceDisksNames]
1 = %DISKID%,,,

;-------------------------------------------------------------------------------
[SourceDisksFiles]
wlluc48.sys=1


;-------------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
;--------------------------------------------------------------------------
STATIONNAME                 = "1. Station Name"
;--------------------------------------------------------------------------
CHANNEL                     = "2. Channel"
DEFAULT                     = "Use default channel"
CHANNEL1                    = "01"
CHANNEL2                    = "02"
CHANNEL3                    = "03"
CHANNEL4                    = "04"
CHANNEL5                    = "05"
CHANNEL6                    = "06"
CHANNEL7                    = "07"
CHANNEL8                    = "08"
CHANNEL9                    = "09"
CHANNEL10                   = "10"
CHANNEL11                   = "11"
CHANNEL12                   = "12"
CHANNEL13                   = "13"
CHANNEL14                   = "14"
;--------------------------------------------------------------------------
TXRATE                      = "3. Transmit Rate"
FIXEDLOW                    = "Fixed Low"
FIXEDSTD                    = "Fixed Standard"
AUTORATE                    = "Auto Rate Select (High) = default"
FIXEDMED                    = "Fixed Medium"
FIXEDHI                     = "Fixed High"
AUTORATESTD                 = "Auto Rate Select (Standard)"
AUTORATEMED                 = "Auto Rate Select (Medium)"
;--------------------------------------------------------------------------
POWERMANAGEMENT             = "4. Card Power Management"

OFF                         = "Off"
ON                          = "On"


LUCENT                      = "Lucent Technologies"
MSFT                        = "Microsoft"
Sony                        = "Sony Corporation"

DISKID                      = "ORiNOCO Setup Disk"

wlluc48a.DeviceDesc         = "ORiNOCO Wireless LAN PC Card (3.3 and 5 volt)"
wlluc48b.DeviceDesc         = "ORiNOCO Wireless LAN Mini PCI Card"
wlson48_LT.DeviceDesc       = "Sony PCWA-C100 Wireless PC Card"

wlluc48.Service.DispName    = "Wireless LAN PC Card Driver"
