; VA16W2.INF -- This file contains descriptions of VAIO CD-ROM
;             Host Adapters supported in Windows 2000

[version]
signature="$Windows NT$"
;Class=hdc
;ClassGuid={4D36E96A-E325-11CE-BFC1-08002BE10318}	; hdc
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}	; scsi
Provider=%SONY%
;;LayoutFile=layout.inf
Catalogfile=va16xp.cat
DriverVer=07/02/2001,1.11.08

; Class Install
[ClassInstall32.NT]
Addreg=SCSIReg
;Addreg=HDC_Class

[SCSIReg]
HKR,,,,%SCSIClassName%
HKR,,Installer32,,"SysSetup.Dll,ScsiClassInstaller"
HKR,,Icon,,"-10"
HKR,,LegacyInfOption,,"SCSI"
HKR,,DeviceType,0x10001,4                       ; FILE_DEVICE_CONTROLLER
HKR,,DeviceCharacteristics,0x10001,0x100        ; Use same security checks on relative opens

;;[HDC_Class]
;;HKR,,,,%HDCClassName%
;;HKR,,Icon,,"-9"
;;HKR,,Installer32,,"SysSetup.Dll,HdcClassInstaller"
;;HKR,,TroubleShooter-0,,"tshoot.chm,hdw_drives.htm"
;;HKR,,DeviceType,0x10001,4                       ; FILE_DEVICE_CONTROLLER
;;HKR,,DeviceCharacteristics,0x10001,0x100        ; Use same security checks on relative opens

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS

[Manufacturer]
%SONY%=SONY

[SONY]
%NinjaATA.DeviceDesc%   = NinjaATA_Inst,  PCMCIA\_-NINJAATA--3768

[NinjaATA_Inst]
CopyFiles = @va16w2.sys

[NinjaATA_Inst.Services]
AddService = va16w2, %SPSVCINST_ASSOCSERVICE%, NinjaATA_Service_Inst, Miniport_EventLog_Inst

;[NinjaATA_Inst.LogConfigOverride]
;LogConfig = NinjaATA_Inst.LogConfig0

;;[NinjaATA_Inst.LogConfig0]
;;ConfigPriority=NORMAL
;;IOConfig=180-187,386-387
;;IRQConfig=3,5,7,9,10,11
;;PcCardConfig=21:0:0(W)

[NinjaATA_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\va16w2.sys
LoadOrderGroup = SCSI Miniport
AddReg         = pnpsafe_pcmcia_addreg
;AddReg         = pnpsafe_isa_addreg

;;[pnpsafe_isa_addreg]
;;HKR, "Parameters\PnpInterface", "1", 0x00010001, 0x00000001

[pnpsafe_pcmcia_addreg]
; isa with no legacy detection
HKR, "Parameters\PnpInterface", "1", 0x00010001, 0x00000011

;*************************************************************
;The EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7
;HKLM,%DataBase%,"Driver",,"VA16W2"
;HKLM,%DataBase%,"DeviceType",,"SCSI"

[SourceDisksFiles]
va16w2.sys=1

[SourceDisksNames]
1="Sony 16bit ATA PC Card for Windows XP Driver Disk",,,

[Strings]
SONY = "Sony Corporation"
SCSIClassName="SCSI and RAID controllers"
HDCClassName= "IDE ATA/ATAPI controllers"
DataBase = "SYSTEM\CurrentControlSet\Services\Pcmcia\DataBase\ \NinjaATA-"
NinjaATA.DeviceDesc   = "Sony 16bit ATA PC Card for Windows XP"

;*******************************************
;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
