************************************************************
*  Product: Intel(R) Chipset Device Software
*  Release: Production Version
*  Version: 9.2.0.1021
*  Target Products: Intel(R) 6 Series/C200 Series Chipset Family
*		    2nd generation Intel(R) Core(TM) processor family
*  Date: December 23 2010
************************************************************

   NOTE: 
            For the list of supported chipsets, please refer
            to the Release Notes

************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************
This document contains the following sections:

1.  Overview
2.  System Requirements
3.  Contents of the Distribution Package
4.  List of Available Command Line Flag Options 
5.  Contents of the Extracted Files
6.  Installing the Software in Interactive Mode
7.  Installing the Software in Silent Mode
8.  Installing the INF Files Prior to OS Installation
    8A. Installing the Windows* 2000 INF Files Prior
        to OS Installation
    8B. Installing the Windows* XP INF Files Prior
        to OS Installation
    8C. Installing the Windows Server* 2003 INF Files 
        Prior to OS Installation
    8D. Installing the Windows* Vista INF Files Prior
        to OS Installation
    8E. Installing the Windows Server* 2008 INF files Prior
        to OS Installation
    8F. Installing the Windows Server* 2008 R2 INF files 
        Prior to OS Installation
    8G. Installing the Windows 7 INF files Prior
        to OS Installation
9.  Installing the INF Files After OS Installation
    9A. Installing the Windows* 2000 INF Files After
        OS Installation
    9B. Installing the Windows* XP INF Files After
        OS Installation 
    9C. Installing the Windows Server* 2003 INF Files 
        After OS Installation
    9D. Installing the WINDOWS VISTA INF FILES AFTER 
        OS Installation
    9E. Installing the Windows Server* 2008 INF FILES AFTER 
        OS Installation
    9F. Installing the Windows Server* 2008 R2 INF FILES  
        After OS Installation
    9G. Installing the Windows 7 INF FILES AFTER 
        OS Installation
10. Verifying Installation of the Software and 
    Identifying the Software Version Number
11. Troubleshooting


************************************************************
* 1.  OVERVIEW
************************************************************
The Intel(R) Chipset Device Software installs Windows* 
INF files to the target system. These files outline to 
the operating system how to configure the Intel(R) chipset 
components in order to ensure that the following features 
function properly:

            - Core PCI and ISAPNP Services
            - PCIe Support
            - IDE/ATA33/ATA66/ATA100 Storage Support
            - SATA Storage Support
            - USB Support
            - Identification of Intel(R) Chipset Components in 
              the Device Manager

This software can be installed in three modes: Interactive,
Silent and Unattended Preload. Interactive Mode requires 
user input during installation; Silent Mode and Unattended 
Preload do not.  

This software also offers a set of command line flags, 
which provide additional installation choices. The command 
line flags are not case sensitive. Refer to Section 4 for 
detailed descriptions of these flags.

Important Note:
The Intel(R) Chipset Device Software is distributed in two 
formats: self extracting .EXE files (INFINST_AUTOL.EXE) 
or compressed .ZIP files (INFINST_AUTOL.ZIP). Depending on 
which distribution format is being executed, the commandline 
syntax may differ. Refer to Section 4 for more details. 


************************************************************
* 2.  SYSTEM REQUIREMENTS 
************************************************************
1.  Please refer to the Release Notes to view the list of 
    chipsets that the software included with this distribution 
    package is designed to operate with.

2.  One of the following operating systems must be 
    fully installed and running on the system
    before installing this software:

    Microsoft Windows* Server 2003
    Microsoft Windows Server 2003 x64 Edition*
    Microsoft Windows Server 2008
    Microsoft Windows Server 2008 x64 
    Microsoft Windows XP
    Microsoft Windows XP Professional x64  
    Microsoft Windows 2000
    Microsoft Windows Vista
    Microsoft Windows Vista x64  
    Microsoft Windows 7
    Microsoft Windows 7 x64 
    Microsoft Windows 2008 R2
    Microsoft Windows 2008 R2 x64 
    
    This software is designed for the latest Service packs 
    releases of above operating systems.

    To verify which operating system has been installed onto 
    the target system, follow the steps below:

    a.  Click on Start.
    b.  Select Settings.
    c.  Select Control Panel.
    d.  Double-click on the System icon.
    e.  Click on the General system properties tab.
    f.  Verify which OS has been installed by reading
        the System information.
                              
3.  It is recommended that the software be installed on 
    systems with at least 64MB of system memory when using 
    Windows* 2000, Windows* XP, Windows Server* 2003, 
    Windows Server* 2008, and Windows* Vista. 

4.  It is recommended that there be a minimum of 5MB of hard
    disk space on the system in order to install this software.

5.  The operating system must be fully installed and running on 
    the system before running this software.

6.  Close any running applications to avoid installation problems.

7.  It is recommended that the Intel(R) Chipset Device Software 
    be installed onto the target system prior to the 
    installation of other drivers.

Please check with the system provider to determine which 
operating system and Intel(R) chipset are used in the system.


************************************************************
* 3.  CONTENTS OF THE DISTRIBUTION PACKAGE
************************************************************
The Intel(R) Chipset Device Software package contains the 
following items:

    File(s)       
    -------
    INFINST_AUTOL.EXE -or- INFINST_AUTOL.ZIP
    README.TXT, RELEASE_xxx.HTM

   *** NOTE:  
            Only the files that reference the currently 
            detected devices are copied to the system.
	      
            If the -A option is exercised, the files are
            not copied to the <Windows>\INF directory.
            Refer to Section 4 for more information.  

                                       
************************************************************
* 4.  LIST OF AVAILABLE COMMAND LINE FLAG OPTIONS
************************************************************
The Intel(R) Chipset Device Software supports several 
command line flags for various installation options. 

Below is a list of all the available command line flags that
may be used with the program call.  Note that the '-L' and 
the '-S' flags MUST be specified at the end of the command 
line flag list.

Flag        Description
----            -----------
-?              
                Displays the list of available command line 
                flags. This flag works in Interactive Mode only.  

-A              
                Extracts the INF files and Readme to either 
                "C:\Program Files\Intel\InfInst" or the
                <Installation Path> directory specified using 
                the '-P' flag. The software will NOT install 
                these INF files to the system. This flag can 
                be combined only with the '-P' flag. All other
                options will be ignored if the '-A' flag is 
                specified. This flag works in Interactive Mode
                only.

-AONLY          
                Extracts the needed INF files to install on the
                current system. If the install has been run once
                successfully, '-AONLY' will not return any INFs
                when used in conjunction with '-OVERALL' switch, 
                all the needed INFs for the system will be 
                extracted.		

-B              
                Automatically reboots the system after 
                installation. This flag is ignored if '-A' flag
                is specified. This flag works in either Silent 
                Mode or Interactive Mode.

-F2 <path\filename>             
                Specifies an alternate location and name 
                of the log file created by InstallShield Silent.
                This option is used for silent installation from
                a CD. 'Path' indicates the directory path where
                installation status is logged in file 'filename'.

-L <number>    
                Specifies the language of the setup dialogs. 
                This flag works in Interactive Mode only.

-OVERALL       
                Updates ALL INF drivers on all available devices
                even if third party drivers are currently installed. 
                This flag works in Interactive Mode only.

-OVERIDE	
                Updates the storage drivers even if a third
                party storage driver is currently installed. 
                This flag works in Interactive Mode only.

-OVERWRITE       
                Ignores the overwrite warning dialog when 
                installing an older version of the software.

-P<Installation Path>   
                Specifies the hard disk location to which the 
                INF program files are copied. If this flag is 
                not specified at the command line, the 
                <Installation Path> directory is as follows: 
                
                   C:\Program Files\Intel\INFInst
                
               	If this flag is used without the '-A' option, 
               	only the Readme will be copied to 
               	<Installation Path>. The directory name can 
               	include spaces, but then a pair of double quotes 
               	(") must enclose the directory name. There should
                not be any space between the switch '-p' and the 
                directory name. This flag works in either Silent 
                Mode or Interactive Mode.

-S              
                Runs the Installer in Silent Mode (no user 
                interface is displayed). This flag and the
                '-L' flag must be placed at the end of the 
                command line flag list.
                
Below are the language codes used with the '-L' flag:

<number>     Language            
 --------		----------
   0401       Arabic (International)	
   0804       Chinese (Simplified)  	
   0404       Chinese (Traditional) 	
   0405       Czech             		
   0406       Danish            		
   0413       Dutch              		
   0409       English (United States)	
   040B       Finnish            		
   040C       French (International)     	
   0407       German            		
   0408       Greek              		
   040D       Hebrew                                
   040E       Hungarian         		
   0410       Italian            		
   0411       Japanese           		
   0412       Korean             		
   0414       Norwegian          		
   0415       Polish            		
   0416       Portuguese (Brazil)  	
   0816       Portuguese (Standard) 	
   0419       Russian            		
   040A       Spanish (International)	
   041D       Swedish               	
   041E       Thai               		
   041F       Turkish            		


************************************************************
* 5.  CONTENTS OF THE EXTRACTED FILES
************************************************************
INF files are copied to the hard disk after running the 
Intel(R) Chipset Device Software executable with an '-A' 
flag (i.e., "INFINST_AUTOL.EXE -A" or "SETUP.EXE -A"). 
The location of the INF files depends on whether a '-P' 
flag is specified along with the '-A' flag:

1.  If a '-P' flag is not specified, then the INF files are 
    copied to the following directory:  
    
            "C:\Program Files\Intel\INFINST"
    
2.  If a '-P' flag is specified, then the INF files are copied 
    to the location listed immediately after the '-P' flag.  

    Refer to Section 4 for more information on flag usage.

After INF file extraction, the INF files and components are 
copied to the <INF Extract Directory>. These files and 
components are categorized according to the operating system. 
The following table summarizes the locations of the 
INF files by operating system:

   NOTE: 
            "<INF Extract Directory>" is abbreviated "<IED>" in 
            the remainder of this section.

The directories are classified according to the following:

   All\   
            Contains INF files designed for
            Windows* 2000, Windows* XP, Windows Server* 2003,
            Windows Server* 2008, and Windows* Vista

   Win7\   
            Contains INF files designed for
            Windows* 7 and Windows Server* 2008 R2
            
   NOTE: 
            INFAnswr.TXT makes a CUSTOM.INF template that installs 
            the INF files for Intel(R) chipsets during operating
            system setup. OEMs can incorporate this file into the 
            Setup directory for the OEM Preload Kit. 
            (Refer to Section 8 for more details.)


************************************************************
* 6.  INSTALLING THE SOFTWARE IN INTERACTIVE MODE
************************************************************
1.  Verify that all system requirements have been met as 
     described in Section 2 above.

2.  Run the InstallShield* installation program:
     Self-extracting .EXE distribution: INFINST_AUTOL.EXE
     Compressed .ZIP distribution: SETUP.EXE

3.  You will be prompted to agree to the license agreement.  
     If you do not agree, the installation program will exit 
     before extracting any files.
    
4.  Once the operating system reboots, follow the on-screen 
     instructions and accept default settings to complete the 
     setup.


************************************************************
* 7.  INSTALLING THE SOFTWARE IN SILENT MODE
************************************************************
1.  Verify that all system requirements have been met as 
     described in section 2.

2.  Run the InstallShield* installation program:
     For silent install with auto-reboot:
       Self-extracting .EXE distribution: 
       INFINST_AUTOL.EXE -b -s
       Compressed .ZIP distribution:
       SETUP.EXE -b -s
    - or -
     For silent install without auto-reboot:
       Self-extracting .EXE distribution: 
       INFINST_AUTOL.EXE -s
       Compressed .ZIP distribution: SETUP.EXE -s

3.  The utility will perform the necessary updates and 
     record the installation status in the following system 
     registry key:
        HKEY_LOCAL_MACHINE\Software\Intel\INFInst

4.  If the utility was invoked with the "-b" flag, the 
     system will automatically reboot if the update was
     successful.

    NOTE: The system MUST be rebooted for all device 
    updates to take effect.

5.  To determine whether the install was successful, verify 
     the "install" value in the registry key specified in 
     Step 3.

6.  In Silent Mode the utility will not display the license
     agreement. When using Silent Mode the license agreement,
     license.txt, will be placed in the following folder:
     Program Files/Intel/INFInst folder.
     Please read this agreement.

   The following describes the various parameters:

            Name: "install"               
            Type: String
            Data: "success"  
                  The installation was successful.
            
            Data: "fail"
                  The installation was not successful. No INF files 
                  were copied to the system.

             Name: "reboot"           
             Type: String	       
             Data: "Yes" 
                  A reboot is required to complete the installation.
             
             Data: "No"  
                  No reboot is required to complete the installation.

             Name: "version"          
             Type: String          
             Data: <varies> 
                  Current version number of the Intel(R) Chipset Device 
                  Software 


************************************************************
* 8.  INSTALLING THE INF FILES PRIOR TO OS INSTALLATION
************************************************************
    This procedure requires a minimum of 5MB of hard disk space. 
    It is important to make sure there is enough disk space 
    before beginning the copy process. Copy the operating system 
    installation files from the setup directory to a directory
    on the hard disk. This can be done by opening 'My Computer', 
    right-clicking on the correct drive, and selecting 'Properties'.
    The directories shall be referred to as follows:

      Windows* 2000	: <WIN2000 Setup Directory>
      Windows XP	: <WINXP Setup Directory>
      Windows Server* 2003 : <WIN2003 Setup Directory>

        

************************************************************
* 8A.  INSTALLING THE WINDOWS* 2000 INF FILES PRIOR TO
*      OS INSTALLATION
************************************************************
NOTE: The Windows* 2000 OEM Preload Kit distribution CD
      contains a setup directory with all the base operating
      system setup files and installation programs 
      (WINNT.EXE and WINNT32.EXE).  

The name of the directory may vary depending on the 
distribution CD (e.g., \I386\).

1.  Create the following directory structure under the 
    <WIN2000 Setup Directory>: 

       \$OEM$\$$\INF

2.  Copy the Windows* 2000 INF files from 
    <INF Extract Directory>\XXXX\All to the directory
    created in Step 1 above:

       <WIN2000 Setup Directory>\$OEM$\$$\INF

    NOTE: XXXX is the directory name for the chipset of 
          interest.  Refer to Section 8 for more details.

3.  Create the following directory structure under the 
    <WIN2000 Setup Directory>: 

       \$OEM$\$1\drivers\IntelINF

4.  Copy the Windows* 2000 INF files and the catalog files 
    (.CAT) from <INF Extract Directory>\XXXX\All to the 
    directory created in Step 4 above:

       <WIN2000 Setup Directory>\$OEM$\$1\drivers\IntelINF

    NOTE: XXXX is the directory name for the chipset of 
          interest.  Refer to Section 8 for more details.

5.  Either modify the default Windows* 2000 installation
    answer file, UNATTEND.TXT, located in <All Setup 
    Directory>, or create a customized answer file. The
    answer file must include the following information:
   
       [Unattended]
       OemPreinstall = Yes
       OemPnPDriversPath="drivers\IntelINF"

    A sample answer file for preloading the Intel(R) Chipset
    Device Software files is available at: 
    <INF Extract Directory>\XXXX\All\INFAnswr.TXT
    
    For more information about Windows* 2000 answer files 
    and unattended installations, please refer to the 
    Microsoft* Windows* 2000 Guide to Unattended Setup. 
    If you are a computer manufacturer, refer to the 
    Microsoft Windows* 2000 OEM Preinstallation Kit (OPK) 
    User Guide for more information about the \$OEM$ folder. 
    Otherwise, refer to the Microsoft Windows* 2000 Deployment 
    Guide.

6.  Run "WINNT.EXE /u:<answer file name> /s:<WIN2000 Setup 
    Directory>" to install Windows* 2000.


************************************************************
* 8B.  INSTALLING THE WINDOWS* XP INF FILES PRIOR TO
*      OS INSTALLATION
************************************************************
NOTE: The Windows* XP OEM Preload Kit distribution CD contains 
      a setup directory with all the base operating system 
      setup files and installation programs (WINNT.EXE and
      WINNT32.EXE).  

The name of the directory may vary depending on the 
distribution CD (e.g., \I386\).

1.  Create the following directory structure under the 
    <WINXP Setup Directory>: 

       \$OEM$\$$\INF

2.  Copy the Windows* XP INF files from 
    <INF Extract Directory>\XXXX\All to the directory
    created in Step 1 above:

       <WINXP Setup Directory>\$OEM$\$$\INF

    NOTE: XXXX is the directory name for the chipset of 
          interest.  Refer to Section 8 for more details.

3.  Create the following directory structure under the 
    <WINXP Setup Directory>: 

       \$OEM$\$1\drivers\IntelINF

4.  Copy the Windows* XP INF files AND the catalog files 
    (.CAT) from <INF Extract Directory>\XXXX\All to the 
    directory created in Step 4 above:

       <WINXP Setup Directory>\$OEM$\$1\drivers\IntelINF

    NOTE: XXXX is the directory name for the chipset of 
          interest. Refer to Section 8 for more details.

5.  Either modify the default Windows* XP installation
    answer file, UNATTEND.TXT, located in <WINXP Setup 
    Directory>, or create a customized answer file.  The
    answer file must include the following information:
   
       [Unattended]
       OemPreinstall = Yes
       OemPnPDriversPath="drivers\IntelINF"

    A sample answer file for preloading the Intel(R) Chipset
    Device Software files is available: 
    <INF Extract Directory>\XXXX\All\INFAnswr.TXT
    
    If you are a computer manufacturer, refer to the Microsoft* 
    Windows* XP Guide to Unattended Setup for more information 
    about Windows* XP answer files and unattended installations. 
    For more information about the \$OEM$ folder, refer to the 
    Microsoft Windows* XP OEM Preinstallation Kit (OPK) 
    User Guide. If you are not a manufacturer, refer to the Microsoft 
    Windows* XP Deployment Guide.

6.  Run "WINNT.EXE /u:<answer file name> /s:<WINXP Setup 
    Directory>" to install Windows* XP.


************************************************************
* 8C.  INSTALLING THE WINDOWS SERVER* 2003 INF FILES PRIOR 
*      TO OS INSTALLATION
************************************************************
NOTE: The Windows Server* 2003 OEM Preload Kit distribution 
      CD contains a setup directory with all the base operating
      system setup files and installation programs (WINNT.EXE 
      and WINNT32.EXE).  

The name of the directory may vary depending on the 
distribution CD (e.g., \I386\).

1.  Create the following directory structure under the 
    <WIN2003 Setup Directory>: 

       \$OEM$\$$\INF

2.  Copy the Windows Server* 2003 INF files from 
    <INF Extract Directory>\XXXX\All to the directory
    created in Step 1 above:

       <WIN2003 Setup Directory>\$OEM$\$$\INF

    NOTE: XXXX is the directory name for the chipset of 
          interest. Refer to Section 8 for more details.

3.  Create the following directory structure under the 
    <WIN2003 Setup Directory>: 

       \$OEM$\$1\drivers\IntelINF

4.  Copy the Windows Server* 2003 INF files and the catalog 
    files (.CAT) from <INF Extract Directory>\XXXX\All 
    to the directory created in Step 3 above:

       <WIN2003 Setup Directory>\$OEM$\$1\drivers\IntelINF

    NOTE: XXXX is the directory name for the chipset of 
          interest. Refer to Section 8 for more details.

5.  Either modify the default Windows Server* 2003 installation
    answer file, UNATTEND.TXT, located in <WIN2000 Setup 
    Directory>, or create a customized answer file. The
    answer file must include the following information:
   
       [Unattended]
       OemPreinstall = Yes
       OemPnPDriversPath="drivers\IntelINF"

    A sample answer file for preloading the Intel(R) Chipset
    Device Software files is available: 
    <INF Extract Directory>\XXXX\All\INFAnswr.TXT
    
    For more information about Windows Server* 2003 answer 
    files and unattended installations, please refer to the 
    Microsoft Windows Server* 2003 Guide to Unattended Setup.
    If you are a computer manufacturer, refer to the Microsoft 
    Windows Server* 2003 OEM Preinstallation Kit (OPK) User 
    Guide for more information about the \$OEM$ folder. 
    Otherwise, refer to the Microsoft Windows Server* 2003 
    Deployment Guide.


6.  Run "WINNT.EXE /u:<answer file name> /s:<WIN2003 Setup 
    Directory>" to install Windows* 2000.

************************************************************
* 8D.  INSTALLING THE WINDOWS* VISTA INF FILES PRIOR 
*      TO OS INSTALLATION
************************************************************
NOTE: Although $OEM$ method is still supported, it is no longer 
the preferred method.

Microsoft* published a Wndows Automated Installation Kit(WAIK) 
which facilitates creation of answer files and image creation 
for unattended installs of Windows Vista

To add drivers to an offline Windows image

1.  Locate the device driver .inf files that you intend to 
    install on your Windows image.

2.  Use Windows System Image Manager (Windows SIM) to create 
    an answer file that contains the paths to the device 
    drivers that you intend to install.

3.  Add the Microsoft-Windows-PnpCustomizationsNonWinPE component 
    to your answer file in the offlineServicing pass.

4.  Expand the Microsoft-Windows-PnpCustomizationsNonWinPE node 
    in the answer file. Right-click DevicePaths, and then select 
    Insert New PathAndCredentials.

5.  In the Microsoft-Windows-PnpCustomizationsNonWinPE component, 
    specify the path to the device driver and the credentials used 
    to access the file if the file is on a network share.

6.  Save the answer file and exit Windows SIM. The answer file must 
    be similar to the following sample.
 
<?xml version="1.0" ?>
<unattend xmlns="urn:schemas-microsoft-com:asm.v3" xmlns:wcm="http://schemas.microsoft.com/WMIConfig/2002/State">
   <settings pass="offlineServicing">
      <component name="Microsoft-Windows-PnpCustomizationsNonWinPE" processorArchitecture="x86" publicKeyToken="31bf3856ad364e35" language="neutral" versionScope="nonSxS">
         <DriverPaths>
            <PathAndCredentials wcm:keyValue="1">
               <Path>\\networkshare\share\drivers</Path>
               <Credentials>
                  <Domain>Fabrikam</Domain>
                  <Username>MyUserName</Username>
                  <Password>MyPassword</Password>
               </Credentials>
            </PathAndCredentials>
         </DriverPaths>
      </component>
   </settings>
</unattend>
 

7. Mount the Windows image that you intend to install the drivers 
   to by using ImageX. For example:

imagex /mountrw C:\windows_distribution\sources\install.wim 1 C:\wim_mount

8. Enable logging of specific device driver injection actions in a 
   separate log file. Edit the following registry key on the computer 
   on which you are running Package Manager:

Path: HKLM\Software\Microsoft\Windows\CurrentVersion\Device Installer

Key: DebugPkgMgr

Type: REG_DWORD

Value: 0x01

This will create a Drivers.log file during the driver package injection. This log file will log all actions of the driver injection process.

9. Use Package Manager to apply the unattended installation answer 
    file to the mounted Windows image. Specify a location for the log
    file to create. For example,

pkgmgr /o:"C:\wim_mount\;C:\wim_mount\Windows" /n:"C:\unattend.xml" /l:"C:\pkgmgrlogs\logfile.txt"

    For more information about using Package Manager, see Package Manager Command-Line Options.
    The .inf files referenced in the path in the answer file are added to
    the Windows image. A log file is created in the directory 
    C:\Pkgmgrlogs\. Driver log files are created in the directory that
    PkgMgr runs from. You can open the Drivers.log file and review the 
    Package Manager driver injection actions.

10. Review the contents of the %WINDIR%\Inf\ directory in the mounted 
    Windows image to ensure that the .inf files were installed. Drivers
    added to the Windows image are named oem*.inf. This is to ensure 
    unique naming for new drivers added to the computer. For example,
    the files MyDriver1.inf and MyDriver2.inf are renamed oem0.inf and
    oem1.inf.

11. Unmount the .wim file and commit the changes. For example,

imagex /unmount /commit C:\wim_mount

12. The Windows image is ready to be deployed.
    
    For more information about Windows Vista answer 
    files and unattended installations, please refer to the 
    Windows Automated Installation Kit (WAIK) User's Guide.

************************************************************
* 8E.  INSTALLING THE WINDOWS SERVER* 2008 INF FILES PRIOR 
*      TO OS INSTALLATION
************************************************************
NOTE: Although $OEM$ method is still supported, it is no longer 
the preferred method.

Microsoft* published a Wndows Automated Installation Kit(WAIK) 
which facilitates creation of answer files and image creation 
for unattended installs of Windows Server 2008

To add drivers to an offline Windows image

1.  Locate the device driver .inf files that you intend to 
    install on your Windows image.

2.  Use Windows System Image Manager (Windows SIM) to create 
    an answer file that contains the paths to the device 
    drivers that you intend to install.

3.  Add the Microsoft-Windows-PnpCustomizationsNonWinPE component 
    to your answer file in the offlineServicing pass.

4.  Expand the Microsoft-Windows-PnpCustomizationsNonWinPE node 
    in the answer file. Right-click DevicePaths, and then select 
    Insert New PathAndCredentials.

5.  In the Microsoft-Windows-PnpCustomizationsNonWinPE component, 
    specify the path to the device driver and the credentials used 
    to access the file if the file is on a network share.

6.  Save the answer file and exit Windows SIM. The answer file must 
    be similar to the following sample.
 
<?xml version="1.0" ?>
<unattend xmlns="urn:schemas-microsoft-com:asm.v3" xmlns:wcm="http://schemas.microsoft.com/WMIConfig/2002/State">
   <settings pass="offlineServicing">
      <component name="Microsoft-Windows-PnpCustomizationsNonWinPE" processorArchitecture="x86" publicKeyToken="31bf3856ad364e35" language="neutral" versionScope="nonSxS">
         <DriverPaths>
            <PathAndCredentials wcm:keyValue="1">
               <Path>\\networkshare\share\drivers</Path>
               <Credentials>
                  <Domain>Fabrikam</Domain>
                  <Username>MyUserName</Username>
                  <Password>MyPassword</Password>
               </Credentials>
            </PathAndCredentials>
         </DriverPaths>
      </component>
   </settings>
</unattend>
 

7. Mount the Windows image that you intend to install the drivers 
   to by using ImageX. For example:

imagex /mountrw C:\windows_distribution\sources\install.wim 1 C:\wim_mount

8. Enable logging of specific device driver injection actions in a 
   separate log file. Edit the following registry key on the computer 
   on which you are running Package Manager:

Path: HKLM\Software\Microsoft\Windows\CurrentVersion\Device Installer

Key: DebugPkgMgr

Type: REG_DWORD

Value: 0x01

This will create a Drivers.log file during the driver package injection. This log file will log all actions of the driver injection process.

9. Use Package Manager to apply the unattended installation answer 
    file to the mounted Windows image. Specify a location for the log
    file to create. For example,

pkgmgr /o:"C:\wim_mount\;C:\wim_mount\Windows" /n:"C:\unattend.xml" /l:"C:\pkgmgrlogs\logfile.txt"

    For more information about using Package Manager, see Package Manager Command-Line Options.
    The .inf files referenced in the path in the answer file are added to
    the Windows image. A log file is created in the directory 
    C:\Pkgmgrlogs\. Driver log files are created in the directory that
    PkgMgr runs from. You can open the Drivers.log file and review the 
    Package Manager driver injection actions.

10. Review the contents of the %WINDIR%\Inf\ directory in the mounted 
    Windows image to ensure that the .inf files were installed. Drivers
    added to the Windows image are named oem*.inf. This is to ensure 
    unique naming for new drivers added to the computer. For example,
    the files MyDriver1.inf and MyDriver2.inf are renamed oem0.inf and
    oem1.inf.

11. Unmount the .wim file and commit the changes. For example,
    imagex /unmount /commit C:\wim_mount

12. The Windows image is ready to be deployed.
    
    For more information about Windows Server 2008 answer 
    files and unattended installations, please refer to the 
    Windows Automated Installation Kit (WAIK) User's Guide.

************************************************************
* 8F.  INSTALLING THE WINDOWS 7* INF FILES PRIOR 
*      TO OS INSTALLATION
************************************************************
The simplest method for installing Windows? onto new hardware is to
start directly from the Windows product DVD with an answer file called 
Autounattend.xml. Boot the computer with the Windows Setup media in the 
DVD drive and the configuration set available on an external drive. 
By default, Windows Setup searches all removable media for an answer 
file called Autounattend.xml. Autounattend.xml must be located at the 
root of the removable media.

The answer file enables you to automate all or parts of Windows Setup 
Includeing adding INF files. You can create an answer file by using Windows
System Image Manager (Windows SIM).

Microsoft* published a Wndows Automated Installation Kit(WAIK) 
(Must be the windows 7 version) which facilitates creation of answer files 
and image creation for unattended installs of Windows 7 with tools such as Windows SIM

To create a configuration set you will need:
	Windows System Image Manager (Windows SIM) installed on a technician computer.
	An authorized copy of a Windows Vista? product DVD.
	Chipset device driver .inf files.
	Access to a network share or removable media with sufficient storage space.

1. Create a New Answer File
(In this step, you define basic disk configuration and other settings that are required 
for an unattended installation.)
	A. On your technician computer, insert the Windows 7 product DVD into the local 
	   DVD-ROM drive.
	B. On the desktop of the technician computer, navigate to the \Sources directory
	   on your DVD-ROM drive. Copy the Install.wim file from the Windows product DVD
           to a location on the computer.
	C. Open Windows SIM. On the desktop of the computer, click Start, point to 
           Programs, point to Microsoft Windows OPK (or Windows AIK), and then click 
           Windows System Image Manager.
	D. On the File menu, click Select Windows Image.
	E. In the Select a Windows Image dialog box, navigate to the location where 
	   you saved the Install.wim file, and then click Open.
		Note:  
		A warning will appear that a .clg file does not exist. 
		Click OK to create a .clg file. 
		If there is more than one Windows image in the .wim file, you are prompted
		to select the Windows image to open.
	F. On the File menu, click New Answer File.
2. Create a Distribution Share
(In this step, you create a distribution-share folder on your technician computer. 
The distribution share will store out-of-box drivers, applications, and any resource 
files needed for your custom installation.)
	A. In Windows SIM, in the Distribution Share pane, click Select a Distribution
	   Share.
	B. Right-click to select Create Distribution Share.
	C. The Create a Distribution Share dialog box appears.
	D. Click New Folder, and then type a name for the folder. For example 
	   "C:\MyDistributionShareClick"
	E. In the Distribution Share pane, the distribution share folder opens. 
	   Windows SIM automatically creates the following folder structure.
		C:\MyDistributionShare\$OEM$ Folders
		C:\MyDistributionShare\Packages
		C:\MyDistributionShare\Out-of-Box 
3. Add Drivers and Applications to Distribution Share
	A. In Windows SIM, on the Tools menu, select Explore Distribution Share.
	B. The Distribution Share window opens.
	C. Copy your device driver files (.inf) to the Out-of-Box Drivers folder.
		1. Create subdirectories for each driver. For example, 
		   create directories "Chipset" and "Video" in the Out-of-Box Drivers 
		   folder.
	D. Close the distribution share folder.
4. Add a Device Driver to the Answer File
(In this step, you add an out-of-box drivers (.inf) path to your answer file.)	
	A. In Windows SIM, on the Insert menu, click Driver Path, and then click Pass 1
	   windowsPE. 
	B. The Browse for Folder dialog box appears.
	C. Select the driver path to add to the answer file, and then click OK. 
	   For example, "C:\MyDistributionShare\Out-of-Box Drivers\Chipset"
5. Validate the Answer File
(In this step, you validate the settings in your answer file and then save them to a file.)
	A. In Windows SIM, click Tools, and then click Validate Answer File.
	B. If the answer file validates successfully, a "success" message appears in the
           Messages pane; otherwise, error messages appear in the same location.
	C. If an error occurs, in the Messages pane, double-click the error to navigate
           to the incorrect setting. Change the setting to fix the error, and then 
           revalidate the answer file.
	D. On the File menu, click Save Answer File. Save the file as Unattend.xml.
6. Create a Configuration Set
(In this step, you create a configuration set that will gather all of the resource files 
that you specified in your answer file into one location.)
	A. In Windows SIM, on the Tools menu, select Create Configuration Set.
	B. The Create Configuration Set window opens.
	C. Specify a destination location where you intend to publish the configuration set
	D. Select a removable dirve such as a USB flash drive (UFD), and then click OK.
7. Deploying a Configuration Set Without a Network
	A. Turn on the new computer.
	B. Insert both the removable media containing your configuration set and the
	   Windows 7 product DVD into the new computer.	
		Note: When using a USB flash drive, insert the drive directly into the 
                      primary set of USB ports for the computer. For a desktop computer, 
                      this is typically in the back of the computer.
 	C. Restart the computer by pressing CTRL+ALT+DEL.
		Note: This example assumes that the hard drive is blank.
	E. Windows Setup (Setup.exe) begins automatically.
	F. By default, Windows Setup searches all removable media for an answer file 
	   called Autounattend.xml. Autounattend.xml must be located at the root of the 
           removable media.
	G. After Setup completes, validate that all customizations were applied, and then
	   reseal the computer by using the generalize option

    For more information about Windows Server 2008 answer 
    files and unattended installations, please refer to the 
    Windows Automated Installation Kit (WAIK) User's Guide.

************************************************************
* 8G.  INSTALLING THE Windows Server 2008 R2* INF FILES PRIOR 
*      TO OS INSTALLATION
************************************************************
The simplest method for installing Windows? onto new hardware is to
start directly from the Windows product DVD with an answer file called 
Autounattend.xml. Boot the computer with the Windows Setup media in the 
DVD drive and the configuration set available on an external drive. 
By default, Windows Setup searches all removable media for an answer 
file called Autounattend.xml. Autounattend.xml must be located at the 
root of the removable media.

The answer file enables you to automate all or parts of Windows Setup 
Includeing adding INF files. You can create an answer file by using Windows
System Image Manager (Windows SIM).

Microsoft* published a Wndows Automated Installation Kit(WAIK) 
(Must be the Windows Server 2008  R2* version) which facilitates creation of answer files 
and image creation for unattended installs of Windows Server 2008  R2* with tools such as Windows SIM

To create a configuration set you will need:
	Windows System Image Manager (Windows SIM) installed on a technician computer.
	An authorized copy of a Windows Vista? product DVD.
	Chipset device driver .inf files.
	Access to a network share or removable media with sufficient storage space.

1. Create a New Answer File
(In this step, you define basic disk configuration and other settings that are required 
for an unattended installation.)
	A. On your technician computer, insert the Windows Server 2008  R2* product DVD into the local 
	   DVD-ROM drive.
	B. On the desktop of the technician computer, navigate to the \Sources directory
	   on your DVD-ROM drive. Copy the Install.wim file from the Windows product DVD
           to a location on the computer.
	C. Open Windows SIM. On the desktop of the computer, click Start, point to 
           Programs, point to Microsoft Windows OPK (or Windows AIK), and then click 
           Windows System Image Manager.
	D. On the File menu, click Select Windows Image.
	E. In the Select a Windows Image dialog box, navigate to the location where 
	   you saved the Install.wim file, and then click Open.
		Note:  
		A warning will appear that a .clg file does not exist. 
		Click OK to create a .clg file. 
		If there is more than one Windows image in the .wim file, you are prompted
		to select the Windows image to open.
	F. On the File menu, click New Answer File.
2. Create a Distribution Share
(In this step, you create a distribution-share folder on your technician computer. 
The distribution share will store out-of-box drivers, applications, and any resource 
files needed for your custom installation.)
	A. In Windows SIM, in the Distribution Share pane, click Select a Distribution
	   Share.
	B. Right-click to select Create Distribution Share.
	C. The Create a Distribution Share dialog box appears.
	D. Click New Folder, and then type a name for the folder. For example 
	   "C:\MyDistributionShareClick"
	E. In the Distribution Share pane, the distribution share folder opens. 
	   Windows SIM automatically creates the following folder structure.
		C:\MyDistributionShare\$OEM$ Folders
		C:\MyDistributionShare\Packages
		C:\MyDistributionShare\Out-of-Box 
3. Add Drivers and Applications to Distribution Share
	A. In Windows SIM, on the Tools menu, select Explore Distribution Share.
	B. The Distribution Share window opens.
	C. Copy your device driver files (.inf) to the Out-of-Box Drivers folder.
		1. Create subdirectories for each driver. For example, 
		   create directories "Chipset" and "Video" in the Out-of-Box Drivers 
		   folder.
	D. Close the distribution share folder.
4. Add a Device Driver to the Answer File
(In this step, you add an out-of-box drivers (.inf) path to your answer file.)	
	A. In Windows SIM, on the Insert menu, click Driver Path, and then click Pass 1
	   windowsPE. 
	B. The Browse for Folder dialog box appears.
	C. Select the driver path to add to the answer file, and then click OK. 
	   For example, "C:\MyDistributionShare\Out-of-Box Drivers\Chipset"
5. Validate the Answer File
(In this step, you validate the settings in your answer file and then save them to a file.)
	A. In Windows SIM, click Tools, and then click Validate Answer File.
	B. If the answer file validates successfully, a "success" message appears in the
           Messages pane; otherwise, error messages appear in the same location.
	C. If an error occurs, in the Messages pane, double-click the error to navigate
           to the incorrect setting. Change the setting to fix the error, and then 
           revalidate the answer file.
	D. On the File menu, click Save Answer File. Save the file as Unattend.xml.
6. Create a Configuration Set
(In this step, you create a configuration set that will gather all of the resource files 
that you specified in your answer file into one location.)
	A. In Windows SIM, on the Tools menu, select Create Configuration Set.
	B. The Create Configuration Set window opens.
	C. Specify a destination location where you intend to publish the configuration set
	D. Select a removable dirve such as a USB flash drive (UFD), and then click OK.
7. Deploying a Configuration Set Without a Network
	A. Turn on the new computer.
	B. Insert both the removable media containing your configuration set and the
	   Windows Server 2008  R2*  product DVD into the new computer.	
		Note: When using a USB flash drive, insert the drive directly into the 
                      primary set of USB ports for the computer. For a desktop computer, 
                      this is typically in the back of the computer.
 	C. Restart the computer by pressing CTRL+ALT+DEL.
		Note: This example assumes that the hard drive is blank.
	E. Windows Setup (Setup.exe) begins automatically.
	F. By default, Windows Setup searches all removable media for an answer file 
	   called Autounattend.xml. Autounattend.xml must be located at the root of the 
           removable media.
	G. After Setup completes, validate that all customizations were applied, and then
	   reseal the computer by using the generalize option

    For more information about Windows Server 2008  R2* answer 
    files and unattended installations, please refer to the 
    Windows Automated Installation Kit (WAIK) User's Guide.

************************************************************
* 9.  INSTALLING THE INF FILES AFTER OS INSTALLATION
************************************************************

************************************************************
* 9A.  INSTALLING THE WINDOWS* 2000 INF FILES AFTER OS 
*      INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows* 2000, so it may not be necessary to use the INF 
files provided by this software to update Windows* 2000.

The following steps describe the installation process of
the Windows* 2000 INF files. You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows* 2000.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\All 
        directory to the root directory of the floppy disk (A:\).
        
        NOTE:
            XXXX is the directory name for the chipset of 
            interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
            Multiprocessor PC.
        
        NOTE:  
            Only one of the above items will be 
            displayed for a given system.
             
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows* 2000 will launch the Upgrade Device Driver 
            Wizard. Select Next.
    17. Ensure that the following choice is selected:
            Search for a suitable driver for my device 
            (recommended)
    18. Insert the floppy containing the Windows* 2000 INF 
            files into the floppy drive.
    19. Select Next.
    20. Windows* 2000 will list locations from where the 
            updated driver file can be found.  Ensure that the 
            following choice is selected: Floppy disk drives
    21. Select Next.
    22. Windows* 2000 should report that a driver has been
            found: (The detected device name will be displayed.)
            Select Next.            
    23. Select Finish.
    24. Reboot the system when prompted to do so.

************************************************************
* 9B.  INSTALLING THE WINDOWS* XP INF FILES AFTER OS 
*      INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows* XP so it may not be necessary to use the INF 
files provided by this software to update Windows* XP.

The following steps describe the installation process of
the Windows* XP INF files. You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows* XP.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\All 
        directory to the root directory of the floppy disk (A:\).
        
        NOTE: 
            XXXX is the directory name for the chipset 
            of interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select the Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
            Multiprocessor PC.
            
        NOTE: 
            Only one of the above items will be 
            displayed for a given system.
            
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows* XP will launch the Upgrade Device Driver 
            Wizard. Select Next.
    17. Ensure that the following choice is selected:
            Search for a suitable driver for my device 
            (recommended)
    18. Insert the floppy containing the Windows* XP INF 
            files into the floppy drive.
    19. Select Next.
    20. Windows* XP will list locations from where the 
            updated driver file can be found.  Ensure that the 
            following choice is selected: Floppy disk drives
    21. Select Next.
    22. Windows* XP should report that a driver has been
            found: (The detected device name will be displayed.)
            Select Next.            
    23. Select Finish.
    24. Reboot the system when prompted to do so.


************************************************************
* 9C.  INSTALLING THE WINDOWS SERVER* 2003 INF FILES AFTER 
*      OS INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows Server* 2003 so it may not be necessary to use the INF 
files provided by this software to update Windows Server* 2003.

The following steps describe the installation process of
the Windows* XP INF files.  You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows Server* 2003.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\All
        directory to the root directory of the floppy disk (A:\).
        
        NOTE: 
            XXXX is the directory name for the chipset 
            of interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select the Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
            Multiprocessor PC.
            
        NOTE: 
            Only one of the above items will be 
            displayed for a given system.
            
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows Server* 2003 will launch the Upgrade Device 
            Driver Wizard. Select Next.
    17. Ensure that the following choice is selected: Search
            for a suitable driver for my device (recommended)
    18. Insert the floppy containing the Windows Server* 2003 
            INF files into the floppy drive.
    19. Select Next.
    20. Windows Server* 2003 will list locations from where the 
            updated driver file can be found. Ensure that the 
            following choice is selected: Floppy disk drives
    21. Select Next.
    22. Windows Server* 2003 should report that a driver has 
            been found: (The detected device name will be displayed.)
            Select Next.            
    23. Select Finish.
    24. Reboot the system when prompted to do so.

************************************************************
* 9D.  INSTALLING THE WINDOWS VISTA INF FILES AFTER 
*      OS INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows Vista so it may not be necessary to use the INF 
files provided by this software to update Windows Vista.

The following steps describe the installation process of
the Windows* Vista INF files.  You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows Vista.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\All
        directory to the root directory of the floppy disk (A:\).
        
        NOTE: 
            XXXX is the directory name for the chipset 
            of interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select the Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
            Multiprocessor PC.
            
        NOTE: 
            Only one of the above items will be 
            displayed for a given system.
            
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows Vista will launch the Upgrade Device 
            Driver Wizard. Select Browse my computer for the driver software.
    17. Enter "A:\" in the Combo Box
    18. Ensure that the Include Subfolders checkbox is checked
    19. Select Next
    20. The window Will Display the Device that was installed
    21. Select Close
    22. Reboot the system if prompted to do so.

************************************************************
* 9E.  INSTALLING THE Windows Server* 2008 INF FILES AFTER 
*      OS INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows Server* 2008 so it may not be necessary to use the INF 
files provided by this software to update Windows Server* 2008.

The following steps describe the installation process of
the Windows Server* 2008 INF files.  You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows Server* 2008.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\All
        directory to the root directory of the floppy disk (A:\).
        
        NOTE: 
            XXXX is the directory name for the chipset 
            of interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select the Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
            Multiprocessor PC.
            
        NOTE: 
            Only one of the above items will be 
            displayed for a given system.
            
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows Vista will launch the Upgrade Device 
            Driver Wizard. Select Browse my computer for the driver software.
    17. Enter "A:\" in the Combo Box
    18. Ensure that the Include Subfolders checkbox is checked
    19. Select Next
    20. The window Will Display the Device that was installed
    21. Select Close
    22. Reboot the system if prompted to do so.

************************************************************
* 9F.  INSTALLING THE Windows 7* INF FILES AFTER 
*      OS INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows 7* so it may not be necessary to use the INF 
files provided by this software to update Windows 7*.

The following steps describe the installation process of
the Windows 7* INF files.  You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows 7*.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\Win7
        directory to the root directory A removable media, 
	such as a USB flash drive (UFD) or floppy disk (A:\).
        
        NOTE: 
            XXXX is the directory name for the chipset 
            of interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select the Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
            Multiprocessor PC.
            
        NOTE: 
            Only one of the above items will be 
            displayed for a given system.
            
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows 7* will launch the Upgrade Device 
            Driver Wizard. Select Browse my computer for the driver software.
    17. Enter "A:\" in the Combo Box
    18. Ensure that the Include Subfolders checkbox is checked
    19. Select Next
    20. The window Will Display the Device that was installed
    21. Select Close
    22. Reboot the system if prompted to do so.

************************************************************
* 9G.  INSTALLING THE Windows Server* 2008 R2 INF FILES AFTER 
*      OS INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows Server* 2008 R2 so it may not be necessary to use the INF 
files provided by this software to update Windows Server* 2008 R2.

The following steps describe the installation process of
the Windows Server* 2008 R2 INF files.  You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows Server* 2008 R2.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\Win7
         directory to the root directory A removable media, 
	such as a USB flash drive (UFD) or floppy disk (A:\).
        
        NOTE: 
            XXXX is the directory name for the chipset 
            of interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select the Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
            Multiprocessor PC.
            
        NOTE: 
            Only one of the above items will be 
            displayed for a given system.
            
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows Server* 2008 R2 will launch the Upgrade Device 
            Driver Wizard. Select Browse my computer for the driver software.
    17. Enter "A:\" in the Combo Box
    18. Ensure that the Include Subfolders checkbox is checked
    19. Select Next
    20. The window Will Display the Device that was installed
    21. Select Close
    22. Reboot the system if prompted to do so.

************************************************************
* 10.	IDENTIFYING THE SOFTWARE VERSION NUMBER
************************************************************
The version numbers displayed by Device Manager for a given 
device may not be the same as the Intel(R) Chipset Device 
Software version.  
 
The correct version number is shown at the top of this file.


************************************************************
* 11.  TROUBLESHOOTING
************************************************************
It is assumed that the system requirements in Section 2 above 
have been satisfied.

Issue:	    
            USB devices no longer work correctly after you 
            install the Intel Chipset Software Installation 
            Utility in Windows XP or in Windows Server 2003.

Solution:  
            A recommended fix has been provided by Microsoft
            in Knowledge Base article(921411). For additional 
            information, please refer to the KB article located 
            at http://support.microsoft.com/kb/921411/en-us
            
            Please use the following installation procedures: 
                - Windows XP or Windows Server 2003 installed
                - QFE (921411) installed
                - Latest Intel(R) Chipset Device Software

Issue:	    
            At the end of executing the Chipset Device Software,
        		the USB keyboard and mouse will stop functioning. 
        		This problem only occurs when using Windows XP with 
        		SP1 or Windows 2000 Server with SP4 on a system 
        		configured with a USB keyboard and/or mouse. This 
        		condition is temporary until a system reset.

Solution:  
            A recommended fix has been provided by Microsoft
            in Knowledge Base article(822603). For additional 
            information, please refer to the KB article located at
            http://support.microsoft.com/default.aspx?scid=kb;[LN];822603  

            Please use the following installation procedures: 
                - Windows XP installed with SP1
                - QFE (822603) installed
                - Latest Chipset Utility Software installed.

Issue:      
            System locks up during Device Manager Remove or 
            during restart.

Solution:   
            System lockup can occur during reboot as a 
            result of several possible system issues.  In 
            the event of system lockup, reboot the machine 
            and view Device Manager.  If devices are listed 
            properly and the system experiences no further 
            problems, then the .INF file restore process was 
            successful. If devices are not configured 
            correctly, try re-running the procedures 
            outlined in Section 3.

            If this does not fix the issue or further issues
            are experienced, reinstall the operating system.

Issue:      
            After running the setup program and rebooting 
            the machine, Windows reports that it cannot find 
            one of the following files: ESDI_506.pdr

Solution:   
            Click Browse in the dialog box where this issue
            occurs, locate the <Windows>\System\IOSubsys
            directory. Click OK. The system should be able to
            locate this file in this directory and continue 
            re-enumerating for the new devices.

Issue:      
            After running the setup program and rebooting 
            the machine, Windows reports that it cannot find 
            one of the following files:
 
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   
            Click Browse in the dialog box where this issue 
            occurs and locate the following directory:
			
                  <Winnt>\System32\drivers 
                  
            Click OK. The system should be able to locate the 
            files in this directory and continue re-enumerating 
            for the new devices.

Issue:      
            After running the setup program and rebooting 
            the machine, Windows reports that it cannot find 
            the following file: ISAPNP.VXD

Solution:   
            Click Browse in the dialog box where this issue 
            occurs and locate the <Winnt>\System directory. 
            Click OK. The system should be able to locate this 
            file in this directory and continue re-enumerating 
            for the new devices.

Issue:      
            After performing the silent install, the 
            HKLM\Software\Intel\InfInst key was not created 
            or the data of the value "install" is not 
            "success".

Solution:   
            This is caused by one of the following 
            scenarios:
               - The current system does not contain a 
                 supported operating system, or
                 -or-
               - The current system does not contain a 
                 supported chipset.

            Verify that the System Requirements are met as 
            outlined in Section 2.


************************************************************
* DISCLAIMER
************************************************************
Intel is making no claims of usability, efficacy or warranty.  
The Intel(R) SOFTWARE LICENSE AGREEMENT
(OEM / IHV / ISV Distribution & Single User) 
completely defines the licensed use of this software.
************************************************************
Information in this document is provided in connection with 
Intel(R) products.  No license, express or implied, by estoppel 
or otherwise, to any intellectual property rights is granted 
by this document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty relating 
to sale and/or use of Intel(R) products, including liability 
or warranties relating to fitness for a particular purpose, 
merchantability or infringement of any patent, copyright or 
other intellectual property right.  Intel(R) products are 
not intended for use in medical, life saving, or 
life-sustaining applications.

************************************************************
Intel Corporation disclaims all warranties and liabilities 
for the use of this document and the information contained 
herein, and assumes no responsibility for any errors which 
may appear in this document, nor does Intel make a 
commitment to update the information contained herein.  
Intel reserves the right to make changes to this document at 
any time, without notice.
************************************************************
************************************************************

* Intel is a trademark or registered trademark of Intel Corporation 
  or its subsidiaries in the United States and other countries.
* Other brands and names are the property of their 
  respective owners.

Copyright (c) Intel Corporation, 1997-2010
