Reader™ User Guide
Print
Top page > Getting started > Parts and Controls > Removing/attaching the Back Panel (PRS-T3S*)

## Removing/attaching the Back Panel (PRS-T3S*)

* Limited edition only.

### Removing the Back Panel

1. Turn over the Reader.

1. Hold the Reader firmly with one hand.

1. Place you fingernail or a pointed object into the slot on the bottom edge, then carefully lift and remove the Back Panel.

### Attaching the Back Panel

1. Insert the top four tabs of the Back Panel into the upper holes of the Reader.

1. Insert all the tabs in their holes (indicated by arrows), and push down the Back Panel firmly.

Note

- Do not remove the label on the battery.

Go to page top