Reader™ User Guide
Print
Top page > Other Information > Appendix > Specifications

## Specifications

### Model name

PRS-T3/PRS-T3S

### Power source

Built-in rechargeable battery: 3.7 V DC, 1000mAh
USB powered from a computer or the optional AC Adapter PRSA-AC10/PRSA-AC1A (sold separately) via the supplied USB cable.

### Battery life (continuous page turn)

Maximum Battery: Approximately 30,000 continuous page turns when reading only.*
* Measured using a text based content in ePub format and a fully charged battery, consecutive page-turns at approximately one second per page under the recommended operating temperature. Actual battery life may vary based on usage patterns and individual device.

### Charging time

Computer-based charging: Approximately 2.5 hours
AC Adapter PRSA-AC10/PRSA-AC1A (sold separately)-based charging: Approximately 2 hours

### Internal memory capacity (for data storage)

Approximately 1.2GB after initial setting.
Depending on size of pre-loaded excerpts, available memory capacity may vary.

### Operating/Charging temperature

5°C to 35°C (41°F to 95°F)

### Dimensions (w/h/d)

PRS-T3: 109 × 160 × 11.3 mm (4 3/8 × 6 3/8 × 15/32 inches)
PRS-T3S: 107 × 160 × 8.8 mm (4 1/4 × 6 3/8 × 3/8 inches)

### Mass

PRS-T3: 200 g (7.1 oz.)
PRS-T3S: 160 g (5.6 oz.)

### Display

152.4 mm (6 inch) diagonal electrophoretic display
758 × 1024 pixels, 16-level grayscale

### Wi-Fi

Wireless standards: IEEE 802.11b/g/n compliant
Wireless security: WEP (Open System), WEP (Shared Key), WPA-PSK (TKIP), WPA-PSK (AES), WPA2-PSK (TKIP), WPA2-PSK (AES)

### Expansion slots

microSD card slot
See Details for supported card types and precautions.

### Supplied items

USB cable × 1
Quick Start Guide
Go to page top