Reader™ User Guide
Print
Top page > Getting started > Parts and Controls > Removing/attaching the Standard Cover (PRS-T3)

## Removing/attaching the Standard Cover (PRS-T3)

### Removing the Standard Cover

1. Open the Standard Cover and turn over the Reader.

1. Hold the Reader firmly with one hand.

1. Place your fingernail or a pointed object into the slot on the bottom edge, then carefully lift and remove the Standard Cover.

### Attaching the Standard Cover

1. Insert the top four tabs of the Standard Cover into the upper holes of the Reader.

1. Insert all the tabs in their holes (indicated by arrows), and push down the Standard Cover firmly.

Note

- Do not remove the label on the battery.

Tip

- The Standard Cover and Cover with Light (sold separately) include a magnetically-activated wake/sleep feature, which automatically wakes/puts your Reader to sleep when you open/close the cover.

Go to page top