# Digital Still Camera DSC-QX10/QX100

## EV

Adjusts the exposure manually.

1. Connect the camera and the smartphone via Wi-Fi, then touch the exposure compensation value and select the desired value.

   DSC-QX100: Adjusts the exposure manually in a range of –3.0 EV to +3.0 EV.

   DSC-QX10: Adjusts the exposure manually in a range of –2.0 EV to +2.0 EV.

#### Note

- You cannot set the EV value when [Intelligent Auto] or [Superior Auto] is set.
- The exposure compensation value you can see on the screen when shooting is from -2.0 EV to +2.0 EV. If you set the value outside of that range, the brightness on the screen will not change while shooting, but will be reflected in the recorded images (DSC-QX100 only).

#### Hint

A: Overexposure (too much light)

B: Correct exposure

C: Underexposure (too little light)

- When the image shot is overexposed, adjust [EV] to the minus side.
- When the image shot is underexposed, adjust [EV] to the plus side.

Go to Page Top

### Related Topic

- Exposure Mode

Go to Page Top