# Digital Still Camera DSC-QX10/QX100

## Aperture Priority Shooting (DSC-QX100 only)

You can adjust the focus range or degree of background defocus by manually setting the aperture (F value).

1. Connect the camera and the smartphone via Wi-Fi, then set the Exposure Mode to A (Aperture Priority Shooting).

2. Touch the F value and select the desired F value.

   Selects an aperture (F value) from F1.8 to F11.

#### Note

- When you adjust the zoom to the T side, the maximum aperture (minimum F value) will increase.

Go to Page Top

### Related Topic

- Exposure Mode

Go to Page Top