Task

# Inserting/Removing a SIM Card

## To insert a SIM card

1. Make sure all the cables are unplugged from your tablet device, and then shut down the tablet device [Details].

1. Turn over your tablet device, and then open the SIM card cover.

1. Insert a pin or small paper clip (not supplied) into the SIM card eject hole.

1. Eject the SIM tray.

Note

- Make sure to handle the SIM tray gently.

1. Place a SIM card on the SIM tray so that the cutout of the SIM card fits that of the SIM tray.

Note

- Make sure there are no protrusions on the cutting surface after detaching the SIM card from its plastic package. Otherwise, the SIM card may not fit in the SIM tray.

1. Insert the SIM tray.

Note

- Make sure not to insert the SIM tray in the reverse direction.

## To remove a SIM card

1. Follow the procedures up to step 5 of “To insert a SIM card,” then remove the SIM card from the tray.

The procedures after this step are the same as from step 6 of “To insert a SIM card.”
Related Topic
About the Wireless WAN
Enabling Wireless WAN Communications
Disabling Wireless WAN Communications
Notes on the SIM Card
Setting Up an Access Point