VAIO User Guide

Task

# Replacing the AA Battery of the Mouse

Change the AA battery in the mouse when the battery power becomes low.

1. Set the power switch of the mouse to OFF.

1. Turn the mouse upside down. Hold the center of the cover and slide the battery cover in the direction of the arrow.

1. Remove the old battery and insert a new AA alkaline battery (minus (-) end first), then close the cover.

1. Set the power switch of the mouse to ON.

Note

- Use a new AA alkaline replacement battery.

- If you do not intend to use the mouse for a while, set the power switch of the mouse to OFF. If you do not intend to use the mouse for an extended period of time, remove its AA battery.

- When the battery power becomes low, replace with the battery promptly. Keeping a depleted battery in the mouse may cause battery leakage.

- Since the mouse cannot be used with a commercially available rechargeable battery, use a non-rechargeable AA battery. If you use a rechargeable battery, battery leakage may occur, resulting in a malfunction.

- Do not recharge a dry cell AA battery.

- Refer to the supplied safety information manual.

Related Topic
Parts and Controls of the Mouse
Checking the Remaining Battery Power of the Mouse